description = <b>EAGLE Design Rules</b>\n<p>\nThe default Design Rules have been set to cover\na wide range of applications. Your particular design\nmay have different requirements, so please make the\nnecessary adjustments and save your customized\ndesign rules under a new name.
mdWireWire = 12mil
mdWirePad = 12mil
mdWireVia = 12mil
mdPadPad = 12mil
mdPadVia = 12mil
mdViaVia = 12mil
mdSmdPad = 12mil
mdSmdVia = 12mil
mdSmdSmd = 12mil
mdViaViaSameLayer = 8mil
mnLayersViaInSmd = 2
mdCopperDimension = 40mil
mdDrill = 12mil
mdSmdStop = 0mil
msWidth = 10mil
msDrill = 24mil
rvPadTop = 0.250000
rvPadInner = 0.250000
rvPadBottom = 0.250000
rvViaOuter = 0.250000
rvViaInner = 0.250000
rlMinPadTop = 10mil
rlMaxPadTop = 20mil
rlMinPadInner = 10mil
rlMaxPadInner = 20mil
rlMinPadBottom = 10mil
rlMaxPadBottom = 20mil
rlMinViaOuter = 8mil
rlMaxViaOuter = 20mil
rlMinViaInner = 8mil
rlMaxViaInner = 20mil
psTop = -1
psBottom = -1
psFirst = -1
mvStopFrame = 0.100000
mvCreamFrame = 0.000000
mlMinStopFrame = 0mil
mlMaxStopFrame = 20mil
mlMinCreamFrame = 0mil
mlMaxCreamFrame = 0mil
mlViaStopLimit = 0mil
srRoundness = 0.000000
srMinRoundness = 0mil
srMaxRoundness = 0mil
slThermalGap = 0.500000
slMinThermalGap = 20mil
slMaxThermalGap = 100mil
slAnnulusIsolate = 20mil
slThermalIsolate = 10mil
slAnnulusRestring = 0
slThermalRestring = 1
slThermalsForVias = 0
checkGrid = 0
checkAngle = 0
checkFont = 1
checkRestrict = 1
useDiameter = 13
maxErrors = 50
viaSetup = FFFF F0
