
(rules PCB gassensor
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 121)
    (layer_rule F.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.0)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.0)
    )
  )
  (rule
    (width 254.0)
    (clear 254.2)
    (clear 127.0 (type smd_to_turn_gap))
    (clear 63.6 (type smd_smd))
  )
  (padstack "Via[0-1]_685.8:330.2_um"
    (shape
      (circle F.Cu 685.8 0.0 0.0)
    )
    (shape
      (circle B.Cu 685.8 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_685.8:330.2_um" "Via[0-1]_685.8:330.2_um" default
  )
  (via 
    "Via[0-1]_685.8:330.2_um-kicad_default" "Via[0-1]_685.8:330.2_um" "kicad_default"
  )
  (via_rule
    default "Via[0-1]_685.8:330.2_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_685.8:330.2_um-kicad_default"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 254.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    GND VCC /VOUT+ +12V "Net-(D2-Pad1)" "Net-(D3-Pad1)" /A0 /A1
    "Net-(D4-Pad1)" "Net-(D5-Pad1)" /A2 "Net-(D6-Pad1)" /A3 /A4 "Net-(D7-Pad1)" /A5
    "Net-(D8-Pad1)" /A6 "Net-(D9-Pad1)" /A7 "Net-(D10-Pad1)" /D8 /D9 /TX
    /RX "Net-(J1-Pad3)" "Net-(J1-Pad5)" /D3 "Net-(J1-Pad7)" "Net-(J1-Pad8)" /D6 /D7
    /SS /MOSI /MISO /SCK "Net-(J1-Pad17)" "Net-(J1-Pad18)" +5V "Net-(J1-Pad28)"
    /TRIM /VSenseOut /REMOTE "Net-(R13-Pad2)" "Net-(RV2-Pad3)"
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 254.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)