(module MiniXLR-5_Switchcraft_TRAPC_Horizontal (layer F.Cu) (tedit 5C6413EA)
  (descr "http://www.switchcraft.com/ProductSummary.aspx?Parent=620 http://www.switchcraft.com/Drawings/TRAPC_X-TRASM_X_SERIES_CD.PDF")
  (tags "THT Mini XLR 5Pin right angle")
  (fp_text reference REF** (at 8 -5 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MiniXLR-5_Switchcraft_TRAPC_Horizontal (at 0 17.14 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.556 8.763) (end 9.906 8.763) (layer F.Fab) (width 0.1))
  (fp_line (start -3.556 8.763) (end -3.556 -4.191) (layer F.Fab) (width 0.1))
  (fp_line (start 9.906 8.763) (end 9.906 -4.191) (layer F.Fab) (width 0.1))
  (fp_line (start -2.413 15.875) (end 8.763 15.875) (layer F.Fab) (width 0.1))
  (fp_line (start -2.413 8.763) (end -2.413 15.875) (layer F.Fab) (width 0.1))
  (fp_line (start 8.763 15.875) (end 8.763 8.763) (layer F.Fab) (width 0.1))
  (fp_text user "PCB Edge" (at 3.355 8.763 180) (layer Dwgs.User)
    (effects (font (size 0.5 0.5) (thickness 0.08)))
  )
  (fp_line (start -3.556 -4.191) (end 9.906 -4.191) (layer F.Fab) (width 0.1))
  (fp_line (start -4.06 -4.69) (end 10.41 -4.69) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.26 16.38) (end -2.91 16.38) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.033 8.89) (end 10.033 6.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.033 8.89) (end 8.89 8.89) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.89 8.89) (end 8.89 16.002) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.89 16.002) (end -2.54 16.002) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.54 16.002) (end -2.54 8.89) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.54 8.89) (end -3.683 8.89) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.683 8.89) (end -3.683 6.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.033 4.52) (end 10.033 -4.318) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.033 -4.318) (end -3.683 -4.318) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.683 4.52) (end -3.683 -4.318) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -4.318) (end -0.508 -4.826) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.508 -4.826) (end 0.508 -4.826) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.508 -4.826) (end 0 -4.318) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 3.556 5.588 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.508 -4.191) (end 0 -3.683) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -3.683) (end 0.508 -4.191) (layer F.Fab) (width 0.1))
  (fp_line (start -4.06 4.66) (end -4.18 4.66) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.18 4.66) (end -4.18 6.01) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.18 6.01) (end -4.06 6.01) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.41 6.01) (end 10.53 6.01) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.53 6.01) (end 10.53 4.66) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.53 4.66) (end 10.41 4.66) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.41 9.26) (end 10.41 6.01) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.41 4.66) (end 10.41 -4.69) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.06 -4.69) (end -4.06 4.66) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.06 6.01) (end -4.06 9.26) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.91 9.26) (end -4.06 9.26) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.91 16.38) (end -2.91 9.26) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.41 9.26) (end 9.26 9.26) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.26 16.38) (end 9.26 9.26) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 2.54 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 3.81 2.54 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 5.08 0 180) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.794 5.334 180) (size 1.778 1.778) (drill 1.778) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 9.144 5.334 180) (size 1.778 1.778) (drill 1.778) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/MiniXLR-5_Switchcraft_TRAPC_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
