(module mkds_1,5-2 (layer F.Cu)
  (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
  (fp_text reference mkds_1,5/2 (at 0 -6.6) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (fp_text value VAL** (at 0 5.9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (fp_line (start 0 4.1) (end 0 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center 2.5 0.1) (end 0.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center -2.5 0.1) (end -0.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -5 2.6) (end 5 2.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -5 -2.3) (end 5 -2.3) (layer F.SilkS) (width 0.381))
  (fp_line (start -5 4.1) (end 5 4.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -5 4.6) (end 5 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 5 4.6) (end 5 -5.2) (layer F.SilkS) (width 0.381))
  (fp_line (start 5 -5.2) (end -5 -5.2) (layer F.SilkS) (width 0.381))
  (fp_line (start -5 -5.2) (end -5 4.6) (layer F.SilkS) (width 0.381))
  (pad 1 thru_hole circle (at -2.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (model walter/conn_mkds/mkds_1,5-2.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
