# ZMHW Modector

A Zoneminder Motion Sensor (https://www.zoneminder.com)

![Image of Prototype PCB](https://git.steakelectronics.com/adminguy/Electronics_Projects_2019/raw/branch/master/ZMHW_Modector/pics/DSCN1278.JPG)

* docs - Information on the modector, and implementation tips
* pcb - kicad source, and gerber files for a shield
* pics - pictures
* resources - notes, and relevant data sheets
* testsuite - arduino code to test that your hardware is correctly setup


Arduino code requires UIPEthernet Library.
In recent Arduino IDE:
Manage Libraries - UIPEthernet

Gerbers are labeled with CPU pin of each accessory, so for example,
you can use the DHT11 Sensor with pin D8 (see gerbers for more details).

This particular Motion Sensor uses the ZMTrigger.pl script of Zoneminder. For 
more details on how to configure ZMTrigger see https://wiki.zoneminder.com/ZMTrigger
