(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1~bpo9+1)

  (general
    (thickness 1.6002)
    (drawings 99)
    (tracks 530)
    (zones 0)
    (modules 88)
    (nets 1)
  )

  (page User 150.012 200)
  (title_block
    (title High-density-proto-board)
    (date "12 Jun 2014")
    (rev 0.10.a)
    (company "2014 - blog.spitzenpfeil.org")
  )

  (layers
    (0 Front signal)
    (31 Back signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )

  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2032)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.635)
    (via_drill 0.3302)
    (via_min_size 0.635)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.2)
    (mod_text_size 1 1)
    (mod_text_width 0.2)
    (pad_size 1.65 2)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber_files_50x50mm/"))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.635)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )

  (module my_parts:MADW__SIL-1 (layer Front) (tedit 53990693) (tstamp 539922C4)
    (at 24.765 88.9)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -2.032) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad "" np_thru_hole circle (at 0.09 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )

  (module my_parts:MADW__SIL-1 (layer Front) (tedit 53990681) (tstamp 53992279)
    (at 67.945 88.9)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -2.032) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad "" np_thru_hole circle (at -0.09 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )

  (module my_parts:MADW__SIL-1 (layer Front) (tedit 5398BCDC) (tstamp 5398C661)
    (at 22.86 66.04)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -2.032) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992735) (tstamp 5398AE22)
    (at 36.195 102.87)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992700) (tstamp 53999B57)
    (at 56.515 77.47)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999BBF)
    (at 61.595 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926F6) (tstamp 53999B64)
    (at 56.515 85.09)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926FD) (tstamp 53999BD9)
    (at 56.515 74.93)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992703) (tstamp 53999BB2)
    (at 56.515 80.01)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992706) (tstamp 53999B71)
    (at 56.515 82.55)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992724) (tstamp 53999C9C)
    (at 56.515 92.71)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992761) (tstamp 53999CA9)
    (at 56.515 102.87)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 5399275D) (tstamp 53999C5B)
    (at 56.515 100.33)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992759) (tstamp 53999C68)
    (at 56.515 97.79)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992756) (tstamp 53999C27)
    (at 56.515 95.25)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999B3D)
    (at 51.435 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999B30)
    (at 51.435 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999B4A)
    (at 51.435 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999BA5)
    (at 51.435 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999B7E)
    (at 51.435 83.82)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C8F)
    (at 51.435 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C82)
    (at 51.435 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C75)
    (at 51.435 99.06)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999D2B)
    (at 51.435 101.6)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999D1E)
    (at 51.435 104.14)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999BCC)
    (at 61.595 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999BE6)
    (at 61.595 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999B8B)
    (at 61.595 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999B98)
    (at 61.595 83.82)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999CC3)
    (at 61.595 104.14)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999CB6)
    (at 61.595 101.6)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C4E)
    (at 61.595 99.06)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C41)
    (at 61.595 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C34)
    (at 61.595 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999D04)
    (at 51.435 106.68)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999CD0)
    (at 61.595 106.68)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 5399272D) (tstamp 53999CDD)
    (at 56.515 107.95)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992727) (tstamp 53999CF7)
    (at 56.515 110.49)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999D11)
    (at 61.595 111.76)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999CEA)
    (at 51.435 111.76)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999C1A)
    (at 51.435 71.12)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999BF3)
    (at 61.595 71.12)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926FA) (tstamp 53999C00)
    (at 56.515 69.85)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 5399278F) (tstamp 53999C0D)
    (at 56.515 67.31)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 53999922)
    (at 61.595 66.04)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5399992F)
    (at 51.435 66.04)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B252)
    (at 31.115 66.04)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B247)
    (at 41.275 66.04)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926D7) (tstamp 5398B23C)
    (at 36.195 67.31)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926D4) (tstamp 5398B231)
    (at 36.195 69.85)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B226)
    (at 41.275 71.12)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B21B)
    (at 31.115 71.12)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B20E)
    (at 31.115 111.76)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B203)
    (at 41.275 111.76)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992717) (tstamp 5398B1C1)
    (at 36.195 110.49)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992732) (tstamp 5398B1AA)
    (at 36.195 107.95)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B189)
    (at 41.275 106.68)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B17E)
    (at 31.115 106.68)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 539BC05A)
    (at 41.275 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0EB)
    (at 41.275 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0E0)
    (at 41.275 99.06)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0D5)
    (at 41.275 101.6)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0CA)
    (at 41.275 104.14)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0BF)
    (at 41.275 83.82)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0B4)
    (at 41.275 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B0A9)
    (at 41.275 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B09E)
    (at 41.275 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398B080)
    (at 31.115 104.14)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AFF1)
    (at 31.115 101.6)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AFE6)
    (at 31.115 99.06)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AFDB)
    (at 31.115 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AFD0)
    (at 31.115 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AF99)
    (at 31.115 83.82)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AF8E)
    (at 31.115 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AF83)
    (at 31.115 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 539BBDEF)
    (at 31.115 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 53998995) (tstamp 5398AF15)
    (at 31.115 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 53992741) (tstamp 5398AE43)
    (at 36.195 95.25)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 5399273D) (tstamp 5398AE38)
    (at 36.195 97.79)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 5399273A) (tstamp 5398AE2D)
    (at 36.195 100.33)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539BC05D) (tstamp 539BC075)
    (at 36.195 92.71)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926C8) (tstamp 5398AE04)
    (at 36.195 82.55)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926CB) (tstamp 5398ADF9)
    (at 36.195 80.01)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926CD) (tstamp 5398ADEE)
    (at 36.195 77.47)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926D1) (tstamp 5398ADE3)
    (at 36.195 74.93)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8 (layer Front) (tedit 539926C5) (tstamp 5398ADD8)
    (at 36.195 85.09)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.794) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 1.27 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.81 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 6.35 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 0) (size 1.65 2) (drill 1.016) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AD21)
    (at 41.275 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module oshw-logo:OSHW-logo_silkscreen_5mm (layer Back) (tedit 0) (tstamp 5398B43E)
    (at 62.865 88.9)
    (fp_text reference G*** (at 0 -2.65176) (layer B.SilkS) hide
      (effects (font (size 0.22606 0.22606) (thickness 0.04318)) (justify mirror))
    )
    (fp_text value OSHW-logo_silkscreen_5mm (at 0 2.65176) (layer B.SilkS) hide
      (effects (font (size 0.22606 0.22606) (thickness 0.04318)) (justify mirror))
    )
    (fp_poly (pts (xy -1.51384 2.24536) (xy -1.48844 2.23012) (xy -1.43002 2.19456) (xy -1.3462 2.13868)
      (xy -1.24714 2.07264) (xy -1.14808 2.0066) (xy -1.0668 1.95326) (xy -1.01092 1.91516)
      (xy -0.98552 1.90246) (xy -0.97282 1.90754) (xy -0.9271 1.9304) (xy -0.85852 1.96596)
      (xy -0.81788 1.98628) (xy -0.75692 2.01168) (xy -0.7239 2.0193) (xy -0.71882 2.00914)
      (xy -0.69596 1.96088) (xy -0.6604 1.8796) (xy -0.61468 1.77038) (xy -0.5588 1.64338)
      (xy -0.50292 1.50876) (xy -0.4445 1.36906) (xy -0.38862 1.23444) (xy -0.34036 1.11506)
      (xy -0.29972 1.01854) (xy -0.27432 0.94996) (xy -0.26416 0.92202) (xy -0.2667 0.9144)
      (xy -0.29972 0.88392) (xy -0.35306 0.84328) (xy -0.47244 0.74676) (xy -0.58928 0.60198)
      (xy -0.6604 0.43688) (xy -0.68326 0.25146) (xy -0.66294 0.08128) (xy -0.5969 -0.08128)
      (xy -0.4826 -0.2286) (xy -0.3429 -0.33782) (xy -0.18034 -0.4064) (xy 0 -0.42926)
      (xy 0.17272 -0.40894) (xy 0.34036 -0.3429) (xy 0.48768 -0.23114) (xy 0.55118 -0.16002)
      (xy 0.63754 -0.01016) (xy 0.6858 0.14732) (xy 0.69088 0.18796) (xy 0.68326 0.36322)
      (xy 0.63246 0.5334) (xy 0.53848 0.68326) (xy 0.40894 0.80772) (xy 0.3937 0.81788)
      (xy 0.33528 0.8636) (xy 0.29464 0.89408) (xy 0.26416 0.91948) (xy 0.48768 1.45796)
      (xy 0.52324 1.54178) (xy 0.5842 1.6891) (xy 0.63754 1.8161) (xy 0.68072 1.9177)
      (xy 0.7112 1.98374) (xy 0.7239 2.01168) (xy 0.7239 2.01422) (xy 0.74422 2.01676)
      (xy 0.78486 2.00152) (xy 0.86106 1.96596) (xy 0.90932 1.94056) (xy 0.96774 1.91262)
      (xy 0.99314 1.90246) (xy 1.016 1.91516) (xy 1.06934 1.95072) (xy 1.15062 2.00406)
      (xy 1.24714 2.06756) (xy 1.33858 2.13106) (xy 1.4224 2.18694) (xy 1.48336 2.22504)
      (xy 1.51384 2.24282) (xy 1.51892 2.24282) (xy 1.54432 2.22758) (xy 1.59258 2.18694)
      (xy 1.66624 2.11836) (xy 1.77038 2.01422) (xy 1.78562 1.99898) (xy 1.87198 1.91262)
      (xy 1.94056 1.83896) (xy 1.98628 1.78816) (xy 2.00406 1.7653) (xy 1.98882 1.73482)
      (xy 1.95072 1.67386) (xy 1.89484 1.5875) (xy 1.82626 1.48844) (xy 1.64846 1.22936)
      (xy 1.74498 0.98552) (xy 1.77546 0.90932) (xy 1.81356 0.82042) (xy 1.8415 0.75438)
      (xy 1.85674 0.72644) (xy 1.88214 0.71628) (xy 1.95072 0.70104) (xy 2.04724 0.68072)
      (xy 2.16154 0.6604) (xy 2.2733 0.64008) (xy 2.37236 0.61976) (xy 2.44348 0.60706)
      (xy 2.4765 0.59944) (xy 2.48412 0.59436) (xy 2.49174 0.57912) (xy 2.49428 0.5461)
      (xy 2.49682 0.48514) (xy 2.49936 0.39116) (xy 2.49936 0.25146) (xy 2.49936 0.23622)
      (xy 2.49682 0.10668) (xy 2.49428 0) (xy 2.49174 -0.06604) (xy 2.48666 -0.09398)
      (xy 2.45618 -0.1016) (xy 2.38506 -0.11684) (xy 2.286 -0.13462) (xy 2.16662 -0.15748)
      (xy 2.159 -0.16002) (xy 2.04216 -0.18288) (xy 1.9431 -0.2032) (xy 1.87198 -0.21844)
      (xy 1.84404 -0.2286) (xy 1.83642 -0.23622) (xy 1.81356 -0.28194) (xy 1.78054 -0.3556)
      (xy 1.7399 -0.4445) (xy 1.7018 -0.53848) (xy 1.66878 -0.6223) (xy 1.64592 -0.68326)
      (xy 1.6383 -0.7112) (xy 1.64084 -0.71374) (xy 1.65862 -0.74168) (xy 1.69926 -0.80264)
      (xy 1.75514 -0.88646) (xy 1.82372 -0.98806) (xy 1.8288 -0.99568) (xy 1.89738 -1.09474)
      (xy 1.95326 -1.1811) (xy 1.98882 -1.23952) (xy 2.00406 -1.26746) (xy 2.00406 -1.27)
      (xy 1.9812 -1.30048) (xy 1.9304 -1.35636) (xy 1.85674 -1.43256) (xy 1.77038 -1.52146)
      (xy 1.74244 -1.54686) (xy 1.64338 -1.64338) (xy 1.57734 -1.70434) (xy 1.53416 -1.73736)
      (xy 1.51384 -1.74498) (xy 1.48336 -1.7272) (xy 1.41986 -1.68656) (xy 1.33604 -1.62814)
      (xy 1.23444 -1.55956) (xy 1.22682 -1.55448) (xy 1.12776 -1.4859) (xy 1.04394 -1.43002)
      (xy 0.98552 -1.38938) (xy 0.95758 -1.37414) (xy 0.95504 -1.37414) (xy 0.9144 -1.38684)
      (xy 0.84328 -1.41224) (xy 0.75438 -1.44526) (xy 0.66294 -1.48336) (xy 0.57912 -1.51892)
      (xy 0.51562 -1.54686) (xy 0.48514 -1.56464) (xy 0.47498 -1.6002) (xy 0.4572 -1.6764)
      (xy 0.43688 -1.778) (xy 0.41148 -1.89992) (xy 0.40894 -1.92024) (xy 0.38608 -2.03962)
      (xy 0.3683 -2.13868) (xy 0.35306 -2.20726) (xy 0.34544 -2.2352) (xy 0.3302 -2.23774)
      (xy 0.27178 -2.24282) (xy 0.18288 -2.24536) (xy 0.07366 -2.24536) (xy -0.0381 -2.24536)
      (xy -0.14732 -2.24282) (xy -0.2413 -2.24028) (xy -0.30988 -2.2352) (xy -0.33782 -2.23012)
      (xy -0.33782 -2.22758) (xy -0.34798 -2.18948) (xy -0.36576 -2.11582) (xy -0.38608 -2.01168)
      (xy -0.40894 -1.88976) (xy -0.41402 -1.8669) (xy -0.43688 -1.75006) (xy -0.4572 -1.651)
      (xy -0.4699 -1.58496) (xy -0.47752 -1.55702) (xy -0.49022 -1.55194) (xy -0.53848 -1.53162)
      (xy -0.61722 -1.4986) (xy -0.71628 -1.45796) (xy -0.94488 -1.36652) (xy -1.22682 -1.55702)
      (xy -1.25222 -1.5748) (xy -1.35382 -1.64338) (xy -1.4351 -1.69926) (xy -1.49352 -1.73736)
      (xy -1.51638 -1.75006) (xy -1.51892 -1.75006) (xy -1.54686 -1.72466) (xy -1.60274 -1.67132)
      (xy -1.67894 -1.59766) (xy -1.76784 -1.5113) (xy -1.83134 -1.44526) (xy -1.91008 -1.36652)
      (xy -1.95834 -1.31318) (xy -1.98628 -1.28016) (xy -1.9939 -1.25984) (xy -1.99136 -1.2446)
      (xy -1.97358 -1.21666) (xy -1.93294 -1.1557) (xy -1.87452 -1.06934) (xy -1.80594 -0.97028)
      (xy -1.75006 -0.88646) (xy -1.6891 -0.79248) (xy -1.651 -0.72644) (xy -1.63576 -0.69342)
      (xy -1.64084 -0.68072) (xy -1.65862 -0.62484) (xy -1.69418 -0.54102) (xy -1.73482 -0.44196)
      (xy -1.83388 -0.22098) (xy -1.97866 -0.19304) (xy -2.06756 -0.17526) (xy -2.18948 -0.1524)
      (xy -2.30886 -0.12954) (xy -2.49174 -0.09398) (xy -2.49936 0.58166) (xy -2.47142 0.59436)
      (xy -2.44348 0.60198) (xy -2.3749 0.61722) (xy -2.27838 0.63754) (xy -2.16154 0.65786)
      (xy -2.06502 0.67564) (xy -1.96596 0.69596) (xy -1.89484 0.70866) (xy -1.86436 0.71628)
      (xy -1.8542 0.72644) (xy -1.83134 0.7747) (xy -1.79578 0.8509) (xy -1.75514 0.94234)
      (xy -1.71704 1.03632) (xy -1.68148 1.12522) (xy -1.65862 1.19126) (xy -1.64846 1.22428)
      (xy -1.66116 1.25222) (xy -1.69926 1.31064) (xy -1.7526 1.39192) (xy -1.82118 1.49098)
      (xy -1.88722 1.5875) (xy -1.94564 1.67132) (xy -1.98374 1.73228) (xy -2.00152 1.76022)
      (xy -1.99136 1.778) (xy -1.95326 1.82626) (xy -1.8796 1.90246) (xy -1.76784 2.01168)
      (xy -1.75006 2.02946) (xy -1.6637 2.11328) (xy -1.59004 2.18186) (xy -1.5367 2.22758)
      (xy -1.51384 2.24536)) (layer B.SilkS) (width 0.00254))
  )

  (gr_text 15 (at 62.865 105.41) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 10 (at 50.165 105.41) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 5 (at 37.465 105.41) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 1 (at 27.305 105.41) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 15 (at 62.865 72.39) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 10 (at 50.165 72.39) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 5 (at 37.465 72.39) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 1 (at 27.305 72.39) (layer B.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)) (justify mirror))
  )
  (gr_text 15 (at 62.865 105.41) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 10 (at 50.165 105.41) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 5 (at 37.465 105.41) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 1 (at 27.305 105.41) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 15 (at 62.865 72.39) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 10 (at 50.165 72.39) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 5 (at 37.465 72.39) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 1 (at 27.305 72.39) (layer F.SilkS)
    (effects (font (size 0.9 0.9) (thickness 0.2)))
  )
  (gr_text 1 (at 27.305 88.9) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_line (start 27.305 90.17) (end 27.305 91.44) (layer B.SilkS) (width 0.3))
  (gr_line (start 27.305 86.36) (end 27.305 87.63) (layer B.SilkS) (width 0.3))
  (gr_arc (start 25.273 110.617) (end 25.273 113.665) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 25.273 67.183) (end 22.225 67.183) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 67.437 110.617) (end 70.485 110.617) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 67.437 67.183) (end 67.437 64.135) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 70.485 67.183) (end 70.485 110.617) (layer Edge.Cuts) (width 0.2) (tstamp 53992336))
  (gr_text J (at 67.31 102.997) (layer B.SilkS) (tstamp 5398FE88)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text I (at 67.31 100.457) (layer B.SilkS) (tstamp 5398FE89)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text H (at 67.31 97.917) (layer B.SilkS) (tstamp 5398FE8A)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text G (at 67.31 95.377) (layer B.SilkS) (tstamp 5398FE8B)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text F (at 67.31 92.837) (layer B.SilkS) (tstamp 5398FE8C)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text E (at 67.31 85.217) (layer B.SilkS) (tstamp 5398FE8F)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text D (at 67.31 82.677) (layer B.SilkS) (tstamp 5398FE90)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text C (at 67.31 80.137) (layer B.SilkS) (tstamp 5398FE91)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text B (at 67.31 77.597) (layer B.SilkS) (tstamp 5398FE92)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text A (at 67.31 75.057) (layer B.SilkS) (tstamp 5398FE93)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text J (at 25.146 102.87) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text I (at 25.146 100.33) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text H (at 25.146 97.79) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text G (at 25.146 95.25) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text F (at 25.273 92.71) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text E (at 25.146 85.09) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text D (at 25.146 82.55) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text C (at 25.146 80.01) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text B (at 25.146 77.47) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text A (at 25.146 74.93) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_line (start 62.865 90.17) (end 62.865 91.44) (layer F.SilkS) (width 0.3))
  (gr_line (start 62.865 86.36) (end 62.865 87.63) (layer F.SilkS) (width 0.3))
  (gr_line (start 50.165 90.17) (end 50.165 91.44) (layer F.SilkS) (width 0.3))
  (gr_line (start 50.165 86.36) (end 50.165 87.63) (layer F.SilkS) (width 0.3))
  (gr_line (start 27.305 86.36) (end 27.305 87.63) (layer F.SilkS) (width 0.3) (tstamp 539928E0))
  (gr_line (start 27.305 90.17) (end 27.305 91.44) (layer F.SilkS) (width 0.3))
  (gr_line (start 37.465 90.17) (end 37.465 91.44) (layer F.SilkS) (width 0.3))
  (gr_line (start 37.465 86.36) (end 37.465 87.63) (layer F.SilkS) (width 0.3))
  (gr_text 15 (at 62.865 88.9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text 10 (at 50.165 88.9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text 5 (at 37.465 88.9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text 1 (at 27.305 88.9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text - (at 25.146 110.363) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 25.146 107.823) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 67.31 110.363) (layer B.SilkS) (tstamp 5398FE87)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 67.31 107.823) (layer B.SilkS) (tstamp 5398FE8D)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 25.146 69.723) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 25.146 67.183) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 67.31 69.723) (layer B.SilkS) (tstamp 5398FE8E)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 67.31 67.183) (layer B.SilkS) (tstamp 5398FE94)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_line (start 26.67 109.22) (end 66.294 109.22) (angle 90) (layer B.SilkS) (width 0.4))
  (gr_line (start 26.67 68.58) (end 66.294 68.58) (angle 90) (layer B.SilkS) (width 0.4))
  (gr_text A (at 67.31 75.057) (layer F.SilkS) (tstamp 5398FE7A)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text B (at 67.31 77.597) (layer F.SilkS) (tstamp 5398FE7B)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text C (at 67.31 80.137) (layer F.SilkS) (tstamp 5398FE7C)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text D (at 67.31 82.677) (layer F.SilkS) (tstamp 5398FE7D)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text E (at 67.31 85.217) (layer F.SilkS) (tstamp 5398FE7E)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text F (at 67.31 92.837) (layer F.SilkS) (tstamp 5398FE82)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text G (at 67.31 95.377) (layer F.SilkS) (tstamp 5398FE83)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text H (at 67.31 97.917) (layer F.SilkS) (tstamp 5398FE84)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text I (at 67.31 100.457) (layer F.SilkS) (tstamp 5398FE85)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text J (at 67.31 102.997) (layer F.SilkS) (tstamp 5398FE81)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text J (at 25.146 102.87) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text I (at 25.146 100.33) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text H (at 25.146 97.79) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text G (at 25.146 95.25) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text F (at 25.146 92.71) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text E (at 25.146 85.09) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text D (at 25.146 82.55) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text C (at 25.146 80.01) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text B (at 25.146 77.47) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text A (at 25.146 74.93) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)))
  )
  (gr_text + (at 67.31 107.823) (layer F.SilkS) (tstamp 5398FE80)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 67.31 110.363) (layer F.SilkS) (tstamp 5398FE86)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 25.146 110.363) (layer F.SilkS) (tstamp 5399BB0A)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 25.146 107.823) (layer F.SilkS) (tstamp 5399BB09)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 67.31 67.183) (layer F.SilkS) (tstamp 5398FE79)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 67.31 69.723) (layer F.SilkS) (tstamp 5398FE7F)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text - (at 25.146 69.723) (layer F.SilkS) (tstamp 5399BB03)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_text + (at 25.146 67.183) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.35)) (justify mirror))
  )
  (gr_line (start 26.67 109.22) (end 66.294 109.22) (layer F.SilkS) (width 0.4))
  (gr_line (start 26.67 68.58) (end 66.294 68.58) (layer F.SilkS) (width 0.4))
  (gr_line (start 25.273 113.665) (end 67.437 113.665) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 22.225 67.183) (end 22.225 110.617) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 67.437 64.135) (end 25.273 64.135) (layer Edge.Cuts) (width 0.2) (tstamp 5398B62E))

  (segment (start 65.405 102.87) (end 65.405 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 103.505) (end 64.77 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 103.505) (end 66.04 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 101.6) (end 64.77 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 99.06) (end 66.04 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 96.52) (end 64.77 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 93.98) (end 66.04 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 102.87) (end 62.865 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 103.505) (end 63.5 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 103.505) (end 62.23 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 102.87) (end 60.325 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 103.505) (end 60.96 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 103.505) (end 59.69 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 102.87) (end 57.785 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 103.505) (end 58.42 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 103.505) (end 57.15 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 102.87) (end 55.245 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 103.505) (end 55.88 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 103.505) (end 54.61 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 102.87) (end 52.705 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 103.505) (end 53.34 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 103.505) (end 52.07 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 102.87) (end 50.165 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 103.505) (end 50.8 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 103.505) (end 49.53 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 102.87) (end 47.625 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 103.505) (end 48.26 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 103.505) (end 46.99 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 101.6) (end 46.99 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 101.6) (end 49.53 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 101.6) (end 52.07 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 101.6) (end 54.61 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 101.6) (end 57.15 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 101.6) (end 59.69 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 101.6) (end 62.23 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 99.06) (end 63.5 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 99.06) (end 60.96 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 99.06) (end 58.42 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 99.06) (end 55.88 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 99.06) (end 53.34 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 99.06) (end 50.8 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 99.06) (end 48.26 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 96.52) (end 46.99 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 96.52) (end 49.53 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 96.52) (end 52.07 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 96.52) (end 54.61 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 96.52) (end 57.15 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 96.52) (end 59.69 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 96.52) (end 62.23 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 93.98) (end 63.5 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 93.98) (end 60.96 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 93.98) (end 58.42 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 93.98) (end 55.88 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 93.98) (end 53.34 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 93.98) (end 50.8 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 93.98) (end 48.26 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 78.74) (end 66.04 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 81.28) (end 64.77 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 83.82) (end 66.04 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 83.82) (end 63.5 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 81.28) (end 62.23 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 78.74) (end 63.5 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 76.2) (end 66.04 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 76.2) (end 63.5 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 74.93) (end 65.405 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 74.295) (end 66.04 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 74.295) (end 64.77 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 74.93) (end 62.865 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 74.295) (end 63.5 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 74.295) (end 62.23 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 74.93) (end 60.325 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 74.295) (end 60.96 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 74.295) (end 59.69 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 74.93) (end 57.785 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 74.295) (end 58.42 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 74.295) (end 57.15 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 74.93) (end 55.245 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 74.295) (end 55.88 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 74.295) (end 54.61 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 74.93) (end 52.705 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 74.295) (end 53.34 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 74.295) (end 52.07 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 74.93) (end 50.165 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 74.295) (end 50.8 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 74.295) (end 49.53 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 74.93) (end 47.625 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 74.295) (end 48.26 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 74.295) (end 46.99 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 81.28) (end 59.69 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 83.82) (end 60.96 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 83.82) (end 57.15 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 81.28) (end 58.42 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 81.28) (end 54.61 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 83.82) (end 55.88 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 83.82) (end 52.07 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 81.28) (end 53.34 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 81.28) (end 49.53 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 83.82) (end 50.8 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 83.82) (end 48.26 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 81.28) (end 48.26 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 78.74) (end 48.26 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 78.74) (end 49.53 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 78.74) (end 52.07 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 78.74) (end 54.61 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 78.74) (end 57.15 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 78.74) (end 59.69 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 76.2) (end 60.96 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 76.2) (end 58.42 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 76.2) (end 55.88 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 76.2) (end 53.34 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 76.2) (end 50.8 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 76.2) (end 48.26 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 92.71) (end 65.405 100.965) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 100.965) (end 65.405 102.87) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 102.87) (end 62.865 94.615) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 94.615) (end 62.865 92.71) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 92.71) (end 60.325 100.33) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 100.33) (end 60.325 102.87) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 102.87) (end 57.785 94.615) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 94.615) (end 57.785 92.71) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 92.71) (end 55.245 100.965) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 100.965) (end 55.245 102.87) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 102.87) (end 52.705 94.615) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 94.615) (end 52.705 92.71) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 92.71) (end 50.165 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 102.87) (end 47.625 94.615) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 94.615) (end 47.625 92.71) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 85.09) (end 65.405 78.105) (width 0.4064) (layer Back) (net 0))
  (segment (start 65.405 78.105) (end 65.405 74.93) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.865 74.93) (end 62.865 85.09) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 85.09) (end 60.325 76.835) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.325 76.835) (end 60.325 74.93) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 74.93) (end 57.785 80.645) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.785 80.645) (end 57.785 85.09) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.245 85.09) (end 55.245 74.93) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 74.93) (end 52.705 81.915) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.705 81.915) (end 52.705 85.09) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 85.09) (end 50.165 76.835) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 76.835) (end 50.165 74.93) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 74.93) (end 47.625 85.09) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 71.12) (end 57.15 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 70.485) (end 57.785 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 71.12) (end 58.42 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 70.485) (end 57.785 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 71.12) (end 59.69 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 70.485) (end 60.325 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 71.12) (end 60.96 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 70.485) (end 60.325 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 71.12) (end 62.23 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 70.485) (end 62.865 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 71.12) (end 63.5 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 70.485) (end 62.865 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 71.12) (end 64.77 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 70.485) (end 65.405 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 71.12) (end 66.04 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 70.485) (end 65.405 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 66.04) (end 66.04 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 66.675) (end 65.405 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 66.04) (end 64.77 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 66.675) (end 65.405 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 66.04) (end 63.5 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 66.675) (end 62.865 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 66.04) (end 62.23 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 66.675) (end 62.865 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 66.04) (end 60.96 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 66.675) (end 60.325 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 66.04) (end 59.69 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 66.675) (end 60.325 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 66.04) (end 58.42 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 66.675) (end 57.785 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 66.04) (end 57.15 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 66.675) (end 57.785 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 71.12) (end 44.45 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 70.485) (end 45.085 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 71.12) (end 45.72 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 70.485) (end 45.085 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 71.12) (end 46.99 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 70.485) (end 47.625 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 71.12) (end 48.26 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 70.485) (end 47.625 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 71.12) (end 49.53 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 70.485) (end 50.165 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 71.12) (end 50.8 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 70.485) (end 50.165 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 71.12) (end 52.07 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 70.485) (end 52.705 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 71.12) (end 53.34 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 70.485) (end 52.705 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 71.12) (end 54.61 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 70.485) (end 55.245 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 71.12) (end 55.88 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 70.485) (end 55.245 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 66.04) (end 55.88 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 66.675) (end 55.245 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 66.04) (end 54.61 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 66.675) (end 55.245 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 66.04) (end 53.34 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 66.675) (end 52.705 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 66.04) (end 52.07 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 66.675) (end 52.705 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 66.04) (end 50.8 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 66.675) (end 50.165 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 66.04) (end 49.53 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 66.675) (end 50.165 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 66.04) (end 48.26 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 66.675) (end 47.625 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 66.04) (end 46.99 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 66.675) (end 47.625 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 66.04) (end 45.72 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 66.675) (end 45.085 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 66.04) (end 44.45 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 66.675) (end 45.085 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 71.12) (end 36.83 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 70.485) (end 37.465 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 71.12) (end 38.1 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 70.485) (end 37.465 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 71.12) (end 39.37 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 70.485) (end 40.005 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 71.12) (end 40.64 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 70.485) (end 40.005 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 71.12) (end 41.91 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 70.485) (end 42.545 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 71.12) (end 43.18 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 70.485) (end 42.545 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 66.04) (end 43.18 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 66.675) (end 42.545 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 66.04) (end 41.91 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 66.675) (end 42.545 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 66.04) (end 40.64 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 66.675) (end 40.005 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 66.04) (end 39.37 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 66.675) (end 40.005 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 66.04) (end 38.1 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 66.675) (end 37.465 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 66.04) (end 36.83 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 66.675) (end 37.465 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 71.12) (end 26.67 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 70.485) (end 27.305 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 71.12) (end 27.94 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 70.485) (end 27.305 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 71.12) (end 29.21 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 70.485) (end 29.845 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 71.12) (end 30.48 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 70.485) (end 29.845 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 71.12) (end 31.75 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 70.485) (end 32.385 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 71.12) (end 33.02 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 70.485) (end 32.385 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 71.12) (end 34.29 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 70.485) (end 34.925 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 71.12) (end 35.56 70.485) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 70.485) (end 34.925 69.85) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 66.04) (end 35.56 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 66.675) (end 34.925 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 66.04) (end 34.29 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 66.675) (end 34.925 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 66.04) (end 33.02 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 66.675) (end 32.385 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 66.04) (end 31.75 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 66.675) (end 32.385 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 66.04) (end 30.48 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 66.675) (end 29.845 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 66.04) (end 29.21 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 66.675) (end 29.845 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 66.04) (end 27.94 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 66.675) (end 27.305 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 66.04) (end 26.67 66.675) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 66.675) (end 27.305 67.31) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 111.76) (end 62.23 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 111.125) (end 62.865 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 111.76) (end 63.5 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 111.125) (end 62.865 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 111.76) (end 64.77 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 111.125) (end 65.405 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 111.76) (end 66.04 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 111.125) (end 65.405 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 106.68) (end 66.04 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 66.04 107.315) (end 65.405 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 106.68) (end 64.77 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 64.77 107.315) (end 65.405 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 106.68) (end 63.5 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 63.5 107.315) (end 62.865 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 106.68) (end 62.23 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 107.315) (end 62.865 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 111.76) (end 60.96 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 111.125) (end 60.325 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 111.76) (end 59.69 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 111.125) (end 60.325 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 106.68) (end 60.96 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 60.96 107.315) (end 60.325 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 106.68) (end 59.69 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 59.69 107.315) (end 60.325 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 106.68) (end 57.15 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 107.315) (end 57.785 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 106.68) (end 58.42 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 107.315) (end 57.785 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 111.76) (end 58.42 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 58.42 111.125) (end 57.785 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 111.76) (end 57.15 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 57.15 111.125) (end 57.785 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 111.76) (end 55.88 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 111.125) (end 55.245 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 111.76) (end 54.61 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 111.125) (end 55.245 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 106.68) (end 55.88 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 55.88 107.315) (end 55.245 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 106.68) (end 54.61 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 54.61 107.315) (end 55.245 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 106.68) (end 49.53 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 107.315) (end 50.165 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 106.68) (end 50.8 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 107.315) (end 50.165 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 106.68) (end 52.07 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 107.315) (end 52.705 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 106.68) (end 53.34 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 107.315) (end 52.705 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 111.76) (end 53.34 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 53.34 111.125) (end 52.705 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 111.76) (end 52.07 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 52.07 111.125) (end 52.705 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 111.76) (end 50.8 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 111.125) (end 50.165 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 111.76) (end 49.53 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 111.125) (end 50.165 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 111.76) (end 48.26 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 111.125) (end 47.625 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 111.76) (end 46.99 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 111.125) (end 47.625 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 106.68) (end 48.26 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 107.315) (end 47.625 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 106.68) (end 46.99 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 107.315) (end 47.625 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 111.76) (end 45.72 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 111.125) (end 45.085 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 111.76) (end 44.45 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 111.125) (end 45.085 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 106.68) (end 45.72 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 107.315) (end 45.085 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 106.68) (end 44.45 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 107.315) (end 45.085 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 106.68) (end 43.18 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 107.315) (end 42.545 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 111.76) (end 43.18 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 111.125) (end 42.545 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 111.76) (end 41.91 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 111.125) (end 42.545 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 106.68) (end 41.91 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 107.315) (end 42.545 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 106.68) (end 40.64 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 107.315) (end 40.005 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 111.76) (end 40.64 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 111.125) (end 40.005 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 111.76) (end 39.37 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 111.125) (end 40.005 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 106.68) (end 39.37 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 107.315) (end 40.005 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 106.68) (end 36.83 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 107.315) (end 37.465 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 106.68) (end 38.1 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 107.315) (end 37.465 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 111.76) (end 38.1 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 111.125) (end 37.465 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 111.76) (end 36.83 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 111.125) (end 37.465 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 111.76) (end 35.56 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 111.125) (end 34.925 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 111.76) (end 34.29 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 111.125) (end 34.925 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 111.76) (end 33.02 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 111.125) (end 32.385 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 111.76) (end 31.75 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 111.125) (end 32.385 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 106.68) (end 35.56 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 107.315) (end 34.925 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 106.68) (end 34.29 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 107.315) (end 34.925 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 106.68) (end 33.02 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 107.315) (end 32.385 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 106.68) (end 31.75 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 107.315) (end 32.385 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 106.68) (end 30.48 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 107.315) (end 29.845 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 106.68) (end 29.21 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 107.315) (end 29.845 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 111.76) (end 30.48 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 111.125) (end 29.845 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 111.76) (end 29.21 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 111.125) (end 29.845 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 111.76) (end 27.94 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 111.125) (end 27.305 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 111.76) (end 26.67 111.125) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 111.125) (end 27.305 110.49) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 106.68) (end 26.67 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 107.315) (end 27.305 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 106.68) (end 27.94 107.315) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 107.315) (end 27.305 107.95) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.305 74.295) (end 26.67 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.305 85.09) (end 27.305 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 74.295) (end 29.21 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 85.09) (end 29.845 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 74.295) (end 31.75 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 85.09) (end 32.385 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 74.295) (end 34.29 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 85.09) (end 34.925 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 74.295) (end 36.83 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 85.09) (end 37.465 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 74.295) (end 39.37 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 85.09) (end 40.005 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 74.295) (end 41.91 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 85.09) (end 42.545 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 74.295) (end 44.45 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 85.09) (end 45.085 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.305 103.505) (end 26.67 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.305 92.71) (end 27.305 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 103.505) (end 29.21 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 92.71) (end 29.845 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 103.505) (end 31.75 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 92.71) (end 32.385 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 103.505) (end 34.29 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 92.71) (end 34.925 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 103.505) (end 36.83 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 92.71) (end 37.465 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 103.505) (end 39.37 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 92.71) (end 40.005 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 103.505) (end 41.91 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 92.71) (end 42.545 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 103.505) (end 44.45 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 92.71) (end 45.085 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 73.66) (end 27.305 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 74.295) (end 30.48 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 74.93) (end 29.845 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 74.295) (end 33.02 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 74.93) (end 32.385 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 74.295) (end 35.56 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 74.93) (end 34.925 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 74.295) (end 38.1 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 74.93) (end 37.465 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 74.295) (end 40.64 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 74.93) (end 40.005 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 74.295) (end 43.18 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 74.93) (end 42.545 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 74.295) (end 45.72 73.66) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 74.93) (end 45.085 74.295) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.305 103.505) (end 27.94 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.305 102.87) (end 27.305 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 103.505) (end 30.48 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.845 102.87) (end 29.845 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 103.505) (end 33.02 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 32.385 102.87) (end 32.385 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 103.505) (end 35.56 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.925 102.87) (end 34.925 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 103.505) (end 38.1 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 37.465 102.87) (end 37.465 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 103.505) (end 40.64 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.005 102.87) (end 40.005 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 103.505) (end 43.18 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 102.87) (end 42.545 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 103.505) (end 45.72 104.14) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 102.87) (end 45.085 103.505) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 76.2) (end 27.94 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 76.2) (end 30.48 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 78.74) (end 29.21 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 78.74) (end 26.67 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 81.28) (end 27.94 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 81.28) (end 30.48 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 83.82) (end 29.21 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 83.82) (end 26.67 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 83.82) (end 33.02 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 81.28) (end 31.75 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 78.74) (end 33.02 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 76.2) (end 31.75 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 76.2) (end 35.56 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 78.74) (end 34.29 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 81.28) (end 35.56 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 83.82) (end 34.29 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 83.82) (end 38.1 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 81.28) (end 36.83 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 78.74) (end 38.1 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 76.2) (end 36.83 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 76.2) (end 40.64 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 78.74) (end 39.37 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 81.28) (end 40.64 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 83.82) (end 39.37 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 83.82) (end 43.18 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 81.28) (end 41.91 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 78.74) (end 43.18 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 76.2) (end 41.91 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 76.2) (end 45.72 76.2) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 78.74) (end 44.45 78.74) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 81.28) (end 45.72 81.28) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 83.82) (end 44.45 83.82) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 101.6) (end 26.67 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 99.06) (end 27.94 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 27.94 96.52) (end 26.67 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 26.67 93.98) (end 27.94 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 93.98) (end 30.48 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 96.52) (end 29.21 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 29.21 99.06) (end 30.48 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 30.48 101.6) (end 29.21 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 101.6) (end 33.02 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 99.06) (end 31.75 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 31.75 96.52) (end 33.02 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 33.02 93.98) (end 31.75 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 93.98) (end 35.56 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 93.98) (end 38.1 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 101.6) (end 35.56 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 35.56 99.06) (end 34.29 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 96.52) (end 35.56 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 96.52) (end 38.1 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 38.1 99.06) (end 36.83 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 36.83 101.6) (end 38.1 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 101.6) (end 40.64 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 99.06) (end 39.37 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 39.37 96.52) (end 40.64 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 40.64 93.98) (end 39.37 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 93.98) (end 43.18 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 96.52) (end 41.91 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 99.06) (end 43.18 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 101.6) (end 41.91 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 101.6) (end 45.72 101.6) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 99.06) (end 44.45 99.06) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 96.52) (end 45.72 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 93.98) (end 44.45 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 62.23 67.31) (end 65.405 67.31) (width 1.27) (layer Back) (net 0))
  (segment (start 27.305 67.31) (end 62.23 67.31) (width 1.27) (layer Back) (net 0))
  (segment (start 29.21 69.85) (end 27.305 69.85) (width 1.27) (layer Back) (net 0))
  (segment (start 65.405 69.85) (end 29.21 69.85) (width 1.27) (layer Back) (net 0))
  (segment (start 63.5 107.95) (end 65.405 107.95) (width 1.27) (layer Back) (net 0))
  (segment (start 27.305 107.95) (end 63.5 107.95) (width 1.27) (layer Back) (net 0))
  (segment (start 27.305 110.49) (end 65.405 110.49) (width 1.27) (layer Back) (net 0))

)
