(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1~bpo9+1)

  (general
    (thickness 1.6002)
    (drawings 16)
    (tracks 57)
    (zones 0)
    (modules 21)
    (nets 1)
  )

  (page User 150.012 200)
  (title_block
    (title High-density-proto-board)
    (date "12 Jun 2014")
    (rev 0.10.a)
    (company "2014 - blog.spitzenpfeil.org")
  )

  (layers
    (0 Front signal)
    (31 Back signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )

  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2032)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.635)
    (via_drill 0.3302)
    (via_min_size 0.635)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.2)
    (mod_text_size 1 1)
    (mod_text_width 0.2)
    (pad_size 1.76 0.65)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers_rev1/"))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.635)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E955CE5) (tstamp 5E9573FA)
    (at 33.02 69.215)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E955CE5) (tstamp 5E9573E0)
    (at 35.56 69.215)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E955CE5) (tstamp 5E9572D4)
    (at 45.72 69.215)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E955CE5) (tstamp 5E9572BA)
    (at 43.18 69.215)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E955CE5) (tstamp 5E9572A0)
    (at 40.64 69.215)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E977E5E)
    (at 38.608 59.944)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E977E2E)
    (at 40.64 56.896 270)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E977E04)
    (at 40.894 64.643)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E977DD9)
    (at 38.608 61.849)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E958158)
    (at 35.687 57.15)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E95812E)
    (at 33.782 57.15)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E958104)
    (at 31.877 57.15)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E9580D9)
    (at 35.687 64.135)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E9580AF)
    (at 33.782 64.135)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer Front) (tedit 5E804215) (tstamp 5E958082)
    (at 31.877 64.135)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.525 -0.635) (end 1.05 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 -0.635) (end 1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.05 0.635) (end -1.05 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 0.635) (end -1.05 -0.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.05 -0.11) (end -0.525 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.11 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.76) (end 1.11 0.695) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0.76) (end -0.563471 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.563471 0.76) (end 1.11 0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 0) (end -1.11 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.11 -0.76) (end 0 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.15) (end -1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 1.15) (end 1.55 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 1.15) (end 1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 -1.15) (end -1.55 -1.15) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer Front) (tedit 5E6DC4FF) (tstamp 5E79B29C)
    (at 49.022 65.786)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-1 (layer Front) (tedit 5398BCDC) (tstamp 5398C661)
    (at 22.86 66.04)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -2.032) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer Front) (tedit 5E955025) (tstamp 5E958080)
    (at 33.782 60.579 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference REF** (at 0 -2.9 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOT-23-6_Handsoldering (at 0 2.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -2.4 -1.8) (end 2.4 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1.8) (end 2.4 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 1.8) (end -2.4 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1.8) (end -2.4 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.61) (end -2.05 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprintslocal:QFN-16_4x4_Pitch0.5mm_ADXL_test1 (layer Front) (tedit 5E9558B8) (tstamp 5E971A9D)
    (at 42.64 60.575)
    (attr smd)
    (fp_text reference REF353 (at 0 -4) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value QFN-16_4x4_Pitch0.5mm (at 0 4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -2) (end -2 -1) (layer F.Fab) (width 0.15))
    (fp_line (start -2 -1) (end -2 2) (layer F.Fab) (width 0.15))
    (fp_line (start -2 2) (end 2 2) (layer F.Fab) (width 0.15))
    (fp_line (start 2 2) (end 2 -2) (layer F.Fab) (width 0.15))
    (fp_line (start 2 -2) (end -1 -2) (layer F.Fab) (width 0.15))
    (fp_line (start 1.25 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.15 -2.15) (end 2.15 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.25 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.15 2.15) (end 2.15 1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.25 2.15) (end -2.15 2.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.15 2.15) (end -2.15 1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.25 -2.15) (end -3 -2.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.25 -3.25) (end 3.25 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 -3.25) (end 3.25 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 3.25) (end -3.25 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.25 3.25) (end -3.25 -3.25) (layer F.CrtYd) (width 0.05))
    (pad 1 smd oval (at -2 -0.75 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 2 smd oval (at -2 -0.25 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 3 smd oval (at -2 0.25 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 4 smd oval (at -2 0.75 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 5 smd oval (at -0.75 2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 6 smd oval (at -0.25 2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 7 smd oval (at 0.25 2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 8 smd oval (at 0.75 2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 9 smd oval (at 2 0.75 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 10 smd oval (at 2 0.25 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 11 smd oval (at 2 -0.25 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 12 smd oval (at 2 -0.75 90) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 13 smd oval (at 0.75 -2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 14 smd oval (at 0.25 -2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 15 smd oval (at -0.25 -2) (size 0.25 2) (layers Front F.Paste F.Mask))
    (pad 16 smd oval (at -0.75 -2) (size 0.25 2) (layers Front F.Paste F.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E955CE5) (tstamp 5E957283)
    (at 38.1 69.215)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0805_2012Metric (layer Front) (tedit 5E955EA0) (tstamp 5E958389)
    (at 44.1175 66.04)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference REF** (at 0 -1.65) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C_0805_2012Metric (at 0 1.65) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.258578 0.71) (end 0.258578 0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.258578 -0.71) (end 0.258578 -0.71) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 30.48 70.485) (end 31.75 70.485) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 30.48 55.88) (end 30.48 70.485) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 46.355 55.88) (end 30.48 55.88) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 52.07 64.77) (end 46.355 55.88) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 52.07 67.31) (end 52.07 64.77) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 48.895 70.485) (end 52.07 67.31) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 31.75 70.485) (end 48.895 70.485) (layer Edge.Cuts) (width 0.2))
  (gr_text GND (at 43.18 64.77) (layer F.SilkS) (tstamp 5E957514)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text 1.8-3.3v (at 43.815 56.515) (layer F.SilkS) (tstamp 5E957510)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text zout (at 38.1 56.515) (layer F.SilkS) (tstamp 5E957509)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text xout (at 40.64 66.675) (layer F.SilkS) (tstamp 5E957505)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text "yout\n" (at 37.465 63.5) (layer F.SilkS) (tstamp 5E9574BC)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text st (at 36.195 60.325) (layer F.SilkS) (tstamp 5E9574B8)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text "ADXL337\n" (at 48.26 60.452 123.5) (layer F.SilkS) (tstamp 5E977EA0)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text "Only solder pads\nyou need." (at 35.0139 66.5861) (layer F.SilkS) (tstamp 5E977D3C)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text 1 (at 38.1 58.547) (layer F.SilkS) (tstamp 5E977CD7)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )

  (segment (start 42.39 58.575) (end 42.39 56.67) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.39 56.67) (end 42.545 56.515) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.89 57.3718) (end 43.18 57.0818) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.89 58.575) (end 42.89 57.3718) (width 0.2032) (layer Front) (net 0))
  (segment (start 43.18 57.0818) (end 43.18 56.515) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.545 56.515) (end 43.18 56.515) (width 0.2032) (layer Front) (net 0))
  (segment (start 43.18 56.515) (end 45.72 56.515) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.39 62.575) (end 42.39 64.996) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.39 64.996) (end 42.672 65.278) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.672 65.278) (end 42.799 65.278) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.89 62.575) (end 42.89 65.242) (width 0.2032) (layer Front) (net 0))
  (segment (start 32.3038 61.929) (end 32.832 61.929) (width 0.2032) (layer Front) (net 0))
  (segment (start 31.877 62.3558) (end 32.3038 61.929) (width 0.2032) (layer Front) (net 0))
  (segment (start 31.877 64.135) (end 31.877 62.3558) (width 0.2032) (layer Front) (net 0))
  (segment (start 33.782 64.135) (end 33.782 61.929) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.2602 61.929) (end 34.732 61.929) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.687 62.3558) (end 35.2602 61.929) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.687 64.135) (end 35.687 62.3558) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.687 57.857106) (end 35.687 57.15) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.687 58.8022) (end 35.687 57.857106) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.2602 59.229) (end 35.687 58.8022) (width 0.2032) (layer Front) (net 0))
  (segment (start 34.732 59.229) (end 35.2602 59.229) (width 0.2032) (layer Front) (net 0))
  (segment (start 33.782 59.229) (end 33.782 57.15) (width 0.2032) (layer Front) (net 0))
  (segment (start 31.877 58.8022) (end 31.877 57.857106) (width 0.2032) (layer Front) (net 0))
  (segment (start 31.877 57.857106) (end 31.877 57.15) (width 0.2032) (layer Front) (net 0))
  (segment (start 32.3038 59.229) (end 31.877 58.8022) (width 0.2032) (layer Front) (net 0))
  (segment (start 32.832 59.229) (end 32.3038 59.229) (width 0.2032) (layer Front) (net 0))
  (segment (start 41.89 57.7) (end 41.086 56.896) (width 0.2032) (layer Front) (net 0))
  (segment (start 41.086 56.896) (end 40.64 56.896) (width 0.2032) (layer Front) (net 0))
  (segment (start 41.89 58.575) (end 41.89 57.7) (width 0.2032) (layer Front) (net 0))
  (segment (start 38.989 60.325) (end 38.608 59.944) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.64 60.325) (end 38.989 60.325) (width 0.2032) (layer Front) (net 0))
  (segment (start 39.132 61.325) (end 38.608 61.849) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.64 61.325) (end 39.132 61.325) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.894 63.935894) (end 40.894 64.643) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.894 63.2428) (end 40.894 63.935894) (width 0.2032) (layer Front) (net 0))
  (segment (start 41.5618 62.575) (end 40.894 63.2428) (width 0.2032) (layer Front) (net 0))
  (segment (start 41.89 62.575) (end 41.5618 62.575) (width 0.2032) (layer Front) (net 0))
  (segment (start 43.18 65.532) (end 43.18 69.215) (width 0.2032) (layer Front) (net 0))
  (segment (start 42.89 65.242) (end 43.18 65.532) (width 0.2032) (layer Front) (net 0))
  (segment (start 46.569999 57.364999) (end 45.72 56.515) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.894 68.961) (end 40.64 69.215) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.894 64.643) (end 40.894 68.961) (width 0.2032) (layer Front) (net 0))
  (segment (start 38.608 68.707) (end 38.1 69.215) (width 0.2032) (layer Front) (net 0))
  (segment (start 38.608 61.849) (end 38.608 68.707) (width 0.2032) (layer Front) (net 0))
  (segment (start 37.465 61.087) (end 38.608 59.944) (width 0.2032) (layer Front) (net 0))
  (segment (start 37.465 67.31) (end 37.465 61.087) (width 0.2032) (layer Front) (net 0))
  (segment (start 35.56 69.215) (end 37.465 67.31) (width 0.2032) (layer Front) (net 0))
  (segment (start 36.83 65.405) (end 36.83 59.055) (width 0.2032) (layer Front) (net 0))
  (segment (start 33.02 69.215) (end 36.83 65.405) (width 0.2032) (layer Front) (net 0))
  (segment (start 38.989 56.896) (end 36.83 59.055) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.64 56.896) (end 38.989 56.896) (width 0.2032) (layer Front) (net 0))
  (segment (start 45.055 68.55) (end 45.72 69.215) (width 0.2032) (layer Front) (net 0))
  (segment (start 45.055 66.04) (end 45.055 68.55) (width 0.2032) (layer Front) (net 0))
  (segment (start 45.055 64.379999) (end 46.569999 62.865) (width 0.2032) (layer Front) (net 0))
  (segment (start 45.055 66.04) (end 45.055 64.379999) (width 0.2032) (layer Front) (net 0))
  (segment (start 46.569999 62.865) (end 46.569999 57.364999) (width 0.2032) (layer Front) (net 0))

)
