(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1~bpo9+1)

  (general
    (thickness 1.6002)
    (drawings 28)
    (tracks 244)
    (zones 0)
    (modules 227)
    (nets 1)
  )

  (page User 150.012 200)
  (title_block
    (title High-density-proto-board)
    (date "12 Jun 2014")
    (rev 0.10.a)
    (company "2014 - blog.spitzenpfeil.org")
  )

  (layers
    (0 Front signal)
    (31 Back signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )

  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2032)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.635)
    (via_drill 0.3302)
    (via_min_size 0.635)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.2)
    (mod_text_size 1 1)
    (mod_text_width 0.2)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.635)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E79E196)
    (at 85.09 93.98)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E79E189)
    (at 85.09 91.44)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E79E17C)
    (at 85.09 88.9)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E79E153)
    (at 85.09 76.2)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E79E139)
    (at 85.09 78.74)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E79E0FB)
    (at 85.09 81.28)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer Front) (tedit 5E6DC4FF) (tstamp 5E79B29C)
    (at 83.82 59.69)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer Front) (tedit 5E6DC4FF) (tstamp 5E79B28D)
    (at 34 94)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_4.3mm_M4 (layer Front) (tedit 5E6DC4FF) (tstamp 5E70BCB4)
    (at 77.47 85.09)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 4.55 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 4.3 0) (layer Cmts.User) (width 0.15))
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Back) (tedit 5E6DA448) (tstamp 5E70B54C)
    (at 33.02 71.755)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 -2.33) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.8 1.8) (end -1.8 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end 1.8 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 -90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Back) (tedit 5E6DA448) (tstamp 5E70B532)
    (at 34.29 79.375)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 -2.33) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 -90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end 1.8 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end -1.8 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Back) (tedit 5E6DA448) (tstamp 5E70B518)
    (at 31.75 79.375)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 -2.33) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.8 1.8) (end -1.8 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end 1.8 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 -90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FCA82)
    (at 82.55 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FCA68)
    (at 69.85 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FCA34)
    (at 82.55 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FCA27)
    (at 72.39 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC9F2)
    (at 69.85 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC9D8)
    (at 74.93 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC9BD)
    (at 77.47 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC9A3)
    (at 77.47 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC996)
    (at 80.01 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC97B)
    (at 72.39 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC96E)
    (at 74.93 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC961)
    (at 80.01 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC6C7)
    (at 81.28 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC6A0)
    (at 76.2 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC685)
    (at 71.12 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC644)
    (at 78.74 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC61C)
    (at 73.66 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC373)
    (at 73.66 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC366)
    (at 78.74 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC34C)
    (at 81.28 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC332)
    (at 76.2 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FC30B)
    (at 71.12 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBD94)
    (at 70.485 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBD52)
    (at 70.485 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBD27)
    (at 67.945 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBD19)
    (at 65.405 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBCFF)
    (at 67.945 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBCF2)
    (at 67.945 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBCE5)
    (at 65.405 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBCA5)
    (at 62.865 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBC51)
    (at 62.865 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBC44)
    (at 62.865 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBC2A)
    (at 65.405 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBC1C)
    (at 67.945 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBBDA)
    (at 65.405 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBBCD)
    (at 62.865 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBBC0)
    (at 62.865 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBBA4)
    (at 67.945 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBB97)
    (at 67.945 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBB8A)
    (at 70.485 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBB7D)
    (at 70.485 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBB63)
    (at 70.485 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 5E6FBB4B)
    (at 66.675 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FBB40)
    (at 66.675 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBB18)
    (at 70.485 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBAFE)
    (at 70.485 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBAD7)
    (at 62.865 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FBACC)
    (at 66.675 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBAA4)
    (at 62.865 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FBA4F)
    (at 66.675 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FBA0F)
    (at 62.865 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB9AF)
    (at 65.405 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB9A2)
    (at 65.405 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB96A)
    (at 67.945 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB950)
    (at 65.405 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB941)
    (at 62.865 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB933)
    (at 65.405 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB926)
    (at 67.945 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB90B)
    (at 67.945 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 5E6FB8C9)
    (at 66.675 88.9)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FB8BE)
    (at 66.675 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 53998995) (tstamp 5E6FB8B3)
    (at 66.675 86.36)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FB89F)
    (at 66.675 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB88B)
    (at 70.485 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FB863)
    (at 66.675 91.44)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB847)
    (at 65.405 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FB83A)
    (at 70.485 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA7DB)
    (at 50.165 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA7CE)
    (at 52.705 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA7C1)
    (at 52.705 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA7B4)
    (at 57.785 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA7A7)
    (at 45.085 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA799)
    (at 57.785 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA78C)
    (at 45.085 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA772)
    (at 42.545 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA765)
    (at 47.625 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA758)
    (at 47.625 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA74B)
    (at 50.165 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA73E)
    (at 50.165 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA731)
    (at 57.785 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA724)
    (at 55.245 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA717)
    (at 55.245 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA709)
    (at 50.165 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA6FC)
    (at 42.545 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA6EF)
    (at 42.545 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA6CC)
    (at 55.245 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA6BF)
    (at 60.325 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA6B2)
    (at 60.325 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA6A5)
    (at 60.325 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA696)
    (at 52.705 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FA687)
    (at 56.515 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA67A)
    (at 55.245 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA66D)
    (at 57.785 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 5E6FA655)
    (at 56.515 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FA649)
    (at 56.515 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA63C)
    (at 45.085 80.01)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA62F)
    (at 45.085 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FA624)
    (at 56.515 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA613)
    (at 47.625 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA605)
    (at 42.545 82.55)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA5F8)
    (at 47.625 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA5DD)
    (at 52.705 74.93)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6FA5D0)
    (at 60.325 77.47)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 5E6FA5AA)
    (at 46.355 73.66)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FA59F)
    (at 46.355 81.28)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FA580)
    (at 46.355 78.74)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6FA55E)
    (at 46.355 76.2)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E63)
    (at 60.325 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E56)
    (at 55.245 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E49)
    (at 55.245 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E3C)
    (at 52.705 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E2F)
    (at 52.705 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E22)
    (at 57.785 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E15)
    (at 57.785 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9E08)
    (at 60.325 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DFB)
    (at 60.325 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DEE)
    (at 60.325 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DE1)
    (at 52.705 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DD4)
    (at 52.705 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DC7)
    (at 55.245 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DBA)
    (at 55.245 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DAD)
    (at 57.785 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9DA0)
    (at 52.705 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9D93)
    (at 57.785 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9D86)
    (at 57.785 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 5E6F9D7B)
    (at 56.515 88.9)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6F9D70)
    (at 56.515 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 53998995) (tstamp 5E6F9D65)
    (at 56.515 86.36)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6F9D52)
    (at 56.515 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5E6F9D3F)
    (at 56.515 91.44)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9D23)
    (at 55.245 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9D16)
    (at 60.325 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9CB7)
    (at 50.165 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9CAA)
    (at 50.165 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C9D)
    (at 50.165 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C90)
    (at 50.165 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C83)
    (at 50.165 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C35)
    (at 47.625 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C28)
    (at 47.625 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C1B)
    (at 47.625 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C0E)
    (at 47.625 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9C01)
    (at 47.625 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9BB3)
    (at 45.085 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9BA6)
    (at 45.085 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9B99)
    (at 45.085 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9B8C)
    (at 45.085 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9B7F)
    (at 45.085 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9B02)
    (at 42.545 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9AD9)
    (at 42.545 95.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9ABF)
    (at 42.545 92.71)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9AA5)
    (at 42.545 90.17)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6F9A63)
    (at 42.545 87.63)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E99C8)
    (at 59.69 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E99BB)
    (at 54.61 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E99AE)
    (at 44.45 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E99A1)
    (at 67.31 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9994)
    (at 67.31 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9987)
    (at 49.53 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E997A)
    (at 39.37 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E996D)
    (at 59.69 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9953)
    (at 54.61 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9946)
    (at 52.07 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9939)
    (at 36.83 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E992C)
    (at 62.23 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E991F)
    (at 41.91 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9912)
    (at 57.15 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9905)
    (at 64.77 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98F8)
    (at 36.83 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98EB)
    (at 49.53 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98DE)
    (at 41.91 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98D1)
    (at 57.15 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98C4)
    (at 44.45 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98B7)
    (at 62.23 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E98AA)
    (at 39.37 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E989D)
    (at 64.77 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9890)
    (at 46.99 67.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9876)
    (at 52.07 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9869)
    (at 46.99 69.85)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9746)
    (at 66.04 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E972C)
    (at 60.96 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E971F)
    (at 55.88 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9705)
    (at 58.42 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E96F8)
    (at 63.5 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E96EB)
    (at 58.42 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E96D1)
    (at 63.5 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E96C4)
    (at 66.04 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E96B7)
    (at 60.96 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E96AA)
    (at 68.58 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E969D)
    (at 55.88 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E946C)
    (at 50.8 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E945F)
    (at 45.72 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9452)
    (at 48.26 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9445)
    (at 53.34 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9438)
    (at 48.26 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E942B)
    (at 53.34 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E941E)
    (at 50.8 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9411)
    (at 45.72 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E939B)
    (at 38.1 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E938E)
    (at 43.18 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E9381)
    (at 40.64 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E934C)
    (at 43.18 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E933F)
    (at 40.64 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprints:PinHeader_1x01_EDIT (layer Front) (tedit 5E6DA448) (tstamp 5E6E92EF)
    (at 38.1 100.33)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PinHeader_1x01_P2.54mm_Vertical (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module my_parts:MADW__SIL-1 (layer Front) (tedit 5398BCDC) (tstamp 5398C661)
    (at 22.86 66.04)
    (tags "CONN DEV")
    (fp_text reference P? (at 0 -2.032) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AF99)
    (at 46.355 96.52)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AF8E)
    (at 46.355 93.98)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539892D9) (tstamp 5398AF83)
    (at 46.355 91.44)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 539BBDAD) (tstamp 539BBDEF)
    (at 46.355 88.9)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module my_parts:MADW__SIL-8-1.27mm (layer Front) (tedit 53998995) (tstamp 5398AF15)
    (at 46.355 86.36)
    (fp_text reference P? (at 0 -2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (fp_text value VAL** (at 0 2.286) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.2)))
    )
    (pad 1 thru_hole oval (at -4.445 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -3.175 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -1.905 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -0.635 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0.635 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.905 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 3.175 0) (size 1.2 1.4) (drill 0.6 (offset 0.1 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 4.445 0) (size 1.2 1.4) (drill 0.6 (offset -0.1 0)) (layers *.Cu *.Mask))
  )

  (module oshw-logo:OSHW-logo_silkscreen_5mm (layer Front) (tedit 0) (tstamp 5398B43E)
    (at 38.1 97 180)
    (fp_text reference G*** (at 0 2.65176 180) (layer F.SilkS) hide
      (effects (font (size 0.22606 0.22606) (thickness 0.04318)))
    )
    (fp_text value OSHW-logo_silkscreen_5mm (at 0 -2.65176 180) (layer F.SilkS) hide
      (effects (font (size 0.22606 0.22606) (thickness 0.04318)))
    )
    (fp_poly (pts (xy -1.51384 -2.24536) (xy -1.48844 -2.23012) (xy -1.43002 -2.19456) (xy -1.3462 -2.13868)
      (xy -1.24714 -2.07264) (xy -1.14808 -2.0066) (xy -1.0668 -1.95326) (xy -1.01092 -1.91516)
      (xy -0.98552 -1.90246) (xy -0.97282 -1.90754) (xy -0.9271 -1.9304) (xy -0.85852 -1.96596)
      (xy -0.81788 -1.98628) (xy -0.75692 -2.01168) (xy -0.7239 -2.0193) (xy -0.71882 -2.00914)
      (xy -0.69596 -1.96088) (xy -0.6604 -1.8796) (xy -0.61468 -1.77038) (xy -0.5588 -1.64338)
      (xy -0.50292 -1.50876) (xy -0.4445 -1.36906) (xy -0.38862 -1.23444) (xy -0.34036 -1.11506)
      (xy -0.29972 -1.01854) (xy -0.27432 -0.94996) (xy -0.26416 -0.92202) (xy -0.2667 -0.9144)
      (xy -0.29972 -0.88392) (xy -0.35306 -0.84328) (xy -0.47244 -0.74676) (xy -0.58928 -0.60198)
      (xy -0.6604 -0.43688) (xy -0.68326 -0.25146) (xy -0.66294 -0.08128) (xy -0.5969 0.08128)
      (xy -0.4826 0.2286) (xy -0.3429 0.33782) (xy -0.18034 0.4064) (xy 0 0.42926)
      (xy 0.17272 0.40894) (xy 0.34036 0.3429) (xy 0.48768 0.23114) (xy 0.55118 0.16002)
      (xy 0.63754 0.01016) (xy 0.6858 -0.14732) (xy 0.69088 -0.18796) (xy 0.68326 -0.36322)
      (xy 0.63246 -0.5334) (xy 0.53848 -0.68326) (xy 0.40894 -0.80772) (xy 0.3937 -0.81788)
      (xy 0.33528 -0.8636) (xy 0.29464 -0.89408) (xy 0.26416 -0.91948) (xy 0.48768 -1.45796)
      (xy 0.52324 -1.54178) (xy 0.5842 -1.6891) (xy 0.63754 -1.8161) (xy 0.68072 -1.9177)
      (xy 0.7112 -1.98374) (xy 0.7239 -2.01168) (xy 0.7239 -2.01422) (xy 0.74422 -2.01676)
      (xy 0.78486 -2.00152) (xy 0.86106 -1.96596) (xy 0.90932 -1.94056) (xy 0.96774 -1.91262)
      (xy 0.99314 -1.90246) (xy 1.016 -1.91516) (xy 1.06934 -1.95072) (xy 1.15062 -2.00406)
      (xy 1.24714 -2.06756) (xy 1.33858 -2.13106) (xy 1.4224 -2.18694) (xy 1.48336 -2.22504)
      (xy 1.51384 -2.24282) (xy 1.51892 -2.24282) (xy 1.54432 -2.22758) (xy 1.59258 -2.18694)
      (xy 1.66624 -2.11836) (xy 1.77038 -2.01422) (xy 1.78562 -1.99898) (xy 1.87198 -1.91262)
      (xy 1.94056 -1.83896) (xy 1.98628 -1.78816) (xy 2.00406 -1.7653) (xy 1.98882 -1.73482)
      (xy 1.95072 -1.67386) (xy 1.89484 -1.5875) (xy 1.82626 -1.48844) (xy 1.64846 -1.22936)
      (xy 1.74498 -0.98552) (xy 1.77546 -0.90932) (xy 1.81356 -0.82042) (xy 1.8415 -0.75438)
      (xy 1.85674 -0.72644) (xy 1.88214 -0.71628) (xy 1.95072 -0.70104) (xy 2.04724 -0.68072)
      (xy 2.16154 -0.6604) (xy 2.2733 -0.64008) (xy 2.37236 -0.61976) (xy 2.44348 -0.60706)
      (xy 2.4765 -0.59944) (xy 2.48412 -0.59436) (xy 2.49174 -0.57912) (xy 2.49428 -0.5461)
      (xy 2.49682 -0.48514) (xy 2.49936 -0.39116) (xy 2.49936 -0.25146) (xy 2.49936 -0.23622)
      (xy 2.49682 -0.10668) (xy 2.49428 0) (xy 2.49174 0.06604) (xy 2.48666 0.09398)
      (xy 2.45618 0.1016) (xy 2.38506 0.11684) (xy 2.286 0.13462) (xy 2.16662 0.15748)
      (xy 2.159 0.16002) (xy 2.04216 0.18288) (xy 1.9431 0.2032) (xy 1.87198 0.21844)
      (xy 1.84404 0.2286) (xy 1.83642 0.23622) (xy 1.81356 0.28194) (xy 1.78054 0.3556)
      (xy 1.7399 0.4445) (xy 1.7018 0.53848) (xy 1.66878 0.6223) (xy 1.64592 0.68326)
      (xy 1.6383 0.7112) (xy 1.64084 0.71374) (xy 1.65862 0.74168) (xy 1.69926 0.80264)
      (xy 1.75514 0.88646) (xy 1.82372 0.98806) (xy 1.8288 0.99568) (xy 1.89738 1.09474)
      (xy 1.95326 1.1811) (xy 1.98882 1.23952) (xy 2.00406 1.26746) (xy 2.00406 1.27)
      (xy 1.9812 1.30048) (xy 1.9304 1.35636) (xy 1.85674 1.43256) (xy 1.77038 1.52146)
      (xy 1.74244 1.54686) (xy 1.64338 1.64338) (xy 1.57734 1.70434) (xy 1.53416 1.73736)
      (xy 1.51384 1.74498) (xy 1.48336 1.7272) (xy 1.41986 1.68656) (xy 1.33604 1.62814)
      (xy 1.23444 1.55956) (xy 1.22682 1.55448) (xy 1.12776 1.4859) (xy 1.04394 1.43002)
      (xy 0.98552 1.38938) (xy 0.95758 1.37414) (xy 0.95504 1.37414) (xy 0.9144 1.38684)
      (xy 0.84328 1.41224) (xy 0.75438 1.44526) (xy 0.66294 1.48336) (xy 0.57912 1.51892)
      (xy 0.51562 1.54686) (xy 0.48514 1.56464) (xy 0.47498 1.6002) (xy 0.4572 1.6764)
      (xy 0.43688 1.778) (xy 0.41148 1.89992) (xy 0.40894 1.92024) (xy 0.38608 2.03962)
      (xy 0.3683 2.13868) (xy 0.35306 2.20726) (xy 0.34544 2.2352) (xy 0.3302 2.23774)
      (xy 0.27178 2.24282) (xy 0.18288 2.24536) (xy 0.07366 2.24536) (xy -0.0381 2.24536)
      (xy -0.14732 2.24282) (xy -0.2413 2.24028) (xy -0.30988 2.2352) (xy -0.33782 2.23012)
      (xy -0.33782 2.22758) (xy -0.34798 2.18948) (xy -0.36576 2.11582) (xy -0.38608 2.01168)
      (xy -0.40894 1.88976) (xy -0.41402 1.8669) (xy -0.43688 1.75006) (xy -0.4572 1.651)
      (xy -0.4699 1.58496) (xy -0.47752 1.55702) (xy -0.49022 1.55194) (xy -0.53848 1.53162)
      (xy -0.61722 1.4986) (xy -0.71628 1.45796) (xy -0.94488 1.36652) (xy -1.22682 1.55702)
      (xy -1.25222 1.5748) (xy -1.35382 1.64338) (xy -1.4351 1.69926) (xy -1.49352 1.73736)
      (xy -1.51638 1.75006) (xy -1.51892 1.75006) (xy -1.54686 1.72466) (xy -1.60274 1.67132)
      (xy -1.67894 1.59766) (xy -1.76784 1.5113) (xy -1.83134 1.44526) (xy -1.91008 1.36652)
      (xy -1.95834 1.31318) (xy -1.98628 1.28016) (xy -1.9939 1.25984) (xy -1.99136 1.2446)
      (xy -1.97358 1.21666) (xy -1.93294 1.1557) (xy -1.87452 1.06934) (xy -1.80594 0.97028)
      (xy -1.75006 0.88646) (xy -1.6891 0.79248) (xy -1.651 0.72644) (xy -1.63576 0.69342)
      (xy -1.64084 0.68072) (xy -1.65862 0.62484) (xy -1.69418 0.54102) (xy -1.73482 0.44196)
      (xy -1.83388 0.22098) (xy -1.97866 0.19304) (xy -2.06756 0.17526) (xy -2.18948 0.1524)
      (xy -2.30886 0.12954) (xy -2.49174 0.09398) (xy -2.49936 -0.58166) (xy -2.47142 -0.59436)
      (xy -2.44348 -0.60198) (xy -2.3749 -0.61722) (xy -2.27838 -0.63754) (xy -2.16154 -0.65786)
      (xy -2.06502 -0.67564) (xy -1.96596 -0.69596) (xy -1.89484 -0.70866) (xy -1.86436 -0.71628)
      (xy -1.8542 -0.72644) (xy -1.83134 -0.7747) (xy -1.79578 -0.8509) (xy -1.75514 -0.94234)
      (xy -1.71704 -1.03632) (xy -1.68148 -1.12522) (xy -1.65862 -1.19126) (xy -1.64846 -1.22428)
      (xy -1.66116 -1.25222) (xy -1.69926 -1.31064) (xy -1.7526 -1.39192) (xy -1.82118 -1.49098)
      (xy -1.88722 -1.5875) (xy -1.94564 -1.67132) (xy -1.98374 -1.73228) (xy -2.00152 -1.76022)
      (xy -1.99136 -1.778) (xy -1.95326 -1.82626) (xy -1.8796 -1.90246) (xy -1.76784 -2.01168)
      (xy -1.75006 -2.02946) (xy -1.6637 -2.11328) (xy -1.59004 -2.18186) (xy -1.5367 -2.22758)
      (xy -1.51384 -2.24536)) (layer F.SilkS) (width 0.00254))
  )

  (module Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical (layer Back) (tedit 5E6DC3F9) (tstamp 5E70B4BD)
    (at 33.02 75.565 270)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference REF882 (at 0.475 3.2 270) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value U.FL_Hirose_U.FL-R-SMT-1_Vertical (at 0.475 -3.2 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.32 1) (end -2.02 1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.32 -1.8) (end -1.32 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.32 1.8) (end -1.12 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.12 1.8) (end -1.12 2.5) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.08 2.5) (end -1.12 2.5) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.32 1) (end -1.32 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.08 1.8) (end 2.08 2.5) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.08 1.8) (end 2.28 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.885 1.4) (end -0.885 0.76) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.425 -1.5) (end -0.425 -1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.425 -1.3) (end -0.825 -1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.825 -0.3) (end -0.825 -1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -1.075 -0.3) (end -0.825 -0.3) (layer B.Fab) (width 0.1))
    (fp_line (start -1.075 -0.3) (end -1.075 0.15) (layer B.Fab) (width 0.1))
    (fp_line (start -0.925 0.3) (end -0.825 0.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.825 0.3) (end -0.825 1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.425 1.5) (end -0.425 1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.425 1.3) (end -0.825 1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.425 -1.5) (end 1.375 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start 1.375 -1.5) (end 1.375 -1.3) (layer B.Fab) (width 0.1))
    (fp_line (start 1.775 -1.3) (end 1.375 -1.3) (layer B.Fab) (width 0.1))
    (fp_line (start 1.775 1.3) (end 1.775 -1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.425 1.5) (end 1.375 1.5) (layer B.Fab) (width 0.1))
    (fp_line (start 1.375 1.5) (end 1.375 1.3) (layer B.Fab) (width 0.1))
    (fp_line (start 1.775 1.3) (end 1.375 1.3) (layer B.Fab) (width 0.1))
    (fp_line (start -0.925 0.3) (end -1.075 0.15) (layer B.Fab) (width 0.1))
    (fp_line (start -0.885 -1.4) (end -0.885 -0.76) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.885 0.76) (end -1.515 0.76) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.835 1.35) (end 1.835 -1.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.08 -2.5) (end -1.12 -2.5) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.12 -2.5) (end -1.12 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.32 -1.8) (end -1.12 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.28 -1.8) (end 2.28 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.08 -2.5) (end 2.08 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.08 -1.8) (end 2.28 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.32 -1) (end -2.02 -1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.02 -1) (end -2.02 1) (layer B.CrtYd) (width 0.05))
    (fp_text user %R (at 0.475 0 180) (layer B.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)) (justify mirror))
    )
    (pad 2 smd rect (at 0.475 1.475 270) (size 2.2 1.05) (layers Back B.Paste B.Mask))
    (pad 1 smd rect (at -1.05 0 270) (size 1.05 1) (layers Back B.Paste B.Mask))
    (pad 2 smd rect (at 0.475 -1.475 270) (size 2.2 1.05) (layers Back B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (offset (xyz 0.4749999928262157 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LED_THT:LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRBlack (layer Front) (tedit 5E79A367) (tstamp 5E79CAE1)
    (at 38.1 73.66 270)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins")
    (fp_text reference REF100552 (at 1.27 -1.96 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRBlack (at 1.27 7.63 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 5.07) (end -0.29 5.07) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 5.07) (end -0.23 5.07) (angle -180) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 -1.25) (end -1.25 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 6.9) (end 3.75 -1.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 6.9) (end 3.75 6.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.25) (end -1.25 6.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.54 1.08) (end 2.54 1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.21) (end 2.54 1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.21) (end 2.54 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 1.08) (end 2.54 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.08) (end 0 1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.21) (end 0 1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.21) (end 0 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 1.08) (end 0 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.83 1.21) (end 3.23 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.83 2.33) (end 2.83 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.23 2.33) (end 2.83 2.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.23 1.21) (end 3.23 2.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 1.21) (end 2.83 1.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.83 1.21) (end 2.83 5.07) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 1.21) (end -0.29 5.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 1.27) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 1.27) (end 2.54 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 0) (end 2.54 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 1.27) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 1.27) (end 0 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 0 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.77 1.27) (end 3.17 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.77 2.27) (end 2.77 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.17 2.27) (end 2.77 2.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.17 1.27) (end 3.17 2.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.23 1.27) (end 2.77 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.77 1.27) (end 2.77 5.07) (layer F.Fab) (width 0.1))
    (fp_line (start -0.23 1.27) (end -0.23 5.07) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRBlack.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer Front) (tedit 5A02FF57) (tstamp 5E79E0F9)
    (at 85.09 85.09 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference REF** (at 0 -2.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOT-23-6_Handsoldering (at 0 2.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -2.4 -1.8) (end 2.4 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 -1.8) (end 2.4 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.4 1.8) (end -2.4 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.4 1.8) (end -2.4 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.61) (end -2.05 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers Front F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module footprintslocal:sensor_propercolours (layer Front) (tedit 0) (tstamp 5E79E55D)
    (at 37 85 180)
    (fp_text reference G*** (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 1.524 1.524) (thickness 0.3)))
    )
    (fp_text value LOGO (at 0.75 0 180) (layer F.SilkS) hide
      (effects (font (size 1.524 1.524) (thickness 0.3)))
    )
    (fp_poly (pts (xy 0.764272 -0.712497) (xy 0.830281 -0.684174) (xy 0.834216 -0.624479) (xy 0.777263 -0.523195)
      (xy 0.673732 -0.38653) (xy 0.500797 -0.169334) (xy 0.673732 -0.169334) (xy 0.792826 -0.159281)
      (xy 0.842902 -0.125789) (xy 0.846667 -0.105834) (xy 0.825763 -0.06754) (xy 0.752415 -0.047824)
      (xy 0.613833 -0.042334) (xy 0.476273 -0.047195) (xy 0.404875 -0.065397) (xy 0.381507 -0.102371)
      (xy 0.381 -0.112057) (xy 0.4065 -0.182164) (xy 0.47199 -0.287392) (xy 0.529167 -0.362598)
      (xy 0.610833 -0.466367) (xy 0.664647 -0.542617) (xy 0.677333 -0.568042) (xy 0.640485 -0.585344)
      (xy 0.551726 -0.592666) (xy 0.550333 -0.592667) (xy 0.449507 -0.611599) (xy 0.423333 -0.656167)
      (xy 0.445993 -0.6961) (xy 0.524447 -0.715604) (xy 0.635 -0.719667) (xy 0.764272 -0.712497)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 0.227826 -0.700735) (xy 0.254 -0.656167) (xy 0.218707 -0.604453) (xy 0.169333 -0.592667)
      (xy 0.096126 -0.576976) (xy 0.098575 -0.538085) (xy 0.175457 -0.488271) (xy 0.179917 -0.486289)
      (xy 0.25595 -0.415994) (xy 0.28825 -0.309868) (xy 0.280022 -0.19479) (xy 0.234467 -0.097641)
      (xy 0.154792 -0.045299) (xy 0.127 -0.042334) (xy 0.042562 -0.076398) (xy 0.001489 -0.124217)
      (xy -0.037319 -0.211128) (xy -0.024971 -0.247807) (xy 0.021167 -0.254) (xy 0.077502 -0.231142)
      (xy 0.084667 -0.211667) (xy 0.117266 -0.171033) (xy 0.129944 -0.169334) (xy 0.159939 -0.204393)
      (xy 0.161557 -0.264584) (xy 0.1291 -0.336916) (xy 0.047397 -0.348796) (xy -0.019976 -0.349848)
      (xy -0.03851 -0.389663) (xy -0.026549 -0.470504) (xy -0.007641 -0.582495) (xy 0 -0.661459)
      (xy 0.038109 -0.706147) (xy 0.127 -0.719667) (xy 0.227826 -0.700735)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -0.354586 -0.678658) (xy -0.309023 -0.610093) (xy -0.257973 -0.479249) (xy -0.226431 -0.381)
      (xy -0.180366 -0.230553) (xy -0.145743 -0.115684) (xy -0.128631 -0.056581) (xy -0.127802 -0.052917)
      (xy -0.153106 -0.035477) (xy -0.209835 -0.052732) (xy -0.260235 -0.090565) (xy -0.269309 -0.105834)
      (xy -0.32563 -0.153937) (xy -0.402167 -0.169334) (xy -0.492855 -0.147173) (xy -0.535025 -0.105834)
      (xy -0.57448 -0.064177) (xy -0.633291 -0.038226) (xy -0.673704 -0.042099) (xy -0.676531 -0.052917)
      (xy -0.664606 -0.095373) (xy -0.63369 -0.198514) (xy -0.589854 -0.342152) (xy -0.589027 -0.344843)
      (xy -0.463795 -0.344843) (xy -0.436087 -0.301098) (xy -0.402167 -0.296334) (xy -0.346309 -0.3247)
      (xy -0.339315 -0.34925) (xy -0.36132 -0.43146) (xy -0.375757 -0.458633) (xy -0.410392 -0.489444)
      (xy -0.438609 -0.444588) (xy -0.463795 -0.344843) (xy -0.589027 -0.344843) (xy -0.577903 -0.381)
      (xy -0.520966 -0.549989) (xy -0.473457 -0.649577) (xy -0.427871 -0.693322) (xy -0.402167 -0.6985)
      (xy -0.354586 -0.678658)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 0.526735 0.972771) (xy 0.541258 1.093919) (xy 0.549056 1.290024) (xy 0.550333 1.439333)
      (xy 0.549502 1.653774) (xy 0.545451 1.797583) (xy 0.535842 1.884792) (xy 0.518335 1.92943)
      (xy 0.490592 1.945528) (xy 0.465667 1.947333) (xy 0.424544 1.940653) (xy 0.399405 1.90959)
      (xy 0.386369 1.83761) (xy 0.381556 1.708178) (xy 0.381 1.586524) (xy 0.381 1.225714)
      (xy 0.275167 1.295059) (xy 0.200953 1.339244) (xy 0.17324 1.333427) (xy 0.169333 1.289728)
      (xy 0.198472 1.21984) (xy 0.270419 1.124401) (xy 0.361974 1.02812) (xy 0.449933 0.955701)
      (xy 0.505902 0.931333) (xy 0.526735 0.972771)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -0.108265 0.972771) (xy -0.093742 1.093919) (xy -0.085944 1.290024) (xy -0.084667 1.439333)
      (xy -0.085498 1.653774) (xy -0.089549 1.797583) (xy -0.099158 1.884792) (xy -0.116665 1.92943)
      (xy -0.144408 1.945528) (xy -0.169333 1.947333) (xy -0.210456 1.940653) (xy -0.235595 1.90959)
      (xy -0.248631 1.83761) (xy -0.253444 1.708178) (xy -0.254 1.586524) (xy -0.254 1.225714)
      (xy -0.359833 1.295059) (xy -0.434047 1.339244) (xy -0.46176 1.333427) (xy -0.465667 1.289728)
      (xy -0.436528 1.21984) (xy -0.364581 1.124401) (xy -0.273026 1.02812) (xy -0.185067 0.955701)
      (xy -0.129098 0.931333) (xy -0.108265 0.972771)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -1.645296 -2.68572) (xy -1.608667 -2.667) (xy -1.575418 -2.635254) (xy -1.606197 -2.631246)
      (xy -1.685034 -2.654976) (xy -1.7145 -2.667) (xy -1.762212 -2.695873) (xy -1.735667 -2.70571)
      (xy -1.645296 -2.68572)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 2.494324 -0.943841) (xy 2.467827 -0.851952) (xy 2.398704 -0.751924) (xy 2.389204 -0.742053)
      (xy 2.311902 -0.621737) (xy 2.319178 -0.500595) (xy 2.410962 -0.379492) (xy 2.41979 -0.371695)
      (xy 2.483925 -0.270147) (xy 2.485377 -0.202362) (xy 2.469889 -0.152992) (xy 2.461098 -0.172538)
      (xy 2.427994 -0.245766) (xy 2.355456 -0.332976) (xy 2.3495 -0.338667) (xy 2.261715 -0.471688)
      (xy 2.244486 -0.622404) (xy 2.298165 -0.764808) (xy 2.343061 -0.816939) (xy 2.421082 -0.902319)
      (xy 2.466719 -0.973667) (xy 2.486128 -0.998357) (xy 2.494324 -0.943841)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -1.704799 0.69409) (xy -1.717424 0.713331) (xy -1.760361 0.716324) (xy -1.805532 0.705985)
      (xy -1.785938 0.690748) (xy -1.719776 0.685701) (xy -1.704799 0.69409)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 2.494324 0.321522) (xy 2.466951 0.416113) (xy 2.413 0.486833) (xy 2.34869 0.587005)
      (xy 2.328333 0.683535) (xy 2.360828 0.803257) (xy 2.413 0.856491) (xy 2.478958 0.909733)
      (xy 2.497667 0.941516) (xy 2.473615 0.973239) (xy 2.409881 0.943524) (xy 2.335712 0.875688)
      (xy 2.257054 0.738379) (xy 2.257434 0.591328) (xy 2.336427 0.454007) (xy 2.34517 0.444981)
      (xy 2.421792 0.359031) (xy 2.467908 0.290342) (xy 2.468828 0.288155) (xy 2.487014 0.276948)
      (xy 2.494324 0.321522)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -1.704799 1.921756) (xy -1.717424 1.940997) (xy -1.760361 1.943991) (xy -1.805532 1.933652)
      (xy -1.785938 1.918414) (xy -1.719776 1.913368) (xy -1.704799 1.921756)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 2.492346 1.627746) (xy 2.483549 1.668168) (xy 2.416307 1.704708) (xy 2.413 1.705599)
      (xy 2.350789 1.759963) (xy 2.323532 1.861348) (xy 2.330982 1.97977) (xy 2.372894 2.085246)
      (xy 2.416489 2.131278) (xy 2.484267 2.219117) (xy 2.485754 2.292429) (xy 2.470742 2.34931)
      (xy 2.461955 2.323547) (xy 2.461098 2.313259) (xy 2.425471 2.232636) (xy 2.3495 2.151436)
      (xy 2.261697 2.038867) (xy 2.243667 1.932513) (xy 2.26619 1.800268) (xy 2.323164 1.686458)
      (xy 2.398689 1.617771) (xy 2.436567 1.608666) (xy 2.492346 1.627746)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 2.497667 3.661833) (xy 2.4765 3.683) (xy 2.455333 3.661833) (xy 2.4765 3.640666)
      (xy 2.497667 3.661833)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 1.715082 1.851586) (xy 1.719049 1.964085) (xy 1.722617 2.16121) (xy 1.725786 2.442978)
      (xy 1.726881 2.57175) (xy 1.72807 2.868497) (xy 1.72692 3.135375) (xy 1.72366 3.361321)
      (xy 1.718519 3.535275) (xy 1.711723 3.646176) (xy 1.703917 3.683054) (xy 1.694166 3.643025)
      (xy 1.686884 3.531993) (xy 1.682458 3.363595) (xy 1.68128 3.151471) (xy 1.683035 2.952804)
      (xy 1.689349 2.557897) (xy 1.695276 2.247516) (xy 1.700815 2.021678) (xy 1.705963 1.880399)
      (xy 1.71072 1.823696) (xy 1.715082 1.851586)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 0.646389 3.655232) (xy 0.647796 3.669129) (xy 0.581525 3.674805) (xy 0.5715 3.674747)
      (xy 0.505843 3.668642) (xy 0.51211 3.655758) (xy 0.519389 3.653663) (xy 0.611604 3.647465)
      (xy 0.646389 3.655232)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -0.284944 3.655232) (xy -0.283537 3.669129) (xy -0.349808 3.674805) (xy -0.359833 3.674747)
      (xy -0.425491 3.668642) (xy -0.419223 3.655758) (xy -0.411944 3.653663) (xy -0.319729 3.647465)
      (xy -0.284944 3.655232)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy -1.502625 1.808256) (xy -1.498642 1.916246) (xy -1.49505 2.108748) (xy -1.491856 2.385825)
      (xy -1.490453 2.550583) (xy -1.489263 2.850268) (xy -1.490371 3.120186) (xy -1.493554 3.34938)
      (xy -1.49859 3.526893) (xy -1.505257 3.641768) (xy -1.513333 3.683048) (xy -1.513417 3.683052)
      (xy -1.523046 3.642989) (xy -1.530286 3.531729) (xy -1.53476 3.362715) (xy -1.536097 3.149395)
      (xy -1.534322 2.931635) (xy -1.528145 2.533842) (xy -1.522317 2.220192) (xy -1.516844 1.990747)
      (xy -1.511733 1.845568) (xy -1.506991 1.784717) (xy -1.502625 1.808256)) (layer F.SilkS) (width 0.01))
    (fp_poly (pts (xy 1.60375 -3.642478) (xy 1.868768 -3.642323) (xy 2.062221 -3.642082) (xy 2.148417 -3.641871)
      (xy 2.497667 -3.640667) (xy 2.497667 -3.477895) (xy 2.468613 -3.316459) (xy 2.413 -3.2385)
      (xy 2.347705 -3.137821) (xy 2.328333 -3.048) (xy 2.359254 -2.932196) (xy 2.413 -2.8575)
      (xy 2.477121 -2.757315) (xy 2.492756 -2.671023) (xy 2.484889 -2.607948) (xy 2.470394 -2.628685)
      (xy 2.468204 -2.636712) (xy 2.425464 -2.718364) (xy 2.349251 -2.811542) (xy 2.346114 -2.814704)
      (xy 2.260073 -2.94773) (xy 2.258064 -3.090004) (xy 2.340081 -3.240499) (xy 2.3495 -3.251947)
      (xy 2.419208 -3.356998) (xy 2.454327 -3.4534) (xy 2.455333 -3.466862) (xy 2.449522 -3.510308)
      (xy 2.420938 -3.536755) (xy 2.352856 -3.550387) (xy 2.228551 -3.555391) (xy 2.09915 -3.556)
      (xy 1.742967 -3.556) (xy 1.40065 -3.158077) (xy 1.269989 -3.004256) (xy 1.162324 -2.873824)
      (xy 1.088281 -2.779921) (xy 1.058488 -2.735689) (xy 1.058333 -2.734744) (xy 1.097037 -2.722057)
      (xy 1.198663 -2.712949) (xy 1.341484 -2.709337) (xy 1.3462 -2.709334) (xy 1.510629 -2.701908)
      (xy 1.632603 -2.681933) (xy 1.684866 -2.658534) (xy 1.71261 -2.59067) (xy 1.731061 -2.468666)
      (xy 1.735667 -2.3622) (xy 1.735667 -2.116667) (xy 2.092396 -2.116667) (xy 2.270169 -2.119082)
      (xy 2.380343 -2.128557) (xy 2.439904 -2.148437) (xy 2.465836 -2.182069) (xy 2.468485 -2.190751)
      (xy 2.48433 -2.238926) (xy 2.491421 -2.205007) (xy 2.492756 -2.185022) (xy 2.466807 -2.103471)
      (xy 2.397035 -2.012171) (xy 2.389133 -2.004624) (xy 2.313282 -1.896528) (xy 2.31663 -1.780269)
      (xy 2.399813 -1.647489) (xy 2.417865 -1.627105) (xy 2.476724 -1.533327) (xy 2.494324 -1.457772)
      (xy 2.483497 -1.413661) (xy 2.46963 -1.42875) (xy 2.420257 -1.45854) (xy 2.297791 -1.475926)
      (xy 2.096838 -1.481666) (xy 2.093062 -1.481667) (xy 1.737846 -1.481667) (xy 1.722587 -0.052917)
      (xy 1.716652 0.398094) (xy 1.708694 0.77391) (xy 1.697732 1.083995) (xy 1.68278 1.337814)
      (xy 1.662857 1.54483) (xy 1.636978 1.71451) (xy 1.60416 1.856317) (xy 1.56342 1.979716)
      (xy 1.513774 2.094171) (xy 1.495704 2.130734) (xy 1.331751 2.386672) (xy 1.11997 2.617309)
      (xy 0.885465 2.796404) (xy 0.827199 2.829538) (xy 0.728925 2.877963) (xy 0.638495 2.910141)
      (xy 0.534909 2.929351) (xy 0.397169 2.938872) (xy 0.204272 2.941982) (xy 0.105833 2.942166)
      (xy -0.118311 2.940444) (xy -0.279039 2.933217) (xy -0.397564 2.917395) (xy -0.495102 2.889888)
      (xy -0.592868 2.847605) (xy -0.613833 2.837343) (xy -0.883357 2.661666) (xy -1.112324 2.429143)
      (xy -1.288346 2.15712) (xy -1.399033 1.862944) (xy -1.427562 1.698104) (xy -1.44623 1.55937)
      (xy -1.4682 1.4605) (xy -1.375833 1.4605) (xy -1.367436 1.644272) (xy -1.322447 1.877126)
      (xy -1.217566 2.124949) (xy -1.068121 2.363847) (xy -0.889439 2.569922) (xy -0.696847 2.71928)
      (xy -0.667591 2.735374) (xy -0.381555 2.842719) (xy -0.056004 2.897144) (xy 0.281214 2.897019)
      (xy 0.602252 2.840713) (xy 0.685568 2.814616) (xy 0.900318 2.705888) (xy 1.112686 2.539568)
      (xy 1.295475 2.339013) (xy 1.37205 2.225136) (xy 1.437137 2.093162) (xy 1.498617 1.933264)
      (xy 1.549836 1.7684) (xy 1.584143 1.621531) (xy 1.594887 1.515616) (xy 1.587464 1.481608)
      (xy 1.532344 1.455304) (xy 1.425947 1.440514) (xy 1.383536 1.439333) (xy 1.205735 1.439333)
      (xy 1.100284 1.11125) (xy 0.994833 0.783166) (xy -0.798701 0.760332) (xy -0.90975 1.124405)
      (xy -1.020799 1.488477) (xy -1.198316 1.474488) (xy -1.375833 1.4605) (xy -1.4682 1.4605)
      (xy -1.469668 1.453897) (xy -1.48555 1.416061) (xy -1.492715 1.365897) (xy -1.499626 1.239607)
      (xy -1.50611 1.045731) (xy -1.511998 0.79281) (xy -1.517118 0.489384) (xy -1.5201 0.243021)
      (xy -1.474487 0.243021) (xy -1.473637 0.571657) (xy -1.471054 0.833911) (xy -1.466612 1.035872)
      (xy -1.460181 1.183633) (xy -1.451631 1.283284) (xy -1.440835 1.340916) (xy -1.429178 1.361838)
      (xy -1.352627 1.385063) (xy -1.237723 1.396205) (xy -1.226247 1.396351) (xy -1.076661 1.397)
      (xy -0.97184 1.04775) (xy -0.867018 0.6985) (xy 1.037167 0.6985) (xy 1.147952 1.016)
      (xy 1.258738 1.3335) (xy 1.672167 1.3335) (xy 1.683321 -0.074084) (xy 1.694475 -1.481667)
      (xy 1.429321 -1.488784) (xy 1.164167 -1.4959) (xy 1.418167 -1.520534) (xy 1.672167 -1.545167)
      (xy 1.672167 -2.053167) (xy 1.453916 -2.074334) (xy 1.735667 -2.074334) (xy 1.735667 -1.524)
      (xy 2.361539 -1.524) (xy 2.283986 -1.676117) (xy 2.234164 -1.806555) (xy 2.239016 -1.911573)
      (xy 2.246216 -1.932873) (xy 2.27593 -2.017228) (xy 2.286 -2.055923) (xy 2.247376 -2.0653)
      (xy 2.146321 -2.071931) (xy 2.010833 -2.074334) (xy 1.735667 -2.074334) (xy 1.453916 -2.074334)
      (xy 1.418167 -2.077801) (xy 1.164167 -2.102434) (xy 1.42875 -2.109551) (xy 1.693333 -2.116667)
      (xy 1.693333 -2.303705) (xy 1.688582 -2.462155) (xy 1.662933 -2.557482) (xy 1.599292 -2.605671)
      (xy 1.480562 -2.622711) (xy 1.350137 -2.624667) (xy 1.058333 -2.624667) (xy 1.050937 -2.44475)
      (xy 1.043541 -2.264834) (xy 1.027336 -2.44475) (xy 1.009762 -2.55465) (xy 0.984726 -2.618303)
      (xy 0.974515 -2.624667) (xy 0.931028 -2.594937) (xy 0.852728 -2.519154) (xy 0.757635 -2.417426)
      (xy 0.663764 -2.309861) (xy 0.589135 -2.216569) (xy 0.551765 -2.157659) (xy 0.550333 -2.151257)
      (xy 0.588716 -2.132939) (xy 0.688116 -2.116733) (xy 0.79375 -2.108196) (xy 1.037167 -2.0955)
      (xy 1.037167 -1.502834) (xy 0.153558 -1.491376) (xy -0.17891 -1.48881) (xy -0.43308 -1.490975)
      (xy -0.615205 -1.498125) (xy -0.731536 -1.510514) (xy -0.788324 -1.528399) (xy -0.790204 -1.529841)
      (xy -0.826825 -1.595906) (xy -0.840311 -1.722067) (xy -0.837929 -1.837632) (xy -0.826521 -2.074334)
      (xy -0.762 -2.074334) (xy -0.762 -1.827389) (xy -0.75736 -1.689365) (xy -0.745357 -1.587696)
      (xy -0.732909 -1.551354) (xy -0.683446 -1.542947) (xy -0.562753 -1.536662) (xy -0.384246 -1.532775)
      (xy -0.16134 -1.531561) (xy 0.092547 -1.533297) (xy 0.124341 -1.533715) (xy 0.9525 -1.545167)
      (xy 0.965103 -1.80975) (xy 0.977707 -2.074334) (xy 0.729066 -2.074334) (xy 0.574793 -2.06788)
      (xy 0.476142 -2.043161) (xy 0.404687 -1.992142) (xy 0.39209 -1.979084) (xy 0.322138 -1.874007)
      (xy 0.289461 -1.778) (xy 0.256616 -1.695656) (xy 0.173648 -1.672192) (xy 0.169333 -1.672167)
      (xy 0.088772 -1.689652) (xy 0.063947 -1.758497) (xy 0.0635 -1.778) (xy 0.082111 -1.859412)
      (xy 0.15407 -1.89355) (xy 0.179933 -1.897231) (xy 0.282215 -1.935168) (xy 0.340172 -1.992481)
      (xy 0.353963 -2.02527) (xy 0.34599 -2.047886) (xy 0.304059 -2.062213) (xy 0.215976 -2.070138)
      (xy 0.069544 -2.073547) (xy -0.147429 -2.074327) (xy -0.189011 -2.074334) (xy -0.762 -2.074334)
      (xy -0.826521 -2.074334) (xy -0.8255 -2.0955) (xy -0.254 -2.105818) (xy -0.035606 -2.111078)
      (xy 0.157811 -2.118175) (xy 0.307585 -2.126253) (xy 0.395048 -2.134452) (xy 0.403331 -2.136011)
      (xy 0.472449 -2.176726) (xy 0.573263 -2.26506) (xy 0.6847 -2.38242) (xy 0.691521 -2.390276)
      (xy 0.893879 -2.624667) (xy -0.804333 -2.624667) (xy -0.811729 -2.44475) (xy -0.819125 -2.264834)
      (xy -0.835418 -2.446554) (xy -0.851711 -2.628275) (xy -1.156106 -2.615888) (xy -1.4605 -2.6035)
      (xy -1.471511 -0.637763) (xy -1.473736 -0.158089) (xy -1.474487 0.243021) (xy -1.5201 0.243021)
      (xy -1.521299 0.143994) (xy -1.524371 -0.23482) (xy -1.526073 -0.606871) (xy -1.526955 -1.098715)
      (xy -1.526406 -1.511444) (xy -1.5243 -1.8506) (xy -1.520514 -2.121725) (xy -1.514924 -2.330362)
      (xy -1.507406 -2.482051) (xy -1.497835 -2.582335) (xy -1.486088 -2.636755) (xy -1.480409 -2.64735)
      (xy -1.411334 -2.685654) (xy -1.277038 -2.705455) (xy -1.137817 -2.709334) (xy -0.846667 -2.709334)
      (xy -0.846667 -3.556) (xy -0.804333 -3.556) (xy -0.804333 -2.70765) (xy 0.994833 -2.7305)
      (xy 1.006949 -3.14325) (xy 1.019065 -3.556) (xy 1.058333 -3.556) (xy 1.059856 -3.185584)
      (xy 1.061378 -2.815167) (xy 1.155106 -2.926764) (xy 1.228535 -3.012847) (xy 1.336374 -3.137691)
      (xy 1.457149 -3.276452) (xy 1.475272 -3.297181) (xy 1.70171 -3.556001) (xy 1.380022 -3.556001)
      (xy 1.058333 -3.556) (xy 1.019065 -3.556) (xy 1.019066 -3.556001) (xy 0.107366 -3.556001)
      (xy -0.804333 -3.556) (xy -0.846667 -3.556) (xy -1.566333 -3.556) (xy -1.828655 -3.555522)
      (xy -2.01812 -3.553181) (xy -2.146538 -3.54762) (xy -2.225719 -3.537481) (xy -2.267471 -3.521407)
      (xy -2.283604 -3.498039) (xy -2.286 -3.473258) (xy -2.257409 -3.38825) (xy -2.187811 -3.292542)
      (xy -2.180167 -3.284682) (xy -2.091907 -3.14697) (xy -2.074333 -3.048) (xy -2.114332 -2.898881)
      (xy -2.180167 -2.811319) (xy -2.261135 -2.723927) (xy -2.275121 -2.682507) (xy -2.219235 -2.677706)
      (xy -2.142682 -2.690051) (xy -2.02974 -2.696796) (xy -1.970889 -2.670866) (xy -1.978118 -2.635483)
      (xy -2.018958 -2.631438) (xy -2.163736 -2.638013) (xy -2.243835 -2.614401) (xy -2.278248 -2.543367)
      (xy -2.285965 -2.407676) (xy -2.286 -2.389101) (xy -2.280604 -2.246115) (xy -2.256459 -2.155335)
      (xy -2.201627 -2.084577) (xy -2.159 -2.046671) (xy -2.055545 -1.921623) (xy -2.032 -1.824553)
      (xy -2.057294 -1.722209) (xy -2.118679 -1.618142) (xy -2.194405 -1.542996) (xy -2.245316 -1.524001)
      (xy -2.265234 -1.485227) (xy -2.279735 -1.383073) (xy -2.285946 -1.238783) (xy -2.286 -1.223176)
      (xy -2.282943 -1.061313) (xy -2.269342 -0.959917) (xy -2.238554 -0.894877) (xy -2.183935 -0.842085)
      (xy -2.180167 -0.839104) (xy -2.108068 -0.761018) (xy -2.078042 -0.656865) (xy -2.074333 -0.5715)
      (xy -2.086603 -0.436258) (xy -2.132836 -0.347587) (xy -2.180167 -0.303897) (xy -2.236266 -0.251079)
      (xy -2.268175 -0.187321) (xy -2.282536 -0.088511) (xy -2.285994 0.06946) (xy -2.286 0.080175)
      (xy -2.282071 0.244072) (xy -2.268294 0.33826) (xy -2.24169 0.377419) (xy -2.224901 0.381)
      (xy -2.149398 0.417662) (xy -2.080037 0.507375) (xy -2.037197 0.61973) (xy -2.032 0.668842)
      (xy -2.060952 0.760964) (xy -2.133036 0.86744) (xy -2.159 0.895512) (xy -2.246514 1.004017)
      (xy -2.281878 1.120901) (xy -2.286 1.208108) (xy -2.286 1.393703) (xy -1.915583 1.407813)
      (xy -1.545167 1.421922) (xy -1.915583 1.430628) (xy -2.117962 1.441224) (xy -2.240998 1.465119)
      (xy -2.28964 1.507654) (xy -2.268838 1.574171) (xy -2.183541 1.67001) (xy -2.159 1.693333)
      (xy -2.061694 1.812143) (xy -2.040758 1.926234) (xy -2.096191 2.051804) (xy -2.159 2.131365)
      (xy -2.286 2.27601) (xy -2.286 2.979505) (xy -2.28859 3.269002) (xy -2.296219 3.484721)
      (xy -2.308679 3.623292) (xy -2.32576 3.681347) (xy -2.329672 3.683) (xy -2.346521 3.642165)
      (xy -2.355751 3.519209) (xy -2.357378 3.313453) (xy -2.351419 3.024218) (xy -2.348732 2.938323)
      (xy -2.339573 2.670865) (xy -2.330978 2.474731) (xy -2.320772 2.336622) (xy -2.306779 2.24324)
      (xy -2.286826 2.181287) (xy -2.258738 2.137464) (xy -2.220339 2.098472) (xy -2.20981 2.088779)
      (xy -2.139909 2.013026) (xy -2.136748 1.970702) (xy -2.153207 1.960498) (xy -2.189726 1.933674)
      (xy -2.153207 1.898643) (xy -2.130093 1.861766) (xy -2.164163 1.806173) (xy -2.233083 1.741935)
      (xy -2.319311 1.648116) (xy -2.367202 1.557756) (xy -2.370667 1.535028) (xy -2.392939 1.453888)
      (xy -2.423584 1.425036) (xy -2.454779 1.405909) (xy -2.423583 1.400342) (xy -2.387295 1.357005)
      (xy -2.371334 1.236076) (xy -2.370667 1.19476) (xy -2.361899 1.0587) (xy -2.324463 0.966786)
      (xy -2.241663 0.879347) (xy -2.235707 0.874095) (xy -2.154726 0.794877) (xy -2.135328 0.746703)
      (xy -2.161623 0.717149) (xy -2.195084 0.684996) (xy -2.169583 0.677981) (xy -2.120009 0.652626)
      (xy -2.128173 0.591141) (xy -2.187477 0.512438) (xy -2.243667 0.465666) (xy -2.307047 0.416135)
      (xy -2.344822 0.364341) (xy -2.363604 0.288036) (xy -2.370008 0.164969) (xy -2.370667 0.038402)
      (xy -2.368997 -0.130353) (xy -2.360377 -0.233933) (xy -2.339398 -0.291816) (xy -2.300644 -0.323478)
      (xy -2.266016 -0.338218) (xy -2.172437 -0.411499) (xy -2.133643 -0.488458) (xy -2.128801 -0.606256)
      (xy -2.162094 -0.716776) (xy -2.221272 -0.790316) (xy -2.263926 -0.804334) (xy -2.321418 -0.832506)
      (xy -2.329477 -0.85725) (xy -2.331489 -0.923697) (xy -2.335703 -1.048536) (xy -2.341232 -1.205548)
      (xy -2.3416 -1.215809) (xy -2.345239 -1.376116) (xy -2.337572 -1.475662) (xy -2.312127 -1.538214)
      (xy -2.262431 -1.587539) (xy -2.234623 -1.608659) (xy -2.135569 -1.722692) (xy -2.11615 -1.848788)
      (xy -2.176033 -1.971209) (xy -2.243667 -2.032001) (xy -2.310788 -2.085529) (xy -2.348845 -2.142475)
      (xy -2.366035 -2.227645) (xy -2.370555 -2.365844) (xy -2.370667 -2.416297) (xy -2.366502 -2.580727)
      (xy -2.35024 -2.684189) (xy -2.316233 -2.750137) (xy -2.282135 -2.783832) (xy -2.171609 -2.916428)
      (xy -2.144614 -3.059876) (xy -2.181397 -3.17738) (xy -2.236674 -3.262586) (xy -2.284189 -3.301723)
      (xy -2.287087 -3.302) (xy -2.312917 -3.339559) (xy -2.327282 -3.433385) (xy -2.328333 -3.471334)
      (xy -2.328333 -3.640667) (xy -1.598083 -3.641261) (xy -1.051144 -3.641673) (xy -0.521012 -3.642007)
      (xy -0.01551 -3.642263) (xy 0.457539 -3.64244) (xy 0.890314 -3.642535) (xy 1.274992 -3.642548)
      (xy 1.60375 -3.642478)) (layer F.SilkS) (width 0.01))
  )

  (module Package_TO_SOT_THT:TO-92 (layer Front) (tedit 5E79AD3C) (tstamp 5E7A33AC)
    (at 84 98)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference REF** (at 1.27 -3.56) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TO-92 (at 1.27 2.79) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end 1.27 -2.6) (angle 135) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle -135) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 1.27 -2.6) (angle -135) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 1.27 -2.48) (angle 135) (layer F.Fab) (width 0.1))
    (fp_line (start 4 2.01) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4 2.01) (end 4 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.46 -2.73) (end 4 -2.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 1.75) (end 3 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -0.53 1.85) (end 3.07 1.85) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text 3 (at 87.108478 99.838478) (layer F.SilkS) (tstamp 5E7A33DF)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text 1 (at 83 96) (layer F.SilkS) (tstamp 5E7A33DA)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text "FET 3,   2,   1" (at 67 85) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_poly (pts (xy 40.8 83.4) (xy 40.8 82.6) (xy 38.4 82.6) (xy 38.4 83.4)) (layer F.Mask) (width 0.15))
  (gr_poly (pts (xy 40.8 84.8) (xy 40.8 84) (xy 38.4 84) (xy 38.4 84.8)) (layer F.Mask) (width 0.15))
  (gr_poly (pts (xy 40.8 86) (xy 40.8 85.2) (xy 38.4 85.2) (xy 38.4 86)) (layer F.Mask) (width 0.15))
  (gr_poly (pts (xy 40.8 87.2) (xy 40.8 86.4) (xy 38.4 86.4) (xy 38.4 87.2)) (layer F.Mask) (width 0.15))
  (gr_text "VDD\nCLK\nDATA\nGND" (at 33 85) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_line (start 30.48 54.61) (end 87.63 54.61) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 30.48 102.87) (end 30.48 54.61) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 31.75 105.41) (end 30.48 102.87) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 87.63 105.41) (end 31.75 105.41) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 87.63 54.61) (end 87.63 105.41) (layer Edge.Cuts) (width 0.2))
  (gr_poly (pts (xy 82.55 64.77) (xy 82.55 55.88) (xy 34.29 55.88) (xy 34.29 64.77)) (layer F.Mask) (width 0.15))
  (gr_text GND (at 33.02 69.85) (layer F.SilkS) (tstamp 5E79A5E7)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text GND (at 84.455 102.87) (layer F.SilkS) (tstamp 5E79A57E)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text V+ (at 84.455 100.33) (layer F.SilkS) (tstamp 5E79A57D)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_line (start 72.39 84.455) (end 82.55 84.455) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 72.39 85.725) (end 72.39 84.455) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 82.55 85.725) (end 72.39 85.725) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 82.55 84.455) (end 82.55 85.725) (layer Edge.Cuts) (width 0.2))
  (gr_poly (pts (xy 72.39 101.6) (xy 82.55 101.6) (xy 82.55 68.58) (xy 72.39 68.58)) (layer F.Mask) (width 0.15))
  (gr_text V+ (at 85.725 67.31) (layer F.SilkS) (tstamp 5E706317)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text GND (at 85.725 69.85) (layer F.SilkS) (tstamp 5E6FB8FC)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text V+ (at 63.5 99.06) (layer F.SilkS) (tstamp 5E6F8E4A)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text GND (at 33.02 102.87) (layer F.SilkS) (tstamp 5E6F8E3A)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text V+ (at 33.02 100.33) (layer F.SilkS) (tstamp 5E6F8E37)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )
  (gr_text V+ (at 33.02 67.31) (layer F.SilkS) (tstamp 5E6F8E1A)
    (effects (font (size 0.7 0.7) (thickness 0.175)))
  )

  (segment (start 42.545 86.995) (end 41.91 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 42.545 97.79) (end 42.545 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 86.995) (end 44.45 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 97.79) (end 45.085 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 86.995) (end 46.99 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 97.79) (end 47.625 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 86.995) (end 49.53 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 97.79) (end 50.165 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 86.36) (end 42.545 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 86.995) (end 45.72 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.085 87.63) (end 45.085 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 86.995) (end 48.26 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 47.625 87.63) (end 47.625 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 86.995) (end 50.8 86.36) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.165 87.63) (end 50.165 86.995) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 88.9) (end 43.18 88.9) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 88.9) (end 45.72 88.9) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 91.44) (end 44.45 91.44) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 91.44) (end 41.91 91.44) (width 0.4064) (layer Back) (net 0))
  (segment (start 41.91 93.98) (end 43.18 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 44.45 93.98) (end 45.72 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 45.72 96.52) (end 44.45 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 43.18 96.52) (end 41.91 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 96.52) (end 48.26 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 93.98) (end 46.99 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 46.99 91.44) (end 48.26 91.44) (width 0.4064) (layer Back) (net 0))
  (segment (start 48.26 88.9) (end 46.99 88.9) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 88.9) (end 50.8 88.9) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 91.44) (end 49.53 91.44) (width 0.4064) (layer Back) (net 0))
  (segment (start 49.53 93.98) (end 50.8 93.98) (width 0.4064) (layer Back) (net 0))
  (segment (start 50.8 96.52) (end 49.53 96.52) (width 0.4064) (layer Back) (net 0))
  (segment (start 34.29 99.06) (end 35.56 100.33) (width 1.27) (layer Front) (net 0))
  (segment (start 34.29 97.79) (end 34.29 99.06) (width 1.27) (layer Front) (net 0))
  (segment (start 35.56 100.33) (end 68.58 100.33) (width 1.27) (layer Front) (net 0))
  (segment (start 66.04 102.87) (end 35.56 102.87) (width 1.27) (layer Back) (net 0))
  (segment (start 34.29 69.85) (end 67.31 69.85) (width 1.27) (layer Back) (net 0))
  (segment (start 52.07 88.9) (end 53.34 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D30))
  (segment (start 54.61 88.9) (end 55.88 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D31))
  (segment (start 55.88 91.44) (end 54.61 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D32))
  (segment (start 53.34 91.44) (end 52.07 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D33))
  (segment (start 52.07 93.98) (end 53.34 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D34))
  (segment (start 54.61 93.98) (end 55.88 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D35))
  (segment (start 55.88 96.52) (end 54.61 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D36))
  (segment (start 53.34 96.52) (end 52.07 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D37))
  (segment (start 57.15 96.52) (end 58.42 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D38))
  (segment (start 58.42 93.98) (end 57.15 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D39))
  (segment (start 57.15 91.44) (end 58.42 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D3A))
  (segment (start 58.42 88.9) (end 57.15 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D3B))
  (segment (start 59.69 88.9) (end 60.96 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D3C))
  (segment (start 60.96 91.44) (end 59.69 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D3D))
  (segment (start 59.69 93.98) (end 60.96 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D3E))
  (segment (start 60.325 97.79) (end 60.325 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D4A))
  (segment (start 52.705 86.995) (end 52.07 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D4B))
  (segment (start 52.705 97.79) (end 52.705 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D4C))
  (segment (start 55.245 86.995) (end 54.61 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D4D))
  (segment (start 55.245 97.79) (end 55.245 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D4E))
  (segment (start 57.785 86.995) (end 57.15 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D4F))
  (segment (start 57.785 97.79) (end 57.785 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D50))
  (segment (start 60.325 86.995) (end 59.69 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D51))
  (segment (start 60.96 96.52) (end 59.69 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D5D))
  (segment (start 53.34 86.36) (end 52.705 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D5E))
  (segment (start 55.245 86.995) (end 55.88 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D5F))
  (segment (start 55.245 87.63) (end 55.245 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D60))
  (segment (start 57.785 86.995) (end 58.42 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D61))
  (segment (start 57.785 87.63) (end 57.785 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D62))
  (segment (start 60.325 86.995) (end 60.96 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D63))
  (segment (start 60.325 87.63) (end 60.325 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6F9D64))
  (segment (start 53.34 81.28) (end 52.07 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA534))
  (segment (start 41.91 73.66) (end 43.18 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA54F))
  (segment (start 44.45 73.66) (end 45.72 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA550))
  (segment (start 45.72 76.2) (end 44.45 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA551))
  (segment (start 43.18 76.2) (end 41.91 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA552))
  (segment (start 41.91 78.74) (end 43.18 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA553))
  (segment (start 44.45 78.74) (end 45.72 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA554))
  (segment (start 45.72 81.28) (end 44.45 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA555))
  (segment (start 43.18 81.28) (end 41.91 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA556))
  (segment (start 46.99 81.28) (end 48.26 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA557))
  (segment (start 48.26 78.74) (end 46.99 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA558))
  (segment (start 46.99 76.2) (end 48.26 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA559))
  (segment (start 48.26 73.66) (end 46.99 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA55A))
  (segment (start 49.53 73.66) (end 50.8 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA55B))
  (segment (start 50.8 76.2) (end 49.53 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA55C))
  (segment (start 49.53 78.74) (end 50.8 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA55D))
  (segment (start 57.15 81.28) (end 58.42 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA569))
  (segment (start 55.88 76.2) (end 54.61 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA578))
  (segment (start 50.8 81.28) (end 49.53 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA58B))
  (segment (start 53.34 76.2) (end 52.07 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA58C))
  (segment (start 54.61 73.66) (end 55.88 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA5CF))
  (segment (start 60.96 76.2) (end 59.69 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA5EA))
  (segment (start 59.69 78.74) (end 60.96 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA612))
  (segment (start 58.42 73.66) (end 57.15 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA654))
  (segment (start 54.61 78.74) (end 55.88 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA6A3))
  (segment (start 55.88 81.28) (end 54.61 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA6A4))
  (segment (start 60.96 81.28) (end 59.69 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA6D9))
  (segment (start 59.69 73.66) (end 60.96 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA6EC))
  (segment (start 58.42 78.74) (end 57.15 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA6ED))
  (segment (start 52.07 73.66) (end 53.34 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA6EE))
  (segment (start 57.15 76.2) (end 58.42 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA716))
  (segment (start 52.07 78.74) (end 53.34 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FA7A6))
  (segment (start 62.23 88.9) (end 63.5 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB854))
  (segment (start 64.77 88.9) (end 66.04 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB855))
  (segment (start 66.04 91.44) (end 64.77 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB856))
  (segment (start 63.5 91.44) (end 62.23 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB857))
  (segment (start 62.23 93.98) (end 63.5 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB858))
  (segment (start 64.77 93.98) (end 66.04 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB859))
  (segment (start 66.04 96.52) (end 64.77 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB85A))
  (segment (start 63.5 96.52) (end 62.23 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB85B))
  (segment (start 67.31 96.52) (end 68.58 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB85C))
  (segment (start 68.58 93.98) (end 67.31 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB85D))
  (segment (start 67.31 91.44) (end 68.58 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB85E))
  (segment (start 68.58 88.9) (end 67.31 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB85F))
  (segment (start 69.85 88.9) (end 71.12 88.9) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB860))
  (segment (start 71.12 91.44) (end 69.85 91.44) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB861))
  (segment (start 69.85 93.98) (end 71.12 93.98) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB862))
  (segment (start 70.485 97.79) (end 70.485 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB86F))
  (segment (start 62.865 86.995) (end 62.23 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB898))
  (segment (start 62.865 97.79) (end 62.865 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB899))
  (segment (start 65.405 86.995) (end 64.77 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB89A))
  (segment (start 65.405 97.79) (end 65.405 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB89B))
  (segment (start 67.945 86.995) (end 67.31 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB89C))
  (segment (start 67.945 97.79) (end 67.945 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB89D))
  (segment (start 70.485 86.995) (end 69.85 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB89E))
  (segment (start 71.12 96.52) (end 69.85 96.52) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8AA))
  (segment (start 63.5 86.36) (end 62.865 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8AC))
  (segment (start 65.405 86.995) (end 66.04 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8AD))
  (segment (start 65.405 87.63) (end 65.405 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8AE))
  (segment (start 67.945 86.995) (end 68.58 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8AF))
  (segment (start 67.945 87.63) (end 67.945 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8B0))
  (segment (start 70.485 86.995) (end 71.12 86.36) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8B1))
  (segment (start 70.485 87.63) (end 70.485 86.995) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB8B2))
  (segment (start 62.23 73.66) (end 63.5 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FB986))
  (segment (start 64.77 73.66) (end 66.04 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBABE))
  (segment (start 66.04 76.2) (end 64.77 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBABF))
  (segment (start 63.5 76.2) (end 62.23 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC0))
  (segment (start 62.23 78.74) (end 63.5 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC1))
  (segment (start 64.77 78.74) (end 66.04 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC2))
  (segment (start 66.04 81.28) (end 64.77 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC3))
  (segment (start 63.5 81.28) (end 62.23 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC4))
  (segment (start 67.31 81.28) (end 68.58 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC5))
  (segment (start 68.58 78.74) (end 67.31 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC6))
  (segment (start 67.31 76.2) (end 68.58 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC7))
  (segment (start 68.58 73.66) (end 67.31 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC8))
  (segment (start 69.85 73.66) (end 71.12 73.66) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBAC9))
  (segment (start 71.12 76.2) (end 69.85 76.2) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBACA))
  (segment (start 69.85 78.74) (end 71.12 78.74) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBACB))
  (segment (start 71.12 81.28) (end 69.85 81.28) (width 0.4064) (layer Back) (net 0) (tstamp 5E6FBC91))
  (segment (start 71.12 102.87) (end 63.85 102.87) (width 1.27) (layer Back) (net 0) (tstamp 5E6FC692))
  (segment (start 69.85 69.85) (end 67.31 69.85) (width 1.27) (layer Back) (net 0))
  (segment (start 69.85 67.31) (end 67.31 67.31) (width 1.27) (layer Front) (net 0))
  (segment (start 33.02 71.755) (end 33.02 74.515) (width 0.508) (layer Back) (net 0))
  (segment (start 34.495 79.17) (end 34.29 79.375) (width 0.508) (layer Back) (net 0))
  (segment (start 34.495 76.04) (end 34.495 79.17) (width 0.508) (layer Back) (net 0))
  (segment (start 31.545 79.17) (end 31.75 79.375) (width 0.508) (layer Back) (net 0))
  (segment (start 31.545 76.04) (end 31.545 79.17) (width 0.508) (layer Back) (net 0))
  (segment (start 42.545 74.295) (end 41.91 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 42.545 82.55) (end 42.545 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 45.085 74.295) (end 44.45 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 45.085 82.55) (end 45.085 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 47.625 74.295) (end 46.99 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 47.625 82.55) (end 47.625 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 50.165 74.295) (end 49.53 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 50.165 82.55) (end 50.165 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 52.705 74.295) (end 52.07 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 52.705 82.55) (end 52.705 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 55.245 74.295) (end 54.61 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 55.245 74.93) (end 55.245 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 57.785 74.295) (end 57.15 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 57.785 82.55) (end 57.785 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 60.325 74.295) (end 59.69 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 60.325 82.55) (end 60.325 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 62.865 74.295) (end 62.23 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 62.865 82.55) (end 62.865 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 65.405 74.295) (end 64.77 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 65.405 82.55) (end 65.405 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 67.945 74.295) (end 67.31 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 67.945 82.55) (end 67.945 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 70.485 74.295) (end 69.85 73.66) (width 1.27) (layer Front) (net 0))
  (segment (start 70.485 82.55) (end 70.485 74.295) (width 1.27) (layer Front) (net 0))
  (segment (start 42.545 82.55) (end 42.545 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 45.085 82.55) (end 45.085 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 47.625 82.55) (end 47.625 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 50.165 82.55) (end 50.165 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 52.705 82.55) (end 52.705 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 55.245 82.55) (end 55.245 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 57.785 82.55) (end 57.785 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 60.325 82.55) (end 60.325 74.93) (width 1.016) (layer Front) (net 0))
  (segment (start 69.85 67.31) (end 82.55 67.31) (width 1.27) (layer Front) (net 0))
  (segment (start 68.58 100.33) (end 81.28 100.33) (width 1.27) (layer Front) (net 0))
  (segment (start 71.12 102.87) (end 81.28 102.87) (width 1.27) (layer Back) (net 0))
  (segment (start 69.85 69.85) (end 82.55 69.85) (width 1.27) (layer Back) (net 0))
  (segment (start 83.6118 83.74) (end 83.185 83.3132) (width 0.2032) (layer Front) (net 0))
  (segment (start 84.14 83.74) (end 83.6118 83.74) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.185 83.3132) (end 83.185 76.835) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.185 76.835) (end 83.82 76.2) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.82 76.2) (end 85.09 76.2) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.887919 78.74) (end 83.82 78.807919) (width 0.2032) (layer Front) (net 0))
  (segment (start 85.09 78.74) (end 83.887919 78.74) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.82 78.807919) (end 83.82 81.915) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.82 81.915) (end 84.455 82.55) (width 0.2032) (layer Front) (net 0))
  (segment (start 84.455 82.55) (end 85.09 82.55) (width 0.2032) (layer Front) (net 0))
  (segment (start 85.09 82.55) (end 85.09 83.74) (width 0.2032) (layer Front) (net 0))
  (segment (start 86.04 82.23) (end 85.09 81.28) (width 0.2032) (layer Front) (net 0))
  (segment (start 86.04 83.74) (end 86.04 82.23) (width 0.2032) (layer Front) (net 0))
  (segment (start 86.04 87.95) (end 85.09 88.9) (width 0.2032) (layer Front) (net 0))
  (segment (start 86.04 86.44) (end 86.04 87.95) (width 0.2032) (layer Front) (net 0))
  (segment (start 85.09 86.44) (end 85.09 87.63) (width 0.2032) (layer Front) (net 0))
  (segment (start 85.09 87.63) (end 84.455 87.63) (width 0.2032) (layer Front) (net 0))
  (segment (start 84.455 87.63) (end 83.82 88.265) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.82 88.265) (end 83.82 90.17) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.82 90.17) (end 85.09 91.44) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.6118 86.44) (end 83.185 86.8668) (width 0.2032) (layer Front) (net 0))
  (segment (start 84.14 86.44) (end 83.6118 86.44) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.185 86.8668) (end 83.185 92.075) (width 0.2032) (layer Front) (net 0))
  (segment (start 83.185 92.075) (end 85.09 93.98) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.4 70.88) (end 39.37 69.85) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.4 77.8) (end 40.4 70.88) (width 0.2032) (layer Front) (net 0))
  (segment (start 38.8 87) (end 38 87) (width 0.2032) (layer Front) (net 0))
  (segment (start 37.2 81) (end 40.4 77.8) (width 0.2032) (layer Front) (net 0))
  (segment (start 38 87) (end 37.2 86.2) (width 0.2032) (layer Front) (net 0))
  (segment (start 37.2 86.2) (end 37.2 81) (width 0.2032) (layer Front) (net 0))
  (segment (start 41.8 71.8) (end 43 71.8) (width 0.2032) (layer Front) (net 0))
  (segment (start 41 78.2) (end 41 72.6) (width 0.2032) (layer Front) (net 0))
  (segment (start 43.2 71.6) (end 43.2 67.31) (width 0.2032) (layer Front) (net 0))
  (segment (start 34.29 67.31) (end 43.2 67.31) (width 1.27) (layer Front) (net 0))
  (segment (start 41 72.6) (end 41.8 71.8) (width 0.2032) (layer Front) (net 0))
  (segment (start 43.2 67.31) (end 67.31 67.31) (width 1.27) (layer Front) (net 0))
  (segment (start 40.6 83.2) (end 40.6 78.6) (width 0.2032) (layer Front) (net 0))
  (segment (start 43 71.8) (end 43.2 71.6) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.6 78.6) (end 41 78.2) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.695 84.4) (end 42.545 82.55) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.4 84.4) (end 40.695 84.4) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.515 85.6) (end 42.545 87.63) (width 0.2032) (layer Front) (net 0))
  (segment (start 40.4 85.6) (end 40.515 85.6) (width 0.2032) (layer Front) (net 0))
  (segment (start 70.695 98) (end 70.485 97.79) (width 0.2032) (layer Back) (net 0))
  (segment (start 84 98) (end 70.695 98) (width 0.2032) (layer Back) (net 0))
  (segment (start 85.27 96.73) (end 82.73 96.73) (width 0.2032) (layer Back) (net 0))
  (segment (start 69 85) (end 67.945 86.055) (width 0.2032) (layer Back) (net 0))
  (segment (start 82.73 96.73) (end 71 85) (width 0.2032) (layer Back) (net 0))
  (segment (start 67.945 86.055) (end 67.945 87.63) (width 0.2032) (layer Back) (net 0))
  (segment (start 71 85) (end 69 85) (width 0.2032) (layer Back) (net 0))
  (segment (start 65.405 98.992081) (end 65.405 97.79) (width 0.2032) (layer Back) (net 0))
  (segment (start 65.412919 99) (end 65.405 98.992081) (width 0.2032) (layer Back) (net 0))
  (segment (start 85.54 99) (end 65.412919 99) (width 0.2032) (layer Back) (net 0))
  (segment (start 86.54 98) (end 85.54 99) (width 0.2032) (layer Back) (net 0))

  (zone (net 0) (net_name "") (layer Front) (tstamp 5E6EE475) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 99.06) (xy 82.55 101.6) (xy 82.55 86.36) (xy 72.39 86.36) (xy 72.39 101.6)
        (xy 82.55 101.6)
      )
    )
    (filled_polygon
      (pts
        (xy 75.271086 101.473) (xy 74.588914 101.473) (xy 74.708299 101.342) (xy 75.151701 101.342)
      )
    )
    (filled_polygon
      (pts
        (xy 77.811086 101.473) (xy 77.128914 101.473) (xy 77.248299 101.342) (xy 77.691701 101.342)
      )
    )
    (filled_polygon
      (pts
        (xy 80.351086 101.473) (xy 79.668914 101.473) (xy 79.788299 101.342) (xy 80.231701 101.342)
      )
    )
    (filled_polygon
      (pts
        (xy 82.423 101.473) (xy 82.208914 101.473) (xy 82.423 101.238085)
      )
    )
    (filled_polygon
      (pts
        (xy 72.731086 101.473) (xy 72.517 101.473) (xy 72.517 101.342) (xy 72.611701 101.342)
      )
    )
    (filled_polygon
      (pts
        (xy 75.100397 86.654637) (xy 75.486706 86.893689) (xy 75.593339 86.787057) (xy 75.772944 86.966662) (xy 75.666311 87.073294)
        (xy 75.905363 87.459603) (xy 76.931272 87.877988) (xy 78.039197 87.871928) (xy 79.034637 87.459603) (xy 79.273689 87.073294)
        (xy 79.167057 86.966662) (xy 79.346662 86.787057) (xy 79.453294 86.893689) (xy 79.839603 86.654637) (xy 79.907969 86.487)
        (xy 82.423 86.487) (xy 82.423 99.421915) (xy 82.161358 99.134817) (xy 81.636892 98.888514) (xy 81.407 99.009181)
        (xy 81.407 99.104224) (xy 81.400847 99.103) (xy 81.159153 99.103) (xy 81.153 99.104224) (xy 81.153 99.009181)
        (xy 80.923108 98.888514) (xy 80.398642 99.134817) (xy 80.231701 99.318) (xy 79.788299 99.318) (xy 79.621358 99.134817)
        (xy 79.096892 98.888514) (xy 78.867 99.009181) (xy 78.867 99.104224) (xy 78.860847 99.103) (xy 78.619153 99.103)
        (xy 78.613 99.104224) (xy 78.613 99.009181) (xy 78.383108 98.888514) (xy 77.858642 99.134817) (xy 77.691701 99.318)
        (xy 77.248299 99.318) (xy 77.081358 99.134817) (xy 76.556892 98.888514) (xy 76.327 99.009181) (xy 76.327 99.104224)
        (xy 76.320847 99.103) (xy 76.079153 99.103) (xy 76.073 99.104224) (xy 76.073 99.009181) (xy 75.843108 98.888514)
        (xy 75.318642 99.134817) (xy 75.151701 99.318) (xy 74.708299 99.318) (xy 74.541358 99.134817) (xy 74.016892 98.888514)
        (xy 73.787 99.009181) (xy 73.787 99.104224) (xy 73.780847 99.103) (xy 73.539153 99.103) (xy 73.533 99.104224)
        (xy 73.533 99.009181) (xy 73.303108 98.888514) (xy 72.778642 99.134817) (xy 72.611701 99.318) (xy 72.517 99.318)
        (xy 72.517 86.487) (xy 75.03096 86.487)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Front) (tstamp 5E6EE472) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 68.58) (xy 82.55 83.82) (xy 72.39 83.82) (xy 72.39 68.58)
      )
    )
    (filled_polygon
      (pts
        (xy 81.668642 71.045183) (xy 82.193108 71.291486) (xy 82.423 71.170819) (xy 82.423 83.693) (xy 79.90904 83.693)
        (xy 79.839603 83.525363) (xy 79.453294 83.286311) (xy 79.346662 83.392944) (xy 79.167057 83.213339) (xy 79.273689 83.106706)
        (xy 79.034637 82.720397) (xy 78.008728 82.302012) (xy 76.900803 82.308072) (xy 75.905363 82.720397) (xy 75.666311 83.106706)
        (xy 75.772944 83.213339) (xy 75.593339 83.392944) (xy 75.486706 83.286311) (xy 75.100397 83.525363) (xy 75.032031 83.693)
        (xy 72.517 83.693) (xy 72.517 71.170819) (xy 72.746892 71.291486) (xy 73.271358 71.045183) (xy 73.66 70.618729)
        (xy 74.048642 71.045183) (xy 74.573108 71.291486) (xy 74.803 71.170819) (xy 74.803 71.075776) (xy 74.809153 71.077)
        (xy 75.050847 71.077) (xy 75.057 71.075776) (xy 75.057 71.170819) (xy 75.286892 71.291486) (xy 75.811358 71.045183)
        (xy 76.2 70.618729) (xy 76.588642 71.045183) (xy 77.113108 71.291486) (xy 77.343 71.170819) (xy 77.343 71.075776)
        (xy 77.349153 71.077) (xy 77.590847 71.077) (xy 77.597 71.075776) (xy 77.597 71.170819) (xy 77.826892 71.291486)
        (xy 78.351358 71.045183) (xy 78.74 70.618729) (xy 79.128642 71.045183) (xy 79.653108 71.291486) (xy 79.883 71.170819)
        (xy 79.883 71.075776) (xy 79.889153 71.077) (xy 80.130847 71.077) (xy 80.137 71.075776) (xy 80.137 71.170819)
        (xy 80.366892 71.291486) (xy 80.891358 71.045183) (xy 81.28 70.618729)
      )
    )
    (filled_polygon
      (pts
        (xy 73.678962 69.85) (xy 73.704224 69.977) (xy 73.615776 69.977) (xy 73.641038 69.85) (xy 73.615776 69.723)
        (xy 73.704224 69.723)
      )
    )
    (filled_polygon
      (pts
        (xy 76.218962 69.85) (xy 76.244224 69.977) (xy 76.155776 69.977) (xy 76.181038 69.85) (xy 76.155776 69.723)
        (xy 76.244224 69.723)
      )
    )
    (filled_polygon
      (pts
        (xy 78.758962 69.85) (xy 78.784224 69.977) (xy 78.695776 69.977) (xy 78.721038 69.85) (xy 78.695776 69.723)
        (xy 78.784224 69.723)
      )
    )
    (filled_polygon
      (pts
        (xy 81.298962 69.85) (xy 81.324224 69.977) (xy 81.235776 69.977) (xy 81.261038 69.85) (xy 81.235776 69.723)
        (xy 81.324224 69.723)
      )
    )
    (filled_polygon
      (pts
        (xy 81.28 69.081271) (xy 80.938914 68.707) (xy 81.621086 68.707)
      )
    )
    (filled_polygon
      (pts
        (xy 78.74 69.081271) (xy 78.398914 68.707) (xy 79.081086 68.707)
      )
    )
    (filled_polygon
      (pts
        (xy 76.2 69.081271) (xy 75.858914 68.707) (xy 76.541086 68.707)
      )
    )
    (filled_polygon
      (pts
        (xy 73.66 69.081271) (xy 73.318914 68.707) (xy 74.001086 68.707)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Front) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 64.77) (xy 82.55 55.88) (xy 34.29 55.88) (xy 34.29 64.77)
      )
    )
    (filled_polygon
      (pts
        (xy 82.423 57.250959) (xy 82.255363 57.320397) (xy 82.016311 57.706706) (xy 82.122944 57.813339) (xy 81.943339 57.992944)
        (xy 81.836706 57.886311) (xy 81.450397 58.125363) (xy 81.032012 59.151272) (xy 81.038072 60.259197) (xy 81.450397 61.254637)
        (xy 81.836706 61.493689) (xy 81.943339 61.387057) (xy 82.122944 61.566662) (xy 82.016311 61.673294) (xy 82.255363 62.059603)
        (xy 82.423 62.127969) (xy 82.423 64.643) (xy 34.417 64.643) (xy 34.417 56.007) (xy 82.423 56.007)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Front) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.6 87.2) (xy 38.4 87.2) (xy 38.4 86.4) (xy 40.8 86.4) (xy 40.8 87.2)
        (xy 39.8 87.2)
      )
    )
    (filled_polygon
      (pts
        (xy 40.673 87.073) (xy 39.273455 87.073) (xy 39.287976 87) (xy 39.250831 86.81326) (xy 39.145051 86.654949)
        (xy 38.98674 86.549169) (xy 38.875289 86.527) (xy 40.673 86.527)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Front) (tstamp 5E79E687) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.6 86) (xy 38.4 86) (xy 38.4 85.2) (xy 40.8 85.2) (xy 40.8 86)
        (xy 39.8 86)
      )
    )
    (filled_polygon
      (pts
        (xy 39.949169 85.41326) (xy 39.912024 85.6) (xy 39.949169 85.78674) (xy 40.006806 85.873) (xy 38.527 85.873)
        (xy 38.527 85.327) (xy 40.006806 85.327)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Front) (tstamp 5E79E689) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.6 84.8) (xy 38.4 84.8) (xy 38.4 84) (xy 40.8 84) (xy 40.8 84.8)
        (xy 39.8 84.8)
      )
    )
    (filled_polygon
      (pts
        (xy 39.949169 84.21326) (xy 39.912024 84.4) (xy 39.949169 84.58674) (xy 40.006806 84.673) (xy 38.527 84.673)
        (xy 38.527 84.127) (xy 40.006806 84.127)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Front) (tstamp 5E79E68B) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.6 83.4) (xy 38.4 83.4) (xy 38.4 82.6) (xy 40.8 82.6) (xy 40.8 83.4)
        (xy 39.8 83.4)
      )
    )
    (filled_polygon
      (pts
        (xy 40.1214 83.247135) (xy 40.126545 83.273) (xy 38.527 83.273) (xy 38.527 82.727) (xy 40.1214 82.727)
      )
    )
  )
)
