(module Jack_3.5mm_PJ311_Horizontal (layer F.Cu) (tedit 5A1DBF1B)
  (descr "PJ311 6pin SMD 3.5mm stereo headphones jack.")
  (tags "headphones jack plug stereo 3.5mm PJ311")
  (attr smd)
  (fp_text reference REF** (at 0 -10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_PJ311_Horizontal (at 0 7.17) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.1 -3.75) (end -4.45 -3.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -5.6) (end -4.45 -5.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -5.6) (end -3.1 -6.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -2.25) (end -3.1 -3.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 3.25) (end -3.1 -0.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.35 5.3) (end -3.1 5.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.1 3.45) (end 3.1 3.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.1 -3.75) (end 3.1 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.1 -6.9) (end 3.1 -5.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.6 -6.9) (end -2.6 -8.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.6 -8.9) (end 2.6 -8.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.6 -8.9) (end 2.6 -6.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.6 -6.9) (end 3.1 -6.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -6.9) (end -2.6 -6.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -3 5.2) (end 3 5.2) (layer F.Fab) (width 0.1))
  (fp_line (start 3 5.2) (end 3 -6.8) (layer F.Fab) (width 0.1))
  (fp_line (start 3 -6.8) (end 2.5 -6.8) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -6.8) (end 2.5 -8.8) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -8.8) (end -2.5 -8.8) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -8.8) (end -2.5 -6.8) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -6.8) (end -3 -6.8) (layer F.Fab) (width 0.1))
  (fp_line (start -3 -6.8) (end -3 5.2) (layer F.Fab) (width 0.1))
  (fp_line (start -5 -9.31) (end 5 -9.31) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5 -9.31) (end -5 5.94) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5 5.94) (end 5 -9.31) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5 5.94) (end 5 5.94) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -2.35 -4.65) (end -2.1 -4.65) (layer F.Fab) (width 0.12))
  (pad 6 smd rect (at -3.5 4.2) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3.5 -1.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.5 -4.7) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.5 4.7) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3.5 2.5) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 0 -4.3) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 2.7) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 smd rect (at 3.5 -4.7) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ311_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
