(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Air_Quality_Sensor_PPD42/pcb/msp_shield/msp_shield.sch)
    (date "Thu 06 Dec 2018 12:25:10 AM EST")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source msp_shield.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value CONN_01X10)
      (footprint Pin_Headers:Pin_Header_Straight_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08A58D))
    (comp (ref P2)
      (value CONN_01X10)
      (footprint Pin_Headers:Pin_Header_Straight_1x10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08A5F5))
    (comp (ref CON1)
      (value BARREL_JACK)
      (footprint Connectors:BARREL_JACK)
      (libsource (lib conn) (part BARREL_JACK))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08AC7C))
    (comp (ref U1)
      (value LM7805)
      (footprint TO_SOT_Packages_SMD:TO-252-2Lead)
      (datasheet regulator\lm78xx.pdf)
      (libsource (lib regul) (part LM7805))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08B030))
    (comp (ref C1)
      (value 1uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08B515))
    (comp (ref C2)
      (value 1uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08B57D))
    (comp (ref U2)
      (value MCP1703A-3302_MB)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf)
      (libsource (lib regul) (part MCP1703A-3302_MB))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08BABD))
    (comp (ref C3)
      (value 1uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08BEEC))
    (comp (ref C4)
      (value 1uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08BF42))
    (comp (ref P3)
      (value CONN_01X01)
      (footprint Pin_Headers:Pin_Header_Angled_2x40)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08D0ED))
    (comp (ref P4)
      (value CONN_02X05)
      (footprint Pin_Headers:Pin_Header_Straight_2x05)
      (libsource (lib conn) (part CONN_02X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C08D3A0))
    (comp (ref J1)
      (value JACK_2P)
      (footprint Connector_Audio:Jack_3.5mm_CUI_SJ1-3533NG_Horizontal_CircularHoles)
      (libsource (lib conn) (part JACK_2P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0925EC)))
  (libparts
    (libpart (lib conn) (part BARREL_JACK)
      (description "DC Barrel Jack")
      (fields
        (field (name Reference) CON)
        (field (name Value) BARREL_JACK))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X10)
      (description "Connector, single row, 01x10")
      (footprints
        (fp Pin_Header_Straight_1X10)
        (fp Pin_Header_Angled_1X10)
        (fp Socket_Strip_Straight_1X10)
        (fp Socket_Strip_Angled_1X10))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X10))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib conn) (part CONN_02X05)
      (description "Connector, double row, 02x05")
      (footprints
        (fp Pin_Header_Straight_2X05)
        (fp Pin_Header_Angled_2X05)
        (fp Socket_Strip_Straight_2X05)
        (fp Socket_Strip_Angled_2X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib conn) (part JACK_2P)
      (fields
        (field (name Reference) J)
        (field (name Value) JACK_2P))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib regul) (part 7805)
      (aliases
        (alias LM7805)
        (alias LM7812)
        (alias 78L05))
      (description "Linear Regulator +5V")
      (docs regulator\lm78xx.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 7805))
      (pins
        (pin (num GND) (name GND) (type input))
        (pin (num VI) (name VI) (type input))
        (pin (num VO) (name VO) (type power_out))))
    (libpart (lib regul) (part MCP1703A-3302_MB)
      (aliases
        (alias MCP1703A-3302E_MB)
        (alias MCP1703A-1202_MB)
        (alias MCP1703A-1502_MB)
        (alias MCP1703A-1802_MB)
        (alias MCP1703A-2502_MB)
        (alias MCP1703A-2802_MB)
        (alias MCP1703A-3002_MB)
        (alias MCP1703A-4002_MB)
        (alias MCP1703A-5002_MB)
        (alias MCP1703A-1202E_MB)
        (alias MCP1703A-1502E_MB)
        (alias MCP1703A-1802E_MB)
        (alias MCP1703A-2502E_MB)
        (alias MCP1703A-2802E_MB)
        (alias MCP1703A-3002E_MB)
        (alias MCP1703A-4002E_MB)
        (alias MCP1703A-5002E_MB))
      (description "Low Quiescent Current LDO Regulator, 3.3V, 250 mA, Vin<=16V")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf)
      (footprints
        (fp SOT89*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP1703A-3302_MB)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT89-3_Housing))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VI) (type power_in))
        (pin (num 3) (name VO) (type power_out)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib)))
  (nets
    (net (code 1) (name /WOL)
      (node (ref P4) (pin 3)))
    (net (code 2) (name GND)
      (node (ref C4) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref C1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref CON1) (pin 2))
      (node (ref CON1) (pin 3))
      (node (ref U1) (pin GND))
      (node (ref P4) (pin 10))
      (node (ref C3) (pin 2)))
    (net (code 3) (name /P2.5)
      (node (ref P1) (pin 8))
      (node (ref P3) (pin 1)))
    (net (code 4) (name /CLKOUT)
      (node (ref P4) (pin 1)))
    (net (code 5) (name /INT)
      (node (ref P4) (pin 2)))
    (net (code 6) (name /MISO)
      (node (ref P1) (pin 7))
      (node (ref P4) (pin 4)))
    (net (code 7) (name /MOSI)
      (node (ref P4) (pin 5))
      (node (ref P1) (pin 6)))
    (net (code 8) (name /P1.5)
      (node (ref P4) (pin 6))
      (node (ref P2) (pin 7)))
    (net (code 9) (name /RST)
      (node (ref P1) (pin 5))
      (node (ref P4) (pin 8)))
    (net (code 10) (name +3V3)
      (node (ref P2) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 11) (name /P1.2)
      (node (ref P2) (pin 4))
      (node (ref J1) (pin 1)))
    (net (code 12) (name /P1.1)
      (node (ref J1) (pin 2))
      (node (ref P2) (pin 3)))
    (net (code 13) (name /CS)
      (node (ref P2) (pin 8))
      (node (ref P4) (pin 7)))
    (net (code 15) (name /P2.2)
      (node (ref P2) (pin 10)))
    (net (code 16) (name /P2.1)
      (node (ref P2) (pin 9)))
    (net (code 17) (name /P2.3)
      (node (ref P1) (pin 10)))
    (net (code 18) (name /XIN)
      (node (ref P1) (pin 2)))
    (net (code 19) (name /XOUT)
      (node (ref P1) (pin 3)))
    (net (code 20) (name /TEST)
      (node (ref P1) (pin 4)))
    (net (code 21) (name /P2.4)
      (node (ref P1) (pin 9)))
    (net (code 22) (name /P1.0)
      (node (ref P2) (pin 2)))
    (net (code 23) (name /P1.3)
      (node (ref P2) (pin 5)))
    (net (code 24) (name /P1.4)
      (node (ref P2) (pin 6)))
    (net (code 25) (name "Net-(C1-Pad1)")
      (node (ref U1) (pin VI))
      (node (ref CON1) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 26) (name +5V)
      (node (ref U1) (pin VO))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref P4) (pin 9)))))