(module EdgeConnectorGasSensorPCB (layer F.Cu) (tedit 5CCA2B25)
  (fp_text reference PCB** (at 0 1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value EdgeConnectorGasSensorPCB (at 5 3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 0) (end 10 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 12 0) (end 12 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 -3) (end 0 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -3) (end 0 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 12 -3) (end 10 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 0) (end 12 0) (layer F.SilkS) (width 0.15))
  (fp_text user +7V (at 1 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user +5V (at 4 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 7.5 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Sns (at 10.5 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole oval (at 1.5 -1.5 90) (size 2.5 2.7) (drill oval 1.8 2) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 4.5 -1.5 90) (size 2.5 2.7) (drill oval 1.8 2) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 7.5 -1.5 90) (size 2.5 2.7) (drill oval 1.8 2) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 10.5 -1.5 90) (size 2.5 2.7) (drill oval 1.8 2) (layers *.Cu *.Mask))
)
