(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Misc_2019/Computer_Switchboard/pcb/pcb.sch)
    (date "Sun 17 Mar 2019 07:42:30 PM EDT")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source pcb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Arduino_Nano_Header)
      (footprint w_conn_misc:arduino_nano_header)
      (libsource (lib w_connectors) (part Arduino_Nano_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EC8FE))
    (comp (ref SW3)
      (value Rotary_Encoder)
      (footprint Rotary_Encoder:RotaryEncoder_Alps_EC11E_Vertical_H20mm)
      (libsource (lib device) (part Rotary_Encoder))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8ECF7B))
    (comp (ref R10)
      (value R2200)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8ED02C))
    (comp (ref R11)
      (value R2200)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8ED08A))
    (comp (ref SW2)
      (value SW_DIP_x08)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib switches) (part SW_DIP_x08))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE142))
    (comp (ref R3)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE393))
    (comp (ref R4)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE470))
    (comp (ref R5)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE53D))
    (comp (ref R6)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE543))
    (comp (ref R7)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE566))
    (comp (ref R8)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE56C))
    (comp (ref R9)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE572))
    (comp (ref R2)
      (value R)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EE595))
    (comp (ref P1)
      (value CONN_01X10)
      (footprint Displays_7-Segment:7SEGMENT-LED__HDSM531_HDSM533_SMD)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8EF6E0))
    (comp (ref SW1)
      (value SW_DIP_x01)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib switches) (part SW_DIP_x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8F04AF))
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8F1E48)))
  (libparts
    (libpart (lib conn) (part CONN_01X10)
      (description "Connector, single row, 01x10")
      (footprints
        (fp Pin_Header_Straight_1X10)
        (fp Pin_Header_Angled_1X10)
        (fp Socket_Strip_Straight_1X10)
        (fp Socket_Strip_Angled_1X10))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X10))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Rotary_Encoder)
      (description "Rotary encoder, dual channel, incremental quadrate outputs")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) Rotary_Encoder))
      (pins
        (pin (num 1) (name A) (type input))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type input))))
    (libpart (lib switches) (part SW_DIP_x01)
      (description "1x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x1*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x01))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))))
    (libpart (lib switches) (part SW_DIP_x08)
      (description "8x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x8*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x08))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type input))
        (pin (num 7) (name ~) (type input))
        (pin (num 8) (name ~) (type input))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name ~) (type input))
        (pin (num 15) (name ~) (type input))
        (pin (num 16) (name ~) (type input))))
    (libpart (lib w_connectors) (part Arduino_Nano_Header)
      (fields
        (field (name Reference) J)
        (field (name Value) Arduino_Nano_Header))
      (pins
        (pin (num 1) (name D1/TX) (type passive))
        (pin (num 2) (name D0/RX) (type passive))
        (pin (num 3) (name RESET) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name D2/INT0) (type passive))
        (pin (num 6) (name D3/INT1) (type passive))
        (pin (num 7) (name D4/T0) (type passive))
        (pin (num 8) (name D5/T1) (type passive))
        (pin (num 9) (name D6/AIN0) (type passive))
        (pin (num 10) (name D7/AIN1) (type passive))
        (pin (num 11) (name D8/ICP) (type passive))
        (pin (num 12) (name D9/0C1) (type passive))
        (pin (num 13) (name D10/SS) (type passive))
        (pin (num 14) (name D11/MOSI) (type passive))
        (pin (num 15) (name D12/MISO) (type passive))
        (pin (num 16) (name SCK/D13) (type passive))
        (pin (num 17) (name 3V3) (type passive))
        (pin (num 18) (name AREF) (type passive))
        (pin (num 19) (name A0) (type passive))
        (pin (num 20) (name A1) (type passive))
        (pin (num 21) (name A2) (type passive))
        (pin (num 22) (name A3) (type passive))
        (pin (num 23) (name A4) (type passive))
        (pin (num 24) (name A5) (type passive))
        (pin (num 25) (name A6) (type passive))
        (pin (num 26) (name A7) (type passive))
        (pin (num 27) (name 5V) (type passive))
        (pin (num 28) (name RESET) (type passive))
        (pin (num 29) (name GND) (type passive))
        (pin (num 30) (name VIN) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical switches)
      (uri /usr/share/kicad/library/switches.lib))
    (library (logical w_connectors)
      (uri /home/layoutdev/Desktop/code/documentation_general/Misc_2019/Computer_Switchboard/pcb/symbols/w_connectors.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref SW3) (pin 2))
      (node (ref SW2) (pin 8))
      (node (ref SW2) (pin 9))
      (node (ref SW2) (pin 13))
      (node (ref F1) (pin 2))
      (node (ref SW1) (pin 1)))
    (net (code 2) (name /7seg4)
      (node (ref P1) (pin 4))
      (node (ref R4) (pin 2)))
    (net (code 3) (name "Net-(R9-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref SW2) (pin 7)))
    (net (code 4) (name /7seg2)
      (node (ref R5) (pin 1))
      (node (ref P1) (pin 2)))
    (net (code 5) (name "Net-(R5-Pad2)")
      (node (ref SW2) (pin 3))
      (node (ref R5) (pin 2)))
    (net (code 6) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref SW2) (pin 4)))
    (net (code 7) (name /7seg1)
      (node (ref P1) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 8) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref SW2) (pin 5)))
    (net (code 9) (name "Net-(R8-Pad2)")
      (node (ref SW2) (pin 6))
      (node (ref R8) (pin 2)))
    (net (code 10) (name /7seg5)
      (node (ref R9) (pin 2))
      (node (ref P1) (pin 5)))
    (net (code 11) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref SW2) (pin 15)))
    (net (code 12) (name "Net-(J1-Pad12)")
      (node (ref SW1) (pin 2))
      (node (ref J1) (pin 12)))
    (net (code 13) (name "Net-(F1-Pad1)")
      (node (ref F1) (pin 1))
      (node (ref J1) (pin 4)))
    (net (code 14) (name /PWR3v3+)
      (node (ref J1) (pin 17))
      (node (ref R10) (pin 2))
      (node (ref R11) (pin 2)))
    (net (code 15) (name /7seg6)
      (node (ref R3) (pin 1))
      (node (ref P1) (pin 6)))
    (net (code 16) (name /7seg7)
      (node (ref R2) (pin 2))
      (node (ref P1) (pin 7)))
    (net (code 17) (name "Net-(P1-Pad8)")
      (node (ref P1) (pin 8)))
    (net (code 18) (name /7seg9)
      (node (ref P1) (pin 9))
      (node (ref R7) (pin 2)))
    (net (code 19) (name /7seg10)
      (node (ref R8) (pin 1))
      (node (ref P1) (pin 10)))
    (net (code 20) (name "Net-(J1-Pad18)")
      (node (ref J1) (pin 18)))
    (net (code 21) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 22) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 23) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 24) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25)))
    (net (code 25) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 26) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 27) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 28) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 29) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 30) (name "Net-(J1-Pad29)")
      (node (ref J1) (pin 29)))
    (net (code 31) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 32) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 33) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 34) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 35) (name /74HC14)
      (node (ref SW2) (pin 14))
      (node (ref J1) (pin 7)))
    (net (code 36) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 37) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 38) (name "Net-(J1-Pad30)")
      (node (ref J1) (pin 30)))
    (net (code 39) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 40) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 41) (name /74HC12)
      (node (ref SW2) (pin 12))
      (node (ref J1) (pin 10)))
    (net (code 42) (name /PWR5+)
      (node (ref SW2) (pin 16))
      (node (ref P1) (pin 3))
      (node (ref SW2) (pin 10))
      (node (ref J1) (pin 27)))
    (net (code 43) (name /74HC11)
      (node (ref SW2) (pin 11))
      (node (ref J1) (pin 11)))
    (net (code 44) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref SW2) (pin 1)))
    (net (code 45) (name "Net-(R4-Pad1)")
      (node (ref SW2) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 46) (name /ROT1)
      (node (ref J1) (pin 20))
      (node (ref R10) (pin 1))
      (node (ref SW3) (pin 1)))
    (net (code 47) (name /ROT2)
      (node (ref R11) (pin 1))
      (node (ref SW3) (pin 3))
      (node (ref J1) (pin 21)))
    (net (code 48) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))))