(module stm32vl_discovery_header (layer F.Cu)
  (descr "STM32 Value Line Discovery Header")
  (tags "STM32VL Discovery")
  (fp_text reference STM32VL_Discovery_Header (at 0 1.27) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.2032)))
  )
  (fp_text value Val** (at 0 -1.27) (layer F.SilkS) hide
    (effects (font (size 1.016 0.889) (thickness 0.2032)))
  )
  (fp_line (start 42.3 -21.6) (end -42.3 -21.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -42.3 21.6) (end 42.3 21.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 42.3 21.6) (end 42.3 -21.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -42.3 21.6) (end -42.3 -21.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -32.14 -16.51) (end -32.14 -13.97) (layer F.SilkS) (width 0.381))
  (fp_line (start -32.14 -13.97) (end 38.98 -13.97) (layer F.SilkS) (width 0.381))
  (fp_line (start 38.98 -16.51) (end 38.98 -13.97) (layer F.SilkS) (width 0.381))
  (fp_line (start -32.14 -16.51) (end 38.98 -16.51) (layer F.SilkS) (width 0.381))
  (fp_line (start -37.12 -7.62) (end -37.12 7.62) (layer F.SilkS) (width 0.381))
  (fp_line (start -37.12 7.62) (end -34.58 7.62) (layer F.SilkS) (width 0.381))
  (fp_line (start -34.58 -7.62) (end -34.58 7.62) (layer F.SilkS) (width 0.381))
  (fp_line (start -37.12 -7.62) (end -34.58 -7.62) (layer F.SilkS) (width 0.381))
  (fp_line (start -32.14 13.97) (end 38.98 13.97) (layer F.SilkS) (width 0.381))
  (fp_line (start -32.14 16.51) (end 38.98 16.51) (layer F.SilkS) (width 0.381))
  (fp_line (start 38.98 16.51) (end 38.98 13.97) (layer F.SilkS) (width 0.381))
  (fp_line (start -32.14 16.51) (end -32.14 13.97) (layer F.SilkS) (width 0.381))
  (pad 35 thru_hole rect (at -30.87 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 36 thru_hole oval (at -28.33 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 37 thru_hole oval (at -25.79 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 38 thru_hole oval (at -23.25 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 39 thru_hole oval (at -20.71 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 40 thru_hole oval (at -18.17 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 41 thru_hole oval (at -15.63 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 42 thru_hole oval (at -13.09 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 43 thru_hole oval (at -10.55 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 44 thru_hole oval (at -8.01 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 45 thru_hole oval (at -5.47 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 46 thru_hole oval (at -2.93 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 47 thru_hole oval (at -0.39 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 48 thru_hole oval (at 2.15 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 49 thru_hole oval (at 4.69 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 50 thru_hole oval (at 7.23 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 51 thru_hole oval (at 9.77 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 52 thru_hole oval (at 12.31 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 53 thru_hole oval (at 14.85 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 54 thru_hole oval (at 17.39 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 55 thru_hole oval (at 19.93 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 56 thru_hole oval (at 22.47 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 57 thru_hole oval (at 25.01 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 58 thru_hole oval (at 27.55 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 59 thru_hole oval (at 30.09 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 60 thru_hole oval (at 32.63 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 61 thru_hole oval (at 35.17 15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 62 thru_hole oval (at 37.71 15.24) (size 1.5 2.2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole rect (at 37.71 -15.24) (size 1.5 2.2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 35.17 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole oval (at 32.63 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole oval (at 30.09 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole oval (at 27.55 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole oval (at 25.01 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole oval (at 22.47 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole oval (at 19.93 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole oval (at 17.39 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole oval (at 14.85 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole oval (at 12.31 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole oval (at 9.77 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole oval (at 7.23 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole oval (at 4.69 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole oval (at 2.15 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 16 thru_hole oval (at -0.39 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 17 thru_hole oval (at -2.93 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 18 thru_hole oval (at -5.47 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 19 thru_hole oval (at -8.01 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 20 thru_hole oval (at -10.55 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 21 thru_hole oval (at -13.09 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 22 thru_hole oval (at -15.63 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 23 thru_hole oval (at -18.17 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 24 thru_hole oval (at -20.71 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 25 thru_hole oval (at -23.25 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 26 thru_hole oval (at -25.79 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 27 thru_hole oval (at -28.33 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 28 thru_hole oval (at -30.87 -15.24) (size 1.5 2.2) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 29 thru_hole rect (at -35.85 -6.35) (size 2.2 1.5) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 30 thru_hole oval (at -35.85 -3.81) (size 2.2 1.5) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 31 thru_hole oval (at -35.85 -1.27) (size 2.2 1.5) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 32 thru_hole oval (at -35.85 1.27) (size 2.2 1.5) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 33 thru_hole oval (at -35.85 3.81) (size 2.2 1.5) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (pad 34 thru_hole oval (at -35.85 6.35) (size 2.2 1.5) (drill 0.99822) (layers *.Cu *.Mask F.SilkS))
  (model walter/conn_misc/stm32vl_discovery_header.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
