(module Jack_3.5mm_Ledino_KB3SPRS_Horizontal (layer F.Cu) (tedit 5BC12D58)
  (descr https://www.reichelt.de/index.html?ACTION=7&LA=3&OPEN=0&INDEX=0&FILENAME=C160%252FKB3SPRS.pdf)
  (tags "jack stereo TRS")
  (fp_text reference REF** (at -3.5 2.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_Ledino_KB3SPRS_Horizontal (at 2.3 -12.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 2.7 -4.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.5 2.05) (end 0 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.5 2.05) (end 0.5 2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 1.5) (end -0.5 2.05) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.3 -7.6) (end -9.3 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -9.3 -1.6) (end -5.7 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -9.3 -7.6) (end -5.7 -7.6) (layer F.Fab) (width 0.1))
  (fp_line (start -5.7 -10.7) (end -5.7 0.9) (layer F.Fab) (width 0.1))
  (fp_line (start -5.7 0.9) (end 8.6 0.9) (layer F.Fab) (width 0.1))
  (fp_line (start 8.6 0.9) (end 8.6 -10.7) (layer F.Fab) (width 0.1))
  (fp_line (start 8.6 -10.7) (end -5.7 -10.7) (layer F.Fab) (width 0.1))
  (fp_line (start -9.8 2) (end 9.1 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.1 -11.4) (end -9.8 -11.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.8 -10.8) (end 1.95 -10.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.3 -10.8) (end 8.7 -10.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.7 -10.8) (end 8.7 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.7 1) (end 8.6 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 1) (end 2.25 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 1) (end -5.8 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.8 1) (end -5.8 -10.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.8 -7.7) (end -9.4 -7.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.4 -7.7) (end -9.4 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.4 -1.5) (end -5.8 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.8 -11.4) (end -9.8 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.1 2) (end 9.1 -11.4) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0.1 -1.75) (end 0.4 -1.55) (layer F.Fab) (width 0.12))
  (pad T thru_hole rect (at 0 0) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask))
  (pad TN thru_hole oval (at 7.3 -0.5 90) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask))
  (pad RN thru_hole oval (at 2.9 -7.1) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask))
  (pad R thru_hole oval (at 4.1 -9.8) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask))
  (pad S thru_hole oval (at -3.9 -4.6) (size 2.2 4) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_Ledino_KB3SPRS_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
