(module Jack_3.5mm_Neutrik_NMJ6HCD2_Horizontal (layer F.Cu) (tedit 5BF5E39A)
  (descr "NMJ6HCD2, TRS 1/4in (http://www.neutrik.com/en/audio/plugs-and-jacks/m-series/nmj6hcd2)")
  (tags "NMJ6HCD2 TRS stereo jack connector")
  (fp_text reference REF** (at 6.35 -3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_Neutrik_NMJ6HCD2_Horizontal (at 6.35 19) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 6.35 8.115) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 17.1 -1.55) (end 14.6 -1.55) (layer F.SilkS) (width 0.12))
  (fp_line (start 17.1 0.45) (end 17.1 -1.55) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.7 0.5) (end 11.65 -1.05) (layer F.Fab) (width 0.1))
  (fp_line (start 14 -1.05) (end 12.7 0.5) (layer F.Fab) (width 0.1))
  (fp_line (start -7.05 12.15) (end -3.8 12.15) (layer F.Fab) (width 0.1))
  (fp_line (start -7.05 3.85) (end -7.05 12.15) (layer F.Fab) (width 0.1))
  (fp_line (start -3.8 3.85) (end -7.05 3.85) (layer F.Fab) (width 0.1))
  (fp_line (start 19.6 13.75) (end 16.6 13.75) (layer F.Fab) (width 0.1))
  (fp_line (start 19.6 2.25) (end 19.6 13.75) (layer F.Fab) (width 0.1))
  (fp_line (start 16.6 2.25) (end 19.6 2.25) (layer F.Fab) (width 0.1))
  (fp_line (start -3.8 -1.05) (end 16.6 -1.05) (layer F.Fab) (width 0.1))
  (fp_line (start -3.8 17.05) (end -3.8 -1.05) (layer F.Fab) (width 0.1))
  (fp_line (start 16.6 17.05) (end -3.8 17.05) (layer F.Fab) (width 0.1))
  (fp_line (start 16.6 -1.05) (end 16.6 17.05) (layer F.Fab) (width 0.1))
  (fp_line (start 19.95 -1.75) (end -7.45 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.45 -1.75) (end -7.45 17.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.45 17.95) (end 19.95 17.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start 19.95 -1.75) (end 19.95 17.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.94 12.26) (end -7.16 12.26) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.18 3.75) (end -7.18 12.23) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.94 3.75) (end -7.16 3.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 19.7 2.16) (end 16.7 2.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 19.7 2.16) (end 19.7 13.86) (layer F.SilkS) (width 0.12))
  (fp_line (start 19.7 13.86) (end 16.7 13.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.91 -1.14) (end -3.91 17.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.91 17.15) (end -1.46 17.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.91 -1.14) (end -1.46 -1.14) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.45 -1.15) (end 16.7 -1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.8 -1.15) (end 10.95 -1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.46 -1.14) (end 4.89 -1.14) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.89 17.15) (end 1.46 17.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.24 17.15) (end 7.81 17.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 16.7 17.15) (end 14.15 17.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 16.7 -1.15) (end 16.7 17.15) (layer F.SilkS) (width 0.12))
  (pad RN thru_hole circle (at 6.35 16.23) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad TN thru_hole circle (at 0 16.23) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad SN thru_hole circle (at 12.7 16.23) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad R thru_hole circle (at 6.35 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad T thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (pad S thru_hole rect (at 12.7 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_Neutrik_NMJ6HCD2_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
