(module mkds_1,5-16 (layer F.Cu)
  (descr "16-way 5mm pitch terminal block, Phoenix MKDS series")
  (fp_text reference mkds_1,5/16 (at 0 -6.6) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (fp_text value VAL** (at 0 5.9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (fp_circle (center 37.5 0.1) (end 35.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start 35 4.1) (end 35 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 30 4.1) (end 30 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center 32.5 0.1) (end 30.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center 27.5 0.1) (end 25.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start 25 4.1) (end 25 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 20 4.1) (end 20 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center 22.5 0.1) (end 20.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center 17.5 0.1) (end 15.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start 15 4.1) (end 15 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 10 4.1) (end 10 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center 12.5 0.1) (end 10.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center 7.5 0.1) (end 5.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start 5 4.1) (end 5 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 0 4.1) (end 0 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center 2.5 0.1) (end 0.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center -2.5 0.1) (end -4.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -5 4.1) (end -5 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -10 4.1) (end -10 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center -7.5 0.1) (end -9.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center -12.5 0.1) (end -14.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -15 4.1) (end -15 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -20 4.1) (end -20 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center -17.5 0.1) (end -19.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -25 4.1) (end -25 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center -22.5 0.1) (end -24.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center -27.5 0.1) (end -29.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -30 4.1) (end -30 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -35 4.1) (end -35 4.6) (layer F.SilkS) (width 0.381))
  (fp_circle (center -32.5 0.1) (end -34.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_circle (center -37.5 0.1) (end -35.5 0.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -40 2.6) (end 40 2.6) (layer F.SilkS) (width 0.381))
  (fp_line (start -40 -2.3) (end 40 -2.3) (layer F.SilkS) (width 0.381))
  (fp_line (start -40 4.1) (end 40 4.1) (layer F.SilkS) (width 0.381))
  (fp_line (start -40 4.6) (end 40 4.6) (layer F.SilkS) (width 0.381))
  (fp_line (start 40 4.6) (end 40 -5.2) (layer F.SilkS) (width 0.381))
  (fp_line (start 40 -5.2) (end -40 -5.2) (layer F.SilkS) (width 0.381))
  (fp_line (start -40 -5.2) (end -40 4.6) (layer F.SilkS) (width 0.381))
  (pad 16 thru_hole circle (at 37.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole circle (at 32.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole circle (at 27.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole circle (at 22.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole circle (at 17.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole circle (at 12.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at 7.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole circle (at 2.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at -2.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at -7.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at -12.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -17.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at -22.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at -27.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -37.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -32.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
  (model walter/conn_mkds/mkds_1,5-16.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
