(module Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5C06A514)
  (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
  (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
  (attr smd)
  (fp_text reference REF** (at 0.05 -5.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_PJ320D_Horizontal (at -0.025 6.35) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at -1.195 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.05 -3.1) (end 3.05 -4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.6 -3.1) (end 4.6 -4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.575 2.9) (end -6.225 2.9) (layer F.Fab) (width 0.1))
  (fp_line (start -6.225 2.9) (end -6.225 2.3) (layer F.Fab) (width 0.1))
  (fp_line (start -6.225 2.3) (end -8.225 2.3) (layer F.Fab) (width 0.1))
  (fp_line (start -8.225 2.3) (end -8.225 -2.3) (layer F.Fab) (width 0.1))
  (fp_line (start -8.225 -2.3) (end -6.225 -2.3) (layer F.Fab) (width 0.1))
  (fp_line (start -6.225 -2.3) (end -6.225 -2.9) (layer F.Fab) (width 0.1))
  (fp_line (start -6.225 -2.9) (end 5.575 -2.9) (layer F.Fab) (width 0.1))
  (fp_line (start 5.575 -2.9) (end 5.575 2.9) (layer F.Fab) (width 0.1))
  (fp_line (start 4.15 3.1) (end -6.375 3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.6 -3.1) (end 5.725 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.65 -3.1) (end 3.05 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.35 -3.1) (end -1 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.375 -3.1) (end -4 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.07 5) (end 6.07 -5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.73 5) (end -8.73 -5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.725 3.1) (end 5.725 -3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.73 5) (end 6.07 5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -8.73 -5) (end 6.07 -5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.375 -3.1) (end -6.375 -2.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.375 2.5) (end -6.375 3.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.375 -2.5) (end -8.375 2.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.375 -2.5) (end -8.375 -2.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.375 2.5) (end -8.375 2.5) (layer F.SilkS) (width 0.12))
  (fp_circle (center 3.9 -2.35) (end 3.95 -2.1) (layer F.Fab) (width 0.12))
  (pad S smd rect (at 4.925 3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
  (pad T smd rect (at 3.825 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
  (pad R1 smd rect (at -0.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
  (pad R2 smd rect (at -3.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at -4.775 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.225 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
