(module Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles (layer F.Cu) (tedit 5C2B6BB2)
  (descr "TRS 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
  (tags "WQP-PJ398SM WQP-PJ301M-12 TRS 3.5mm mono vertical jack thonkiconn qingpu")
  (fp_text reference REF** (at -4.03 1.08 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles (at 0 5 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user KEEPOUT (at 0 6.48) (layer Cmts.User)
    (effects (font (size 0.4 0.4) (thickness 0.051)))
  )
  (fp_line (start -5 12.98) (end -5 -1.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.5 12.48) (end -4.5 2.08) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 8 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.5 1.98) (end -4.5 12.48) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.5 1.98) (end 4.5 12.48) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 6.48) (end 1.5 6.48) (layer Dwgs.User) (width 0.12))
  (fp_line (start 0.09 7.96) (end 1.48 6.57) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.58 7.83) (end 1.36 5.89) (layer Dwgs.User) (width 0.12))
  (fp_line (start -1.07 7.49) (end 1.01 5.41) (layer Dwgs.User) (width 0.12))
  (fp_line (start -1.42 6.875) (end 0.4 5.06) (layer Dwgs.User) (width 0.12))
  (fp_line (start -1.41 6.02) (end -0.46 5.07) (layer Dwgs.User) (width 0.12))
  (fp_line (start 4.5 12.48) (end 0.5 12.48) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.5 12.48) (end -4.5 12.48) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.5 1.98) (end 0.35 1.98) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.35 1.98) (end -4.5 1.98) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 6.48) (end 1.8 6.48) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.06 -1) (end -1.06 -0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.06 -1) (end -0.2 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.5 12.48) (end 4.5 2.08) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 12.48) (end -4.5 12.48) (layer F.Fab) (width 0.1))
  (fp_line (start 5 12.98) (end 5 -1.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5 12.98) (end -5 12.98) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5 -1.42) (end -5 -1.42) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.5 2.03) (end -4.5 2.03) (layer F.Fab) (width 0.1))
  (fp_circle (center 0 6.48) (end 1.8 6.48) (layer F.Fab) (width 0.1))
  (fp_line (start 0 0) (end 0 2.03) (layer F.Fab) (width 0.1))
  (pad TN thru_hole circle (at 0 3.1 180) (size 2.13 2.13) (drill 1.42) (layers *.Cu *.Mask))
  (pad S thru_hole rect (at 0 0 180) (size 1.93 1.83) (drill 1.22) (layers *.Cu *.Mask))
  (pad T thru_hole circle (at 0 11.4 180) (size 2.13 2.13) (drill 1.43) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
