(module Jack_3.5mm_PJ320E_Horizontal (layer F.Cu) (tedit 5BC12BA2)
  (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320E-177.html)")
  (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
  (fp_text reference REF** (at 2.54 -13.97) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_PJ320E_Horizontal (at 2.54 5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 2.54 -13.97) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.7 0.5) (end -1.2 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 -0.5) (end -1.7 0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.2 0) (end -1.7 -0.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.7 2) (end -0.8 2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 2) (end -0.8 -9.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.8 -9.2) (end -0.5 -9.2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -9.2) (end -0.5 -12) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -12) (end 5.1 -12) (layer F.Fab) (width 0.1))
  (fp_line (start 5.1 -12) (end 5.1 -9.2) (layer F.Fab) (width 0.1))
  (fp_line (start 5.1 -9.2) (end 6.3 -9.2) (layer F.Fab) (width 0.1))
  (fp_line (start 6.3 -9.2) (end 6.3 2) (layer F.Fab) (width 0.1))
  (fp_line (start 6.3 2) (end 5.3 2) (layer F.Fab) (width 0.1))
  (fp_line (start -0.9 -9.3) (end -0.9 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.9 2.1) (end 3.7 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.4 2.1) (end 5.3 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 3) (end 6.8 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.3 -12.5) (end -1.3 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.8 -12.5) (end 6.8 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.2 -9.3) (end 6.4 -9.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.9 -9.3) (end -0.6 -9.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.2 -12.1) (end -0.6 -12.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.4 -9.3) (end 6.4 2.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.2 -9.3) (end 5.2 -12.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.6 -9.3) (end -0.6 -12.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 -12.5) (end 6.8 -12.5) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0.9 0) (end 1.2 0.15) (layer F.Fab) (width 0.12))
  (pad "" thru_hole oval (at 5.5 -7 270) (size 2 1.4) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
  (pad S thru_hole oval (at 4.5 1.5 270) (size 2 1.4) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
  (pad T thru_hole rect (at 0 0 270) (size 2 1.4) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
  (pad R1 thru_hole oval (at 0 -4 270) (size 2 1.4) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
  (pad R2 thru_hole oval (at 0 -7 270) (size 2 1.4) (drill oval 1.2 0.6) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.3 -5.7 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.3 1.3 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320E_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
