(module Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal (layer F.Cu) (tedit 5C635470)
  (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
  (tags "3.5mm audio cui horizontal jack stereo")
  (attr smd)
  (fp_text reference REF** (at 0 -9.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal (at 0 13) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3 -6) (end 3 8.5) (layer F.Fab) (width 0.1))
  (fp_line (start 3 8.5) (end -3 8.5) (layer F.Fab) (width 0.1))
  (fp_line (start -3 8.5) (end -3 -6) (layer F.Fab) (width 0.1))
  (fp_line (start -3 -6) (end -2.5 -6) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -6) (end -2.5 -8.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 -8.5) (end 2.5 -8.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -8.5) (end 2.5 -6) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -6) (end 3 -6) (layer F.Fab) (width 0.1))
  (fp_line (start 5.6 -9) (end 5.6 11.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.6 11.6) (end -5.6 11.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.6 11.6) (end -5.6 -9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.6 -9) (end 5.6 -9) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.1 -4.9) (end -3.1 -6.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -6.1) (end -2.6 -6.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.6 -6.1) (end -2.6 -8.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.6 -8.6) (end 2.6 -8.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.6 -8.6) (end 2.6 -6.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.6 -6.1) (end 3.1 -6.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.1 -6.1) (end 3.1 -2.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.1 -0.3) (end 3.1 8.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.1 8.6) (end 2.35 8.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.85 8.6) (end -3.1 8.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 8.6) (end -3.1 7.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 4.2) (end -3.1 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -4.9) (end -5.1 -4.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.1 -2.3) (end -5.1 -2.3) (layer F.SilkS) (width 0.12))
  (pad R smd rect (at 3.7 -1.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask))
  (pad S smd rect (at -3.7 -3.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask))
  (pad TN smd rect (at 0.75 9.8) (size 2.8 2.6) (layers F.Cu F.Paste F.Mask))
  (pad T smd rect (at -3.7 5.8) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 0 -2.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ-3524-SMT_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
