EESchema Schematic File Version 4
LIBS:batterystation-cache
EELAYER 26 0
EELAYER END
$Descr A4 11693 8268
encoding utf-8
Sheet 4 9
Title ""
Date ""
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndDescr
$Comp
L conn:CONN_02X05 P15
U 1 1 5BF754F5
P 3050 3600
F 0 "P15" H 3050 4015 50  0000 C CNN
F 1 "ENCBREAKOUT2x5" H 3050 3924 50  0000 C CNN
F 2 "Pin_Headers:Pin_Header_Straight_2x05" H 3050 2400 50  0001 C CNN
F 3 "" H 3050 2400 50  0000 C CNN
	1    3050 3600
	1    0    0    -1  
$EndComp
$Comp
L conn:CONN_02X06 P16
U 1 1 5BF7553B
P 4750 3650
F 0 "P16" H 4750 4115 50  0000 C CNN
F 1 "ENCBREAKOUT2x6" H 4750 4024 50  0000 C CNN
F 2 "Pin_Headers:Pin_Header_Straight_2x06" H 4750 2450 50  0001 C CNN
F 3 "" H 4750 2450 50  0000 C CNN
	1    4750 3650
	1    0    0    -1  
$EndComp
Text Label 2800 3600 2    50   ~ 0
SCK
Text Label 2800 3500 2    50   ~ 0
MISO
Text Label 2800 3400 2    50   ~ 0
INT
Text Label 3300 3400 0    50   ~ 0
CLKOUT
Text Label 3300 3500 0    50   ~ 0
WOL
Text Label 3300 3600 0    50   ~ 0
MOSI
Text Label 3300 3700 0    50   ~ 0
CS
Text Label 3300 3800 0    50   ~ 0
VCC_Branch
Text Label 4500 3900 2    50   ~ 0
VCC_Branch
Text Label 4500 3800 2    50   ~ 0
INT
Text Label 4500 3700 2    50   ~ 0
MISO
Text Label 4500 3600 2    50   ~ 0
SCK
Text Label 4500 3400 2    50   ~ 0
Q3
Text Label 5000 3800 0    50   ~ 0
CLKOUT
Text Label 5000 3700 0    50   ~ 0
WOL
Text Label 5000 3600 0    50   ~ 0
MOSI
Text Label 5000 3500 0    50   ~ 0
CS
$Comp
L power:GND #PWR0116
U 1 1 5BF757EE
P 5400 3400
F 0 "#PWR0116" H 5400 3150 50  0001 C CNN
F 1 "GND" H 5405 3227 50  0000 C CNN
F 2 "" H 5400 3400 50  0000 C CNN
F 3 "" H 5400 3400 50  0000 C CNN
	1    5400 3400
	-1   0    0    -1  
$EndComp
$Comp
L power:GND #PWR0117
U 1 1 5BF75816
P 5000 3900
F 0 "#PWR0117" H 5000 3650 50  0001 C CNN
F 1 "GND" H 5005 3727 50  0000 C CNN
F 2 "" H 5000 3900 50  0000 C CNN
F 3 "" H 5000 3900 50  0000 C CNN
	1    5000 3900
	-1   0    0    -1  
$EndComp
$Comp
L power:GND #PWR0118
U 1 1 5BF7585C
P 2800 3800
F 0 "#PWR0118" H 2800 3550 50  0001 C CNN
F 1 "GND" H 2805 3627 50  0000 C CNN
F 2 "" H 2800 3800 50  0000 C CNN
F 3 "" H 2800 3800 50  0000 C CNN
	1    2800 3800
	-1   0    0    -1  
$EndComp
$Comp
L conn:CONN_01X02 P13
U 1 1 5BF75EA3
P 2650 4400
F 0 "P13" H 2728 4441 50  0000 L CNN
F 1 "PWRSELECT3v3" H 2728 4350 50  0000 L CNN
F 2 "Pin_Headers:Pin_Header_Straight_1x02" H 2650 4400 50  0001 C CNN
F 3 "" H 2650 4400 50  0000 C CNN
	1    2650 4400
	1    0    0    -1  
$EndComp
$Comp
L conn:CONN_01X02 P14
U 1 1 5BF75ED4
P 2650 4900
F 0 "P14" H 2728 4941 50  0000 L CNN
F 1 "PWRSELECT5V" H 2728 4850 50  0000 L CNN
F 2 "Pin_Headers:Pin_Header_Straight_1x02" H 2650 4900 50  0001 C CNN
F 3 "" H 2650 4900 50  0000 C CNN
	1    2650 4900
	1    0    0    -1  
$EndComp
$Comp
L power:+3.3V #PWR0119
U 1 1 5BF75F40
P 2450 4350
F 0 "#PWR0119" H 2450 4200 50  0001 C CNN
F 1 "+3.3V" H 2465 4523 50  0000 C CNN
F 2 "" H 2450 4350 50  0000 C CNN
F 3 "" H 2450 4350 50  0000 C CNN
	1    2450 4350
	1    0    0    -1  
$EndComp
$Comp
L power:+5V #PWR0120
U 1 1 5BF75F75
P 2450 4850
F 0 "#PWR0120" H 2450 4700 50  0001 C CNN
F 1 "+5V" H 2465 5023 50  0000 C CNN
F 2 "" H 2450 4850 50  0000 C CNN
F 3 "" H 2450 4850 50  0000 C CNN
	1    2450 4850
	1    0    0    -1  
$EndComp
Text Label 2450 4950 2    50   ~ 0
VCC_Branch
Text Label 2450 4450 2    50   ~ 0
VCC_Branch
Text Notes 4050 5000 0    50   ~ 0
Jumpers. Most ENC28J60 Modules\n are 3.3v, but some have vregs, or\nvdividers. There are two possible\npinouts, from my collection that\nI see. 2x5 or 2x6. On my 2x6 module\nVCC is labeled as 5V. On the 2x5 it is\nunlabeled.
Wire Notes Line
	3950 5100 5650 5100
Wire Notes Line
	5650 5100 5650 4400
Wire Notes Line
	5650 4400 3950 4400
Wire Notes Line
	3950 4400 3950 5100
Text Notes 2900 1750 0    150  ~ 0
ENC28J60 Arduino Module
Text Label 2800 3700 2    50   ~ 0
RSTENC
Text Label 4500 3500 2    50   ~ 0
RSTENC
Wire Wire Line
	5000 3400 5400 3400
Text Notes 950  2250 0    50   ~ 0
ENC28J60 modules\nare loaded facing\ndown on the top \nlayer of the PCB.\nThis is good to double\ncheck. The VCC here is \non the inside of the board.\nCompare to existing PCBs.
Wire Notes Line
	850  2350 2100 2350
Wire Notes Line
	2100 2350 2100 1550
Wire Notes Line
	2100 1550 850  1550
Wire Notes Line
	850  1550 850  2350
Text Notes 2650 2700 0    50   ~ 0
HOW TO DOUBLE CHECK PINOUTS\nPick one pin, i.e. pin 10 which is VCC on this board.\n(for the 5x2 connector)\nLook at layout. make sure its in the right place,\nso that the enc will be loaded correctly.
Wire Notes Line
	2550 2850 4800 2850
Wire Notes Line
	4800 2850 4800 2200
Wire Notes Line
	4800 2200 2550 2200
Wire Notes Line
	2550 2200 2550 2850
Text HLabel 2400 3500 0    50   Input ~ 0
MISO
Wire Wire Line
	2400 3500 2800 3500
Text HLabel 2400 3600 0    50   Input ~ 0
SCK
Wire Wire Line
	2400 3600 2800 3600
Text HLabel 3650 3600 2    50   Input ~ 0
MOSI
Text HLabel 3650 3700 2    50   Input ~ 0
CS
Text HLabel 5600 3600 2    50   Input ~ 0
MOSI
Text HLabel 5600 3500 2    50   Input ~ 0
CS
Text HLabel 4200 3700 0    50   Input ~ 0
MISO
Text HLabel 4200 3600 0    50   Input ~ 0
SCK
Wire Wire Line
	3650 3600 3300 3600
Wire Wire Line
	3650 3700 3300 3700
Wire Wire Line
	4200 3600 4500 3600
Wire Wire Line
	4200 3700 4500 3700
Wire Wire Line
	5000 3600 5600 3600
Wire Wire Line
	5600 3500 5000 3500
$EndSCHEMATC
