(module Potentiometer_ACP_CA14-VSMD_Vertical_Hole (layer F.Cu) (tedit 5A3D7171)
  (descr "Potentiometer, vertical, shaft hole, ACP CA14-VSMD, http://www.acptechnologies.com/wp-content/uploads/2017/10/03-ACP-CA14-CE14.pdf")
  (tags "Potentiometer vertical hole ACP CA14-VSMD")
  (attr smd)
  (fp_text reference REF** (at 0 -8.25) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Potentiometer_ACP_CA14-VSMD_Vertical_Hole (at 0 8.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -7.2 -7) (end -7.2 7) (layer F.Fab) (width 0.1))
  (fp_line (start -7.2 7) (end 6.8 7) (layer F.Fab) (width 0.1))
  (fp_line (start 6.8 7) (end 6.8 -7) (layer F.Fab) (width 0.1))
  (fp_line (start 6.8 -7) (end -7.2 -7) (layer F.Fab) (width 0.1))
  (fp_line (start -7.32 -7.12) (end 6.92 -7.12) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.32 7.12) (end 6.92 7.12) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.32 -7.12) (end -7.32 -6.741) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.32 -3.259) (end -7.32 3.26) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.32 6.74) (end -7.32 7.12) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.92 -7.12) (end 6.92 -1.74) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.92 1.74) (end 6.92 7.12) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.75 -7.25) (end -7.75 7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -7.75 7.25) (end 7.75 7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.75 7.25) (end 7.75 -7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.75 -7.25) (end -7.75 -7.25) (layer F.CrtYd) (width 0.05))
  (pad 3 smd rect (at -6.5 -5) (size 3 3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 6.5 0) (size 3 3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -6.5 5) (size 3 3) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at -0.2 0) (size 7 7) (drill 7) (layers *.Cu *.Mask))
  (fp_text user %R (at -6.2 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_ACP_CA14-VSMD_Vertical_Hole.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)