(module Potentiometer_Bourns_PRS11S_Vertical (layer F.Cu) (tedit 5A3C1644)
  (descr "Potentiometer, vertical, Bourns PRS11S, http://www.bourns.com/docs/Product-Datasheets/PRS11S.pdf")
  (tags "Potentiometer vertical Bourns PRS11S")
  (attr smd)
  (fp_text reference REF** (at 0 -7.65) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Potentiometer_Bourns_PRS11S_Vertical (at 0 7.65) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0.25 0) (end 3.25 0) (layer F.Fab) (width 0.1))
  (fp_line (start -6.25 -5.85) (end -6.25 5.85) (layer F.Fab) (width 0.1))
  (fp_line (start -6.25 5.85) (end 6.75 5.85) (layer F.Fab) (width 0.1))
  (fp_line (start 6.75 5.85) (end 6.75 -5.85) (layer F.Fab) (width 0.1))
  (fp_line (start 6.75 -5.85) (end -6.25 -5.85) (layer F.Fab) (width 0.1))
  (fp_line (start -6.37 -5.97) (end -0.723 -5.97) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.224 -5.97) (end 6.87 -5.97) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.37 5.97) (end -0.723 5.97) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.224 5.97) (end 6.87 5.97) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.37 3.9) (end -6.37 5.97) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.87 3.9) (end 6.87 5.97) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -6.65) (end -10.5 6.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10.5 6.65) (end 10.5 6.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.5 6.65) (end 10.5 -6.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.5 -6.65) (end -10.5 -6.65) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at -5.25 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.37 -5.97) (end -6.37 -3.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.87 -5.97) (end 6.87 -3.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.87 -1.1) (end 6.87 1.1) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at -8.25 -2.5) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -8.25 0) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -8.25 2.5) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 8.25 -2.5) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 8.25 2.5) (size 4 2) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 0.25 -5.65) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0.25 5.65) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_PRS11S_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
