(module TO-247-5_Horizontal_TabUp (layer F.Cu) (tedit 5AC8BA0D)
  (descr "TO-247-5, Horizontal, RM 2.54mm, see http://ww1.microchip.com/downloads/en/DeviceDoc/20005685A.pdf")
  (tags "TO-247-5 Horizontal RM 2.54mm")
  (fp_text reference REF** (at 5.08 27.15) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TO-247-5_Horizontal_TabUp (at 5.08 -3.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 5.08 19.86) (end 6.885 19.86) (layer F.Fab) (width 0.1))
  (fp_line (start -2.87 5.08) (end -2.87 26.03) (layer F.Fab) (width 0.1))
  (fp_line (start -2.87 26.03) (end 13.03 26.03) (layer F.Fab) (width 0.1))
  (fp_line (start 13.03 26.03) (end 13.03 5.08) (layer F.Fab) (width 0.1))
  (fp_line (start 13.03 5.08) (end -2.87 5.08) (layer F.Fab) (width 0.1))
  (fp_line (start 0 5.08) (end 0 0) (layer F.Fab) (width 0.1))
  (fp_line (start 2.54 5.08) (end 2.54 0) (layer F.Fab) (width 0.1))
  (fp_line (start 5.08 5.08) (end 5.08 0) (layer F.Fab) (width 0.1))
  (fp_line (start 7.62 5.08) (end 7.62 0) (layer F.Fab) (width 0.1))
  (fp_line (start 10.16 5.08) (end 10.16 0) (layer F.Fab) (width 0.1))
  (fp_line (start -2.99 4.96) (end 13.15 4.96) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.99 26.15) (end 13.15 26.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.99 4.96) (end -2.99 26.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.15 4.96) (end 13.15 26.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 2.4) (end 0 4.96) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.54 2.4) (end 2.54 4.96) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.08 2.4) (end 5.08 4.96) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.62 2.4) (end 7.62 4.96) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.16 2.4) (end 10.16 4.96) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.12 -2.5) (end -3.12 26.28) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.12 26.28) (end 13.28 26.28) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.28 26.28) (end 13.28 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.28 -2.5) (end -3.12 -2.5) (layer F.CrtYd) (width 0.05))
  (pad "" np_thru_hole oval (at 5.08 19.86) (size 3.6 3.6) (drill 3.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2.54 0) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 5.08 0) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 7.62 0) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 10.16 0) (size 1.905 4.5) (drill 1.5) (layers *.Cu *.Mask))
  (fp_text user %R (at 5.08 27.15) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-247-5_Horizontal_TabUp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)