(module TO-92_Inline_Horizontal1 (layer F.Cu) (tedit 5A27990F)
  (descr "TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
  (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
  (fp_text reference REF** (at 1.27 -1.78) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TO-92_Inline_Horizontal1 (at 1.27 10.03) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 1.27 6.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.54 3.94) (end 2.54 1.02) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 3.94) (end 1.27 1.02) (layer F.Fab) (width 0.1))
  (fp_line (start 0 3.94) (end 0 1.02) (layer F.Fab) (width 0.1))
  (fp_line (start -1.02 8.89) (end -1.02 3.94) (layer F.Fab) (width 0.1))
  (fp_line (start -1.02 3.94) (end 3.56 3.94) (layer F.Fab) (width 0.1))
  (fp_line (start 3.56 3.94) (end 3.56 8.89) (layer F.Fab) (width 0.1))
  (fp_line (start 3.56 8.89) (end -1.02 8.89) (layer F.Fab) (width 0.1))
  (fp_line (start 0 1.02) (end 0 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 1.02) (end 1.27 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.54 1.02) (end 2.54 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.13 3.81) (end 3.67 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.67 3.81) (end 3.67 9) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.67 9) (end -1.13 9) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.13 9) (end -1.13 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 -1) (end 3.81 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.27 -1) (end -1.27 9.14) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.81 9.14) (end 3.81 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.81 9.14) (end -1.27 9.14) (layer F.CrtYd) (width 0.05))
  (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Horizontal1.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
