(module SOD-70_P2.54mm (layer F.Cu) (tedit 5AE2F977)
  (descr "Plastic near cylindrical package Sod-70 see: https://www.nxp.com/docs/en/data-sheet/KTY81_SER.pdf  [StepUp generated footprint]")
  (tags Sod-70)
  (fp_text reference REF** (at 1.5 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SOD-70_P2.54mm (at 1 3.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 1.5 -3.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_arc (start 1.27 0) (end 2.969265 1.55) (angle -264.7395971) (layer F.Fab) (width 0.1))
  (fp_line (start 2.969265 1.55) (end -0.429265 1.55) (layer F.Fab) (width 0.1))
  (fp_arc (start 1.27 0) (end 3.017141 1.66) (angle -267.0698621) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.017141 1.66) (end -0.477141 1.66) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.21 -2.55) (end 2.33 -2.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.82 -1.06) (end 3.82 1.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.08 1.8) (end -0.54 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.28 1.06) (end -1.28 -1.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.21 -2.55) (end -1.28 -1.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.33 -2.55) (end 3.82 -1.06) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.28 1.06) (end -0.54 1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.08 1.8) (end 3.82 1.06) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2.54 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/SOD-70_P2.54mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
