MDF Database:  version 1.0
MDF_INFO | counta | XC9572XL-5-VQ44
MACROCELL | 2 | 1 | waitnow<0>
ATTRIBUTES | 4588322 | 0
OUTPUTMC | 27 | 2 | 1 | 0 | 16 | 0 | 9 | 0 | 12 | 0 | 11 | 2 | 3 | 0 | 6 | 3 | 15 | 0 | 15 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 11 | 2 | 12 | 2 | 11 | 2 | 5 | 1 | 0 | 2 | 17 | 3 | 1 | 3 | 13 | 3 | 12 | 0 | 8 | 2 | 0 | 2 | 14 | 3 | 0
INPUTS | 12 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | HZIN  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | XSTALIN
INPUTMC | 10 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 0
EQ | 11 | 
   LED<7>.T = LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN
	# !LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & uartctr<0> & uartctr<1> & 
	uartctr<2> & uartctr<3> & uartctr<4>
	# !LED<7> & LED<6> & !alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4> & !HZIN;
   LED<7>.CLK = XSTALIN;
    waitnow<0>.EXP  =  LED<7> & !LED<6> & !resetclk<0> & uartskip<0> & 
	!HZIN

MACROCELL | 0 | 16 | uartnow<0>
ATTRIBUTES | 4588322 | 0
OUTPUTMC | 41 | 2 | 1 | 0 | 16 | 0 | 10 | 0 | 13 | 0 | 14 | 0 | 5 | 0 | 7 | 0 | 8 | 1 | 0 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 12 | 2 | 13 | 2 | 12 | 2 | 5 | 1 | 17 | 3 | 0 | 3 | 17 | 3 | 14 | 3 | 13 | 2 | 17 | 2 | 16 | 2 | 15 | 3 | 16 | 2 | 4 | 0 | 4 | 0 | 6 | 0 | 9 | 0 | 11 | 0 | 12 | 0 | 15 | 2 | 0 | 2 | 3 | 2 | 11 | 2 | 14 | 3 | 1 | 3 | 11 | 3 | 15
INPUTS | 12 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | HZIN  | XSTALIN
INPUTMC | 10 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTP | 2 | 65 | 63
EQ | 12 | 
   LED<6>.T = !LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & !uartskip<0>
	# LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>
	# LED<6> & alreadystoredcnt<0> & !resetclk<0> & 
	uartskip<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>
	# LED<6> & !alreadystoredcnt<0> & !resetclk<0> & 
	uartctr<0> & uartctr<1> & uartctr<2> & uartctr<3> & 
	uartctr<4> & !HZIN;
   LED<6>.CLK = XSTALIN;

MACROCELL | 0 | 10 | storecounta<10>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 3 | 0 | 10 | 0 | 8 | 0 | 11
INPUTS | 8 | LED<6>  | LED<4>  | alreadystoredcnt<0>  | HZIN  | clkcounta<7>  | LED<3>  | EXP9_.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 0 | 13 | 2 | 0 | 1 | 9 | 0 | 10 | 0 | 11
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 0 | 11
EQ | 9 | 
   LED<3>.D = LED<6> & LED<4> & alreadystoredcnt<0>
	# LED<6> & LED<4> & !HZIN
	# !LED<6> & LED<3> & alreadystoredcnt<0>
	# !alreadystoredcnt<0> & HZIN & clkcounta<7>
;Imported pterms FB1_12
	# !LED<6> & LED<3> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   LED<3>.CLK = XSTALIN;

MACROCELL | 0 | 13 | storecounta<11>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 3 | 0 | 10 | 0 | 13 | 0 | 12
INPUTS | 8 | LED<6>  | LED<5>  | alreadystoredcnt<0>  | HZIN  | clkcounta<8>  | LED<4>  | EXP10_.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 0 | 14 | 2 | 0 | 1 | 8 | 0 | 13 | 0 | 12
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 0 | 12
EQ | 9 | 
   LED<4>.D = LED<6> & LED<5> & alreadystoredcnt<0>
	# LED<6> & LED<5> & !HZIN
	# !LED<6> & LED<4> & alreadystoredcnt<0>
	# !alreadystoredcnt<0> & HZIN & clkcounta<8>
;Imported pterms FB1_13
	# !LED<6> & LED<4> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   LED<4>.CLK = XSTALIN;

MACROCELL | 0 | 14 | storecounta<12>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 3 | 0 | 13 | 0 | 14 | 0 | 15
INPUTS | 8 | LED<6>  | alreadystoredcnt<0>  | storecounta<13>  | HZIN  | clkcounta<9>  | LED<5>  | EXP11_.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 2 | 0 | 1 | 17 | 1 | 7 | 0 | 14 | 0 | 15
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 0 | 15
EQ | 9 | 
   LED<5>.D = LED<6> & alreadystoredcnt<0> & storecounta<13>
	# LED<6> & storecounta<13> & !HZIN
	# !LED<6> & LED<5> & alreadystoredcnt<0>
	# !alreadystoredcnt<0> & HZIN & clkcounta<9>
;Imported pterms FB1_16
	# !LED<6> & LED<5> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   LED<5>.CLK = XSTALIN;

MACROCELL | 0 | 5 | storecounta<7>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 3 | 0 | 5 | 3 | 16 | 0 | 4
INPUTS | 9 | LED<6>  | LED<1>  | alreadystoredcnt<0>  | HZIN  | clkcounta<4>  | LED<0>  | EXP6_.EXP  | EXP7_.EXP  | XSTALIN
INPUTMC | 7 | 0 | 16 | 0 | 7 | 2 | 0 | 1 | 12 | 0 | 5 | 0 | 4 | 0 | 6
INPUTP | 2 | 65 | 63
IMPORTS | 2 | 0 | 4 | 0 | 6
EQ | 10 | 
   LED<0>.D = LED<6> & LED<1> & alreadystoredcnt<0>
	# LED<6> & LED<1> & !HZIN
	# !LED<6> & LED<0> & alreadystoredcnt<0>
	# !alreadystoredcnt<0> & HZIN & clkcounta<4>
;Imported pterms FB1_5
	# !LED<6> & LED<0> & !HZIN
;Imported pterms FB1_7
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   LED<0>.CLK = XSTALIN;

MACROCELL | 0 | 7 | storecounta<8>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 3 | 0 | 5 | 0 | 7 | 0 | 8
INPUTS | 8 | LED<6>  | LED<2>  | alreadystoredcnt<0>  | HZIN  | clkcounta<5>  | LED<1>  | storecounta<9>.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 0 | 8 | 2 | 0 | 1 | 11 | 0 | 7 | 0 | 8
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 0 | 8
EQ | 9 | 
   LED<1>.D = LED<6> & LED<2> & alreadystoredcnt<0>
	# LED<6> & LED<2> & !HZIN
	# !LED<6> & LED<1> & alreadystoredcnt<0>
	# !alreadystoredcnt<0> & HZIN & clkcounta<5>
;Imported pterms FB1_9
	# !LED<6> & LED<1> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   LED<1>.CLK = XSTALIN;

MACROCELL | 0 | 8 | storecounta<9>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 2 | 0 | 7 | 0 | 9
INPUTS | 10 | LED<6>  | LED<3>  | alreadystoredcnt<0>  | HZIN  | LED<1>  | LED<7>  | resetclk<0>  | uartskip<0>  | EXP8_.EXP  | XSTALIN
INPUTMC | 8 | 0 | 16 | 0 | 10 | 2 | 0 | 0 | 7 | 2 | 1 | 2 | 14 | 2 | 2 | 0 | 9
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 0 | 7
IMPORTS | 1 | 0 | 9
EQ | 12 | 
   LED<2>.D = LED<6> & LED<3> & alreadystoredcnt<0>
	# LED<6> & LED<3> & !HZIN
;Imported pterms FB1_10
	# !LED<6> & LED<2> & alreadystoredcnt<0>
	# !LED<6> & LED<2> & !HZIN
	# !alreadystoredcnt<0> & HZIN & clkcounta<6>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   LED<2>.CLK = XSTALIN;
    storecounta<9>.EXP  =  !LED<6> & LED<1> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 2 | 0 | alreadystoredcnt<0>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 51 | 2 | 1 | 0 | 16 | 0 | 10 | 0 | 13 | 0 | 14 | 0 | 5 | 0 | 7 | 0 | 8 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 11 | 2 | 13 | 2 | 12 | 2 | 5 | 1 | 17 | 3 | 0 | 3 | 17 | 3 | 14 | 3 | 13 | 2 | 17 | 2 | 16 | 2 | 15 | 3 | 16 | 2 | 4 | 2 | 3 | 1 | 16 | 1 | 15 | 1 | 0 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14 | 0 | 6 | 0 | 9 | 0 | 11 | 0 | 12 | 0 | 15 | 2 | 11 | 3 | 1 | 3 | 12 | 3 | 15
INPUTS | 9 | alreadystoredcnt<0>  | HZIN  | LED<6>  | storecounta<3>  | LED<7>  | resetclk<0>  | XSTALIN  | uartskip<0>  | waitnow<0>.EXP
INPUTMC | 7 | 2 | 0 | 0 | 16 | 2 | 17 | 2 | 1 | 2 | 14 | 2 | 2 | 2 | 1
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 17
IMPORTS | 1 | 2 | 1
EQ | 9 | 
   !alreadystoredcnt<0>.D = !alreadystoredcnt<0> & !HZIN
;Imported pterms FB3_2
	# LED<7> & !LED<6> & !resetclk<0> & uartskip<0> & 
	!HZIN;
   alreadystoredcnt<0>.CLK = XSTALIN;
    alreadystoredcnt<0>.EXP  =  !LED<6> & alreadystoredcnt<0> & storecounta<3>
	# !LED<6> & storecounta<3> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 2 | 14 | resetclk<0>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 42 | 2 | 1 | 0 | 16 | 0 | 9 | 0 | 12 | 0 | 11 | 1 | 14 | 0 | 6 | 1 | 7 | 0 | 15 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 12 | 2 | 13 | 2 | 12 | 2 | 5 | 1 | 0 | 2 | 17 | 3 | 11 | 3 | 14 | 3 | 13 | 0 | 8 | 2 | 0 | 2 | 14 | 3 | 15 | 2 | 4 | 2 | 3 | 1 | 16 | 1 | 15 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 3 | 0 | 3 | 1 | 2 | 15
INPUTS | 8 | alreadystoredcnt<0>  | HZIN  | XSTALIN  | LED<6>  | storecounta<5>  | LED<7>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 2 | 0 | 0 | 16 | 2 | 15 | 2 | 1 | 2 | 14 | 2 | 2
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 15
EQ | 6 | 
   resetclk<0>.D = !alreadystoredcnt<0> & HZIN;
   resetclk<0>.CLK = XSTALIN;
    resetclk<0>.EXP  =  !LED<6> & alreadystoredcnt<0> & storecounta<5>
	# !LED<6> & storecounta<5> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 2 | 2 | uartskip<0>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 27 | 2 | 1 | 0 | 16 | 0 | 9 | 0 | 12 | 0 | 11 | 2 | 3 | 0 | 6 | 3 | 15 | 0 | 15 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 11 | 2 | 12 | 2 | 11 | 2 | 5 | 1 | 0 | 2 | 17 | 3 | 1 | 3 | 13 | 3 | 12 | 0 | 8 | 2 | 0 | 2 | 14 | 3 | 0
INPUTS | 7 | LED<7>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | LED<6>  | HZIN  | XSTALIN
INPUTMC | 5 | 2 | 1 | 2 | 0 | 2 | 14 | 2 | 2 | 0 | 16
INPUTP | 2 | 65 | 63
EQ | 5 | 
   uartskip<0>.T = !LED<7> & alreadystoredcnt<0> & !resetclk<0> & 
	!uartskip<0>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   uartskip<0>.CLK = XSTALIN;

MACROCELL | 2 | 9 | uartctr<0>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 8 | 2 | 1 | 0 | 16 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 10
INPUTS | 15 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | HZIN  | XSTALIN  | clkcounta<0>  | clkcounta<1>  | uartctr<1>.EXP
INPUTMC | 13 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 3 | 2 | 11 | 2 | 8
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 10
IMPORTS | 1 | 2 | 8
EQ | 13 | 
   uartctr<0>.T = !LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0>
	# LED<6> & !alreadystoredcnt<0> & !resetclk<0> & 
	uartctr<0> & uartctr<1> & uartctr<2> & uartctr<3> & 
	uartctr<4> & !HZIN
;Imported pterms FB3_9
	# LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>;
   uartctr<0>.CLK = XSTALIN;
    uartctr<0>.EXP  =  !resetclk<0> & clkcounta<0> & clkcounta<1>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1>

MACROCELL | 2 | 8 | uartctr<1>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 7 | 2 | 1 | 0 | 16 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTS | 12 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | HZIN  | XSTALIN
INPUTMC | 10 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 9
EQ | 12 | 
   uartctr<1>.T = !LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & uartctr<0>
	# LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>
	# LED<6> & !alreadystoredcnt<0> & !resetclk<0> & 
	uartctr<0> & uartctr<1> & uartctr<2> & uartctr<3> & 
	uartctr<4> & !HZIN;
   uartctr<1>.CLK = XSTALIN;
    uartctr<1>.EXP  =  LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>

MACROCELL | 2 | 7 | uartctr<2>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 7 | 2 | 1 | 0 | 16 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTS | 12 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | HZIN  | XSTALIN
INPUTMC | 10 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTP | 2 | 65 | 63
EQ | 9 | 
   uartctr<2>.T = !LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & uartctr<0> & uartctr<1>
	# LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>
	# LED<6> & !alreadystoredcnt<0> & !resetclk<0> & 
	uartctr<0> & uartctr<1> & uartctr<2> & uartctr<3> & 
	uartctr<4> & !HZIN;
   uartctr<2>.CLK = XSTALIN;

MACROCELL | 2 | 6 | uartctr<3>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 7 | 2 | 1 | 0 | 16 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTS | 12 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | HZIN  | XSTALIN
INPUTMC | 10 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTP | 2 | 65 | 63
EQ | 10 | 
   uartctr<3>.T = !LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & uartctr<0> & uartctr<1> & 
	uartctr<2>
	# LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>
	# LED<6> & !alreadystoredcnt<0> & !resetclk<0> & 
	uartctr<0> & uartctr<1> & uartctr<2> & uartctr<3> & 
	uartctr<4> & !HZIN;
   uartctr<3>.CLK = XSTALIN;

MACROCELL | 3 | 12 | storecounta<18>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 3 | 12 | 3 | 13 | 3 | 11
INPUTS | 10 | LED<6>  | resetclk<0>  | storecounta<18>  | alreadystoredcnt<0>  | storecounta<17>  | HZIN  | LED<7>  | XSTALIN  | uartskip<0>  | EXP14_.EXP
INPUTMC | 8 | 0 | 16 | 2 | 14 | 3 | 12 | 2 | 0 | 3 | 13 | 2 | 1 | 2 | 2 | 3 | 11
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 3 | 13
IMPORTS | 1 | 3 | 11
EQ | 12 | 
   storecounta<18>.D = LED<6> & !resetclk<0>
	# !resetclk<0> & storecounta<18>
;Imported pterms FB4_12
	# LED<6> & !alreadystoredcnt<0> & HZIN
	# !alreadystoredcnt<0> & storecounta<18> & HZIN
	# LED<7> & alreadystoredcnt<0> & !resetclk<0> & 
	uartskip<0> & !HZIN;
   storecounta<18>.CLK = XSTALIN;
    storecounta<18>.EXP  =  !LED<6> & !alreadystoredcnt<0> & storecounta<17> & 
	HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 2 | 13 | storecounta<1>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 2 | 2 | 13 | 2 | 4
INPUTS | 8 | LED<6>  | resetclk<0>  | storecounta<2>  | storecounta<1>  | alreadystoredcnt<0>  | HZIN  | storecounta<2>.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 2 | 14 | 2 | 12 | 2 | 13 | 2 | 0 | 2 | 12
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 2 | 12
EQ | 10 | 
   storecounta<1>.D = LED<6> & !resetclk<0> & storecounta<2>
	# !LED<6> & !resetclk<0> & storecounta<1>
	# LED<6> & !alreadystoredcnt<0> & storecounta<2> & 
	HZIN
	# !LED<6> & !alreadystoredcnt<0> & storecounta<1> & 
	HZIN
;Imported pterms FB3_13
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<1>.CLK = XSTALIN;

MACROCELL | 2 | 12 | storecounta<2>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 2 | 2 | 13 | 2 | 11
INPUTS | 9 | alreadystoredcnt<0>  | resetclk<0>  | HZIN  | LED<6>  | storecounta<3>  | LED<7>  | uartskip<0>  | clkcounta<1>.EXP  | XSTALIN
INPUTMC | 7 | 2 | 0 | 2 | 14 | 0 | 16 | 2 | 17 | 2 | 1 | 2 | 2 | 2 | 11
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 13
IMPORTS | 1 | 2 | 11
EQ | 10 | 
   storecounta<2>.D = LED<6> & storecounta<3>
	# alreadystoredcnt<0> & resetclk<0>
	# resetclk<0> & !HZIN
;Imported pterms FB3_12
	# !LED<6> & storecounta<2>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	uartskip<0> & !HZIN;
   storecounta<2>.CLK = XSTALIN;
    storecounta<2>.EXP  =  LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 2 | 5 | uartctr<4>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 7 | 2 | 1 | 0 | 16 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5
INPUTS | 12 | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartctr<0>  | uartctr<1>  | uartctr<2>  | uartctr<3>  | uartctr<4>  | HZIN  | LED<7>  | uartskip<0>  | XSTALIN
INPUTMC | 10 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 1 | 2 | 2
INPUTP | 2 | 65 | 63
EQ | 10 | 
   uartctr<4>.T = LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartctr<0> & uartctr<1> & uartctr<2> & 
	uartctr<3> & uartctr<4>
	# !LED<7> & LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & uartctr<0> & uartctr<1> & 
	uartctr<2> & uartctr<3>
	# LED<6> & !alreadystoredcnt<0> & !resetclk<0> & 
	uartctr<0> & uartctr<1> & uartctr<2> & uartctr<3> & 
	uartctr<4> & !HZIN;
   uartctr<4>.CLK = XSTALIN;

MACROCELL | 1 | 17 | storecounta<13>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 0 | 14 | 1 | 17 | 1 | 0
INPUTS | 8 | LED<6>  | alreadystoredcnt<0>  | storecounta<14>  | HZIN  | clkcounta<10>  | storecounta<13>  | EXP12_.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 2 | 0 | 3 | 0 | 1 | 16 | 1 | 17 | 1 | 0
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 1 | 0
EQ | 9 | 
   storecounta<13>.D = LED<6> & alreadystoredcnt<0> & storecounta<14>
	# LED<6> & storecounta<14> & !HZIN
	# !LED<6> & alreadystoredcnt<0> & storecounta<13>
	# !alreadystoredcnt<0> & HZIN & clkcounta<10>
;Imported pterms FB2_1
	# !LED<6> & storecounta<13> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<13>.CLK = XSTALIN;

MACROCELL | 3 | 0 | storecounta<14>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 1 | 17 | 3 | 1 | 3 | 17
INPUTS | 9 | LED<6>  | alreadystoredcnt<0>  | storecounta<15>  | HZIN  | LED<7>  | resetclk<0>  | uartskip<0>  | EXP13_.EXP  | XSTALIN
INPUTMC | 7 | 0 | 16 | 2 | 0 | 3 | 17 | 2 | 1 | 2 | 14 | 2 | 2 | 3 | 1
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 3 | 17
IMPORTS | 1 | 3 | 1
EQ | 12 | 
   storecounta<14>.D = LED<6> & alreadystoredcnt<0> & storecounta<15>
	# LED<6> & storecounta<15> & !HZIN
;Imported pterms FB4_2
	# !LED<6> & alreadystoredcnt<0> & storecounta<14>
	# !LED<6> & storecounta<14> & !HZIN
	# !alreadystoredcnt<0> & HZIN & clkcounta<11>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<14>.CLK = XSTALIN;
    storecounta<14>.EXP  =  !LED<6> & storecounta<15> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 3 | 17 | storecounta<15>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 2 | 3 | 0 | 3 | 17
INPUTS | 8 | LED<6>  | alreadystoredcnt<0>  | storecounta<16>  | HZIN  | clkcounta<12>  | storecounta<15>  | storecounta<14>.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 2 | 0 | 3 | 14 | 1 | 14 | 3 | 17 | 3 | 0
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 3 | 0
EQ | 9 | 
   storecounta<15>.D = LED<6> & alreadystoredcnt<0> & storecounta<16>
	# LED<6> & storecounta<16> & !HZIN
	# !LED<6> & alreadystoredcnt<0> & storecounta<15>
	# !alreadystoredcnt<0> & HZIN & clkcounta<12>
;Imported pterms FB4_1
	# !LED<6> & storecounta<15> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<15>.CLK = XSTALIN;

MACROCELL | 3 | 14 | storecounta<16>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 2 | 3 | 17 | 3 | 14
INPUTS | 8 | alreadystoredcnt<0>  | resetclk<0>  | HZIN  | LED<6>  | storecounta<17>  | storecounta<16>  | storecounta<17>.EXP  | XSTALIN
INPUTMC | 6 | 2 | 0 | 2 | 14 | 0 | 16 | 3 | 13 | 3 | 14 | 3 | 13
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 3 | 13
EQ | 8 | 
   storecounta<16>.D = LED<6> & storecounta<17>
	# !LED<6> & storecounta<16>
	# alreadystoredcnt<0> & resetclk<0>
	# resetclk<0> & !HZIN
;Imported pterms FB4_14
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	uartskip<0> & !HZIN;
   storecounta<16>.CLK = XSTALIN;

MACROCELL | 3 | 13 | storecounta<17>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 3 | 14 | 3 | 13 | 3 | 12
INPUTS | 10 | LED<6>  | resetclk<0>  | storecounta<18>  | storecounta<17>  | alreadystoredcnt<0>  | HZIN  | LED<7>  | uartskip<0>  | XSTALIN  | storecounta<18>.EXP
INPUTMC | 8 | 0 | 16 | 2 | 14 | 3 | 12 | 3 | 13 | 2 | 0 | 2 | 1 | 2 | 2 | 3 | 12
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 3 | 14
IMPORTS | 1 | 3 | 12
EQ | 12 | 
   storecounta<17>.D = LED<6> & !resetclk<0> & storecounta<18>
	# !LED<6> & !resetclk<0> & storecounta<17>
	# LED<6> & !alreadystoredcnt<0> & storecounta<18> & 
	HZIN
;Imported pterms FB4_13
	# !LED<6> & !alreadystoredcnt<0> & storecounta<17> & 
	HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<17>.CLK = XSTALIN;
    storecounta<17>.EXP  =  LED<7> & !LED<6> & alreadystoredcnt<0> & 
	uartskip<0> & !HZIN

MACROCELL | 2 | 17 | storecounta<3>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 2 | 12 | 2 | 0 | 2 | 16
INPUTS | 10 | LED<6>  | alreadystoredcnt<0>  | storecounta<4>  | HZIN  | clkcounta<0>  | LED<7>  | resetclk<0>  | uartskip<0>  | alreadystoredcnt<0>.EXP  | XSTALIN
INPUTMC | 8 | 0 | 16 | 2 | 0 | 2 | 16 | 2 | 3 | 2 | 1 | 2 | 14 | 2 | 2 | 2 | 0
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 16
IMPORTS | 1 | 2 | 0
EQ | 11 | 
   storecounta<3>.D = LED<6> & alreadystoredcnt<0> & storecounta<4>
	# LED<6> & storecounta<4> & !HZIN
	# !alreadystoredcnt<0> & HZIN & clkcounta<0>
;Imported pterms FB3_1
	# !LED<6> & alreadystoredcnt<0> & storecounta<3>
	# !LED<6> & storecounta<3> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<3>.CLK = XSTALIN;
    storecounta<3>.EXP  =  LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 2 | 16 | storecounta<4>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 2 | 17 | 2 | 16 | 2 | 15
INPUTS | 9 | LED<6>  | alreadystoredcnt<0>  | storecounta<5>  | HZIN  | clkcounta<1>  | storecounta<4>  | storecounta<5>.EXP  | storecounta<3>.EXP  | XSTALIN
INPUTMC | 7 | 0 | 16 | 2 | 0 | 2 | 15 | 2 | 11 | 2 | 16 | 2 | 15 | 2 | 17
INPUTP | 2 | 65 | 63
IMPORTS | 2 | 2 | 15 | 2 | 17
EQ | 10 | 
   storecounta<4>.D = LED<6> & alreadystoredcnt<0> & storecounta<5>
	# LED<6> & storecounta<5> & !HZIN
	# !LED<6> & alreadystoredcnt<0> & storecounta<4>
	# !alreadystoredcnt<0> & HZIN & clkcounta<1>
;Imported pterms FB3_16
	# !LED<6> & storecounta<4> & !HZIN
;Imported pterms FB3_18
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<4>.CLK = XSTALIN;

MACROCELL | 2 | 15 | storecounta<5>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 2 | 2 | 16 | 2 | 14
INPUTS | 8 | LED<6>  | alreadystoredcnt<0>  | storecounta<6>  | HZIN  | clkcounta<2>  | storecounta<4>  | resetclk<0>.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 2 | 0 | 3 | 16 | 2 | 10 | 2 | 16 | 2 | 14
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 16
IMPORTS | 1 | 2 | 14
EQ | 10 | 
   storecounta<5>.D = LED<6> & alreadystoredcnt<0> & storecounta<6>
	# LED<6> & storecounta<6> & !HZIN
	# !alreadystoredcnt<0> & HZIN & clkcounta<2>
;Imported pterms FB3_15
	# !LED<6> & alreadystoredcnt<0> & storecounta<5>
	# !LED<6> & storecounta<5> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<5>.CLK = XSTALIN;
    storecounta<5>.EXP  =  !LED<6> & storecounta<4> & !HZIN

MACROCELL | 3 | 16 | storecounta<6>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 3 | 2 | 15 | 3 | 16 | 3 | 15
INPUTS | 8 | LED<6>  | LED<0>  | alreadystoredcnt<0>  | HZIN  | clkcounta<3>  | storecounta<6>  | EXP15_.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 0 | 5 | 2 | 0 | 1 | 13 | 3 | 16 | 3 | 15
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 3 | 15
EQ | 9 | 
   storecounta<6>.D = LED<6> & LED<0> & alreadystoredcnt<0>
	# LED<6> & LED<0> & !HZIN
	# !LED<6> & alreadystoredcnt<0> & storecounta<6>
	# !alreadystoredcnt<0> & HZIN & clkcounta<3>
;Imported pterms FB4_16
	# !LED<6> & storecounta<6> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   storecounta<6>.CLK = XSTALIN;

MACROCELL | 2 | 4 | storecounta<0>
ATTRIBUTES | 8782626 | 0
OUTPUTMC | 1 | 2 | 4
INPUTS | 8 | LED<6>  | resetclk<0>  | storecounta<1>  | TX  | alreadystoredcnt<0>  | HZIN  | clkcounta<0>.EXP  | XSTALIN
INPUTMC | 6 | 0 | 16 | 2 | 14 | 2 | 13 | 2 | 4 | 2 | 0 | 2 | 3
INPUTP | 2 | 65 | 63
IMPORTS | 1 | 2 | 3
EQ | 9 | 
   TX.D = LED<6> & !resetclk<0> & storecounta<1>
	# !LED<6> & !resetclk<0> & TX
	# LED<6> & !alreadystoredcnt<0> & storecounta<1> & 
	HZIN
	# !LED<6> & !alreadystoredcnt<0> & HZIN & TX
;Imported pterms FB3_4
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN;
   TX.CLK = XSTALIN;

MACROCELL | 2 | 3 | clkcounta<0>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 16 | 2 | 17 | 2 | 3 | 1 | 16 | 1 | 15 | 2 | 11 | 2 | 9 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14 | 2 | 10 | 2 | 4
INPUTS | 8 | resetclk<0>  | clkcounta<0>  | alreadystoredcnt<0>  | HZIN  | XSTALIN  | LED<7>  | LED<6>  | uartskip<0>
INPUTMC | 6 | 2 | 14 | 2 | 3 | 2 | 0 | 2 | 1 | 0 | 16 | 2 | 2
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 4
EQ | 5 | 
   clkcounta<0>.D = !resetclk<0> & !clkcounta<0>
	# !alreadystoredcnt<0> & HZIN & !clkcounta<0>;
   clkcounta<0>.CLK = XSTALIN;
    clkcounta<0>.EXP  =  LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 1 | 16 | clkcounta<10>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 4 | 1 | 17 | 1 | 16 | 1 | 15 | 1 | 14
INPUTS | 15 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<10>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | clkcounta<6>  | clkcounta<7>  | clkcounta<8>  | clkcounta<9>  | XSTALIN
INPUTMC | 13 | 2 | 0 | 2 | 14 | 1 | 16 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7
INPUTP | 2 | 65 | 63
EQ | 11 | 
   clkcounta<10>.T = alreadystoredcnt<0> & resetclk<0> & 
	clkcounta<10>
	# resetclk<0> & !HZIN & clkcounta<10>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3> & clkcounta<4> & clkcounta<5> & 
	clkcounta<6> & clkcounta<7> & clkcounta<8> & clkcounta<9>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4> & 
	clkcounta<5> & clkcounta<6> & clkcounta<7> & clkcounta<8> & 
	clkcounta<9>;
   clkcounta<10>.CLK = XSTALIN;

MACROCELL | 1 | 15 | clkcounta<11>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 3 | 1 | 14 | 1 | 15 | 3 | 1
INPUTS | 16 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<11>  | HZIN  | clkcounta<0>  | clkcounta<10>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | clkcounta<6>  | clkcounta<7>  | clkcounta<8>  | clkcounta<9>  | XSTALIN
INPUTMC | 14 | 2 | 0 | 2 | 14 | 1 | 15 | 2 | 3 | 1 | 16 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7
INPUTP | 2 | 65 | 63
EQ | 12 | 
   clkcounta<11>.T = alreadystoredcnt<0> & resetclk<0> & 
	clkcounta<11>
	# resetclk<0> & !HZIN & clkcounta<11>
	# !resetclk<0> & clkcounta<0> & clkcounta<10> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4> & 
	clkcounta<5> & clkcounta<6> & clkcounta<7> & clkcounta<8> & 
	clkcounta<9>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<10> & clkcounta<1> & clkcounta<2> & clkcounta<3> & 
	clkcounta<4> & clkcounta<5> & clkcounta<6> & clkcounta<7> & 
	clkcounta<8> & clkcounta<9>;
   clkcounta<11>.CLK = XSTALIN;

MACROCELL | 2 | 11 | clkcounta<1>
ATTRIBUTES | 8520480 | 0
OUTPUTMC | 15 | 2 | 16 | 1 | 16 | 1 | 15 | 2 | 11 | 2 | 9 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14 | 2 | 10 | 2 | 12
INPUTS | 11 | resetclk<0>  | clkcounta<0>  | clkcounta<1>  | LED<6>  | storecounta<2>  | XSTALIN  | LED<7>  | alreadystoredcnt<0>  | uartskip<0>  | HZIN  | clkcounta<2>.EXP
INPUTMC | 9 | 2 | 14 | 2 | 3 | 2 | 11 | 0 | 16 | 2 | 12 | 2 | 1 | 2 | 0 | 2 | 2 | 2 | 10
INPUTP | 2 | 63 | 65
EXPORTS | 1 | 2 | 12
IMPORTS | 1 | 2 | 10
EQ | 11 | 
   clkcounta<1>.D = !resetclk<0> & clkcounta<0> & !clkcounta<1>
	# !resetclk<0> & !clkcounta<0> & clkcounta<1>
;Imported pterms FB3_11
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	!clkcounta<1>
	# !alreadystoredcnt<0> & HZIN & !clkcounta<0> & 
	clkcounta<1>;
   clkcounta<1>.CLK = XSTALIN;
    clkcounta<1>.EXP  =  !LED<6> & storecounta<2>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	uartskip<0> & !HZIN

MACROCELL | 2 | 10 | clkcounta<2>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 13 | 2 | 15 | 1 | 16 | 1 | 15 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14 | 2 | 11
INPUTS | 8 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<2>  | HZIN  | clkcounta<0>  | clkcounta<1>  | XSTALIN  | uartctr<0>.EXP
INPUTMC | 6 | 2 | 0 | 2 | 14 | 2 | 10 | 2 | 3 | 2 | 11 | 2 | 9
INPUTP | 2 | 65 | 63
EXPORTS | 1 | 2 | 11
IMPORTS | 1 | 2 | 9
EQ | 11 | 
   clkcounta<2>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<2>
	# resetclk<0> & !HZIN & clkcounta<2>
;Imported pterms FB3_10
	# !resetclk<0> & clkcounta<0> & clkcounta<1>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1>;
   clkcounta<2>.CLK = XSTALIN;
    clkcounta<2>.EXP  =  !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	!clkcounta<1>
	# !alreadystoredcnt<0> & HZIN & !clkcounta<0> & 
	clkcounta<1>

MACROCELL | 1 | 13 | clkcounta<3>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 11 | 3 | 16 | 1 | 16 | 1 | 15 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14
INPUTS | 8 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<3>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | XSTALIN
INPUTMC | 6 | 2 | 0 | 2 | 14 | 1 | 13 | 2 | 3 | 2 | 11 | 2 | 10
INPUTP | 2 | 65 | 63
EQ | 7 | 
   clkcounta<3>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<3>
	# resetclk<0> & !HZIN & clkcounta<3>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2>;
   clkcounta<3>.CLK = XSTALIN;

MACROCELL | 1 | 12 | clkcounta<4>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 10 | 0 | 5 | 1 | 16 | 1 | 15 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14
INPUTS | 9 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<4>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | XSTALIN
INPUTMC | 7 | 2 | 0 | 2 | 14 | 1 | 12 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13
INPUTP | 2 | 65 | 63
EQ | 7 | 
   clkcounta<4>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<4>
	# resetclk<0> & !HZIN & clkcounta<4>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3>;
   clkcounta<4>.CLK = XSTALIN;

MACROCELL | 1 | 11 | clkcounta<5>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 9 | 0 | 7 | 1 | 16 | 1 | 15 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14
INPUTS | 10 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<5>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | XSTALIN
INPUTMC | 8 | 2 | 0 | 2 | 14 | 1 | 11 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12
INPUTP | 2 | 65 | 63
EQ | 7 | 
   clkcounta<5>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<5>
	# resetclk<0> & !HZIN & clkcounta<5>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3> & clkcounta<4>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4>;
   clkcounta<5>.CLK = XSTALIN;

MACROCELL | 1 | 10 | clkcounta<6>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 8 | 1 | 14 | 1 | 16 | 1 | 15 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 0 | 9
INPUTS | 11 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<6>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | XSTALIN
INPUTMC | 9 | 2 | 0 | 2 | 14 | 1 | 10 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11
INPUTP | 2 | 65 | 63
EQ | 8 | 
   clkcounta<6>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<6>
	# resetclk<0> & !HZIN & clkcounta<6>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3> & clkcounta<4> & clkcounta<5>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4> & 
	clkcounta<5>;
   clkcounta<6>.CLK = XSTALIN;

MACROCELL | 1 | 9 | clkcounta<7>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 7 | 0 | 10 | 1 | 16 | 1 | 15 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14
INPUTS | 12 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<7>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | clkcounta<6>  | XSTALIN
INPUTMC | 10 | 2 | 0 | 2 | 14 | 1 | 9 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10
INPUTP | 2 | 65 | 63
EQ | 9 | 
   clkcounta<7>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<7>
	# resetclk<0> & !HZIN & clkcounta<7>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3> & clkcounta<4> & clkcounta<5> & 
	clkcounta<6>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4> & 
	clkcounta<5> & clkcounta<6>;
   clkcounta<7>.CLK = XSTALIN;

MACROCELL | 1 | 8 | clkcounta<8>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 6 | 0 | 13 | 1 | 16 | 1 | 15 | 1 | 8 | 1 | 7 | 1 | 14
INPUTS | 13 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<8>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | clkcounta<6>  | clkcounta<7>  | XSTALIN
INPUTMC | 11 | 2 | 0 | 2 | 14 | 1 | 8 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9
INPUTP | 2 | 65 | 63
EQ | 9 | 
   clkcounta<8>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<8>
	# resetclk<0> & !HZIN & clkcounta<8>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3> & clkcounta<4> & clkcounta<5> & 
	clkcounta<6> & clkcounta<7>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4> & 
	clkcounta<5> & clkcounta<6> & clkcounta<7>;
   clkcounta<8>.CLK = XSTALIN;

MACROCELL | 1 | 7 | clkcounta<9>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 5 | 0 | 14 | 1 | 16 | 1 | 15 | 1 | 7 | 1 | 14
INPUTS | 14 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<9>  | HZIN  | clkcounta<0>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | clkcounta<6>  | clkcounta<7>  | clkcounta<8>  | XSTALIN
INPUTMC | 12 | 2 | 0 | 2 | 14 | 1 | 7 | 2 | 3 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8
INPUTP | 2 | 65 | 63
EQ | 9 | 
   clkcounta<9>.T = alreadystoredcnt<0> & resetclk<0> & clkcounta<9>
	# resetclk<0> & !HZIN & clkcounta<9>
	# !resetclk<0> & clkcounta<0> & clkcounta<1> & 
	clkcounta<2> & clkcounta<3> & clkcounta<4> & clkcounta<5> & 
	clkcounta<6> & clkcounta<7> & clkcounta<8>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<1> & clkcounta<2> & clkcounta<3> & clkcounta<4> & 
	clkcounta<5> & clkcounta<6> & clkcounta<7> & clkcounta<8>;
   clkcounta<9>.CLK = XSTALIN;

MACROCELL | 1 | 14 | clkcounta<12>
ATTRIBUTES | 4326176 | 0
OUTPUTMC | 2 | 3 | 17 | 1 | 14
INPUTS | 17 | alreadystoredcnt<0>  | resetclk<0>  | clkcounta<12>  | HZIN  | clkcounta<0>  | clkcounta<10>  | clkcounta<11>  | clkcounta<1>  | clkcounta<2>  | clkcounta<3>  | clkcounta<4>  | clkcounta<5>  | clkcounta<6>  | clkcounta<7>  | clkcounta<8>  | clkcounta<9>  | XSTALIN
INPUTMC | 15 | 2 | 0 | 2 | 14 | 1 | 14 | 2 | 3 | 1 | 16 | 1 | 15 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7
INPUTP | 2 | 65 | 63
EQ | 12 | 
   clkcounta<12>.T = alreadystoredcnt<0> & resetclk<0> & 
	clkcounta<12>
	# resetclk<0> & !HZIN & clkcounta<12>
	# !resetclk<0> & clkcounta<0> & clkcounta<10> & 
	clkcounta<11> & clkcounta<1> & clkcounta<2> & clkcounta<3> & 
	clkcounta<4> & clkcounta<5> & clkcounta<6> & clkcounta<7> & 
	clkcounta<8> & clkcounta<9>
	# !alreadystoredcnt<0> & HZIN & clkcounta<0> & 
	clkcounta<10> & clkcounta<11> & clkcounta<1> & clkcounta<2> & 
	clkcounta<3> & clkcounta<4> & clkcounta<5> & clkcounta<6> & 
	clkcounta<7> & clkcounta<8> & clkcounta<9>;
   clkcounta<12>.CLK = XSTALIN;

MACROCELL | 0 | 4 | EXP6_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 0 | 5
INPUTS | 3 | LED<6>  | LED<0>  | HZIN
INPUTMC | 2 | 0 | 16 | 0 | 5
INPUTP | 1 | 65
EXPORTS | 1 | 0 | 5
EQ | 1 | 
       EXP6_.EXP  =  !LED<6> & LED<0> & !HZIN

MACROCELL | 0 | 6 | EXP7_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 0 | 5
INPUTS | 6 | LED<7>  | LED<6>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>  | HZIN
INPUTMC | 5 | 2 | 1 | 0 | 16 | 2 | 0 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 0 | 5
EQ | 2 | 
       EXP7_.EXP  =  LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 0 | 9 | EXP8_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 0 | 8
INPUTS | 8 | LED<6>  | LED<2>  | alreadystoredcnt<0>  | HZIN  | clkcounta<6>  | LED<7>  | resetclk<0>  | uartskip<0>
INPUTMC | 7 | 0 | 16 | 0 | 8 | 2 | 0 | 1 | 10 | 2 | 1 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 0 | 8
EQ | 5 | 
       EXP8_.EXP  =  !LED<6> & LED<2> & alreadystoredcnt<0>
	# !LED<6> & LED<2> & !HZIN
	# !alreadystoredcnt<0> & HZIN & clkcounta<6>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 0 | 11 | EXP9_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 0 | 10
INPUTS | 7 | LED<6>  | LED<3>  | HZIN  | LED<7>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 0 | 16 | 0 | 10 | 2 | 1 | 2 | 0 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 0 | 10
EQ | 3 | 
       EXP9_.EXP  =  !LED<6> & LED<3> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 0 | 12 | EXP10_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 0 | 13
INPUTS | 7 | LED<6>  | LED<4>  | HZIN  | LED<7>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 0 | 16 | 0 | 13 | 2 | 1 | 2 | 0 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 0 | 13
EQ | 3 | 
       EXP10_.EXP  =  !LED<6> & LED<4> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 0 | 15 | EXP11_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 0 | 14
INPUTS | 7 | LED<6>  | LED<5>  | HZIN  | LED<7>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 0 | 16 | 0 | 14 | 2 | 1 | 2 | 0 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 0 | 14
EQ | 3 | 
       EXP11_.EXP  =  !LED<6> & LED<5> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 1 | 0 | EXP12_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 1 | 17
INPUTS | 7 | LED<6>  | storecounta<13>  | HZIN  | LED<7>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 0 | 16 | 1 | 17 | 2 | 1 | 2 | 0 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 1 | 17
EQ | 3 | 
       EXP12_.EXP  =  !LED<6> & storecounta<13> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 3 | 1 | EXP13_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 0
INPUTS | 8 | LED<6>  | alreadystoredcnt<0>  | storecounta<14>  | HZIN  | clkcounta<11>  | LED<7>  | resetclk<0>  | uartskip<0>
INPUTMC | 7 | 0 | 16 | 2 | 0 | 3 | 0 | 1 | 15 | 2 | 1 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 3 | 0
EQ | 5 | 
       EXP13_.EXP  =  !LED<6> & alreadystoredcnt<0> & storecounta<14>
	# !LED<6> & storecounta<14> & !HZIN
	# !alreadystoredcnt<0> & HZIN & clkcounta<11>
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

MACROCELL | 3 | 11 | EXP14_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 12
INPUTS | 7 | LED<6>  | alreadystoredcnt<0>  | HZIN  | storecounta<18>  | LED<7>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 0 | 16 | 2 | 0 | 3 | 12 | 2 | 1 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 3 | 12
EQ | 4 | 
       EXP14_.EXP  =  LED<6> & !alreadystoredcnt<0> & HZIN
	# !alreadystoredcnt<0> & storecounta<18> & HZIN
	# LED<7> & alreadystoredcnt<0> & !resetclk<0> & 
	uartskip<0> & !HZIN

MACROCELL | 3 | 15 | EXP15_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 16
INPUTS | 7 | LED<6>  | storecounta<6>  | HZIN  | LED<7>  | alreadystoredcnt<0>  | resetclk<0>  | uartskip<0>
INPUTMC | 6 | 0 | 16 | 3 | 16 | 2 | 1 | 2 | 0 | 2 | 14 | 2 | 2
INPUTP | 1 | 65
EXPORTS | 1 | 3 | 16
EQ | 3 | 
       EXP15_.EXP  =  !LED<6> & storecounta<6> & !HZIN
	# LED<7> & !LED<6> & alreadystoredcnt<0> & 
	!resetclk<0> & uartskip<0> & !HZIN

PIN | XSTALIN | 64 | 0 | N/A | 63 | 42 | 2 | 1 | 0 | 16 | 0 | 10 | 0 | 13 | 0 | 14 | 0 | 5 | 0 | 7 | 0 | 8 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 12 | 2 | 13 | 2 | 12 | 2 | 5 | 1 | 17 | 3 | 0 | 3 | 17 | 3 | 14 | 3 | 13 | 2 | 17 | 2 | 16 | 2 | 15 | 3 | 16 | 2 | 4 | 2 | 3 | 1 | 16 | 1 | 15 | 2 | 11 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14
PIN | HZIN | 64 | 0 | N/A | 65 | 52 | 2 | 1 | 0 | 16 | 0 | 10 | 0 | 13 | 0 | 14 | 0 | 5 | 0 | 7 | 0 | 8 | 2 | 0 | 2 | 14 | 2 | 2 | 2 | 9 | 2 | 8 | 2 | 7 | 2 | 6 | 3 | 11 | 2 | 13 | 2 | 12 | 2 | 5 | 1 | 17 | 3 | 0 | 3 | 17 | 3 | 14 | 3 | 13 | 2 | 17 | 2 | 16 | 2 | 15 | 3 | 16 | 2 | 4 | 2 | 3 | 1 | 16 | 1 | 15 | 1 | 0 | 2 | 10 | 1 | 13 | 1 | 12 | 1 | 11 | 1 | 10 | 1 | 9 | 1 | 8 | 1 | 7 | 1 | 14 | 0 | 4 | 0 | 6 | 0 | 9 | 0 | 11 | 0 | 12 | 0 | 15 | 2 | 11 | 3 | 1 | 3 | 12 | 3 | 15
PIN | LED<7> | 536871040 | 0 | N/A | 29
PIN | LED<6> | 536871040 | 0 | N/A | 27
PIN | LED<3> | 536871040 | 0 | N/A | 21
PIN | LED<4> | 536871040 | 0 | N/A | 24
PIN | LED<5> | 536871040 | 0 | N/A | 26
PIN | LED<0> | 536871040 | 0 | N/A | 13
PIN | LED<1> | 536871040 | 0 | N/A | 15
PIN | LED<2> | 536871040 | 0 | N/A | 20
PIN | TX | 536871040 | 0 | N/A | 31
