 
cpldfit:  version P.20131013                        Xilinx Inc.
                                  Fitter Report
Design Name: counta                              Date:  8- 4-2020,  0:40AM
Device Used: XC9572XL-5-VQ44
Fitting Status: Successful

*************************  Mapped Resource Summary  **************************

Macrocells     Product Terms    Function Block   Registers      Pins           
Used/Tot       Used/Tot         Inps Used/Tot    Used/Tot       Used/Tot       
42 /72  ( 58%) 227 /360  ( 63%) 86 /216 ( 40%)   42 /72  ( 58%) 11 /34  ( 32%)

** Function Block Resources **

Function    Mcells      FB Inps     Pterms      IO          
Block       Used/Tot    Used/Tot    Used/Tot    Used/Tot    
FB1           7/18       25/54       47/90       7/ 9
FB2          11/18       22/54       57/90       0/ 9
FB3          18/18*      22/54       84/90       2/ 9
FB4           6/18       17/54       39/90       2/ 7
             -----       -----       -----      -----    
             42/72       86/216     227/360     11/34 

* - Resource is exhausted

** Global Control Resources **

Global clock net(s) unused.
Global output enable net(s) unused.
Global set/reset net(s) unused.

** Pin Resources **

Signal Type    Required     Mapped  |  Pin Type            Used    Total 
------------------------------------|------------------------------------
Input         :    2           2    |  I/O              :     8      28
Output        :    9           9    |  GCK/IO           :     3       3
Bidirectional :    0           0    |  GTS/IO           :     0       2
GCK           :    0           0    |  GSR/IO           :     0       1
GTS           :    0           0    |
GSR           :    0           0    |
                 ----        ----
        Total     11          11

** Power Data **

There are 42 macrocells in high performance mode (MCHP).
There are 0 macrocells in low power mode (MCLP).
End of Mapped Resource Summary
**************************  Errors and Warnings  ***************************

WARNING:Cpld - Unable to retrieve the path to the iSE Project Repository. Will
   use the default filename of 'counta.ise'.
*************************  Summary of Mapped Logic  ************************

** 9 Outputs **

Signal               Total Total Loc     Pin  Pin     Pin     Pwr  Slew Reg Init
Name                 Pts   Inps          No.  Type    Use     Mode Rate State
LED<0>               7     10    FB1_6   41   I/O     O       STD  FAST RESET
LED<1>               7     10    FB1_8   42   I/O     O       STD  FAST RESET
LED<2>               7     10    FB1_9   43   GCK/I/O O       STD  FAST RESET
LED<3>               7     10    FB1_11  44   GCK/I/O O       STD  FAST RESET
LED<4>               7     10    FB1_14  1    GCK/I/O O       STD  FAST RESET
LED<5>               7     10    FB1_15  2    I/O     O       STD  FAST RESET
LED<6>               5     12    FB1_17  3    I/O     O       STD  FAST RESET
LED<7>               4     12    FB3_2   5    I/O     O       STD  FAST RESET
TX                   6     9     FB3_5   6    I/O     O       STD  FAST RESET

** 33 Buried Nodes **

Signal               Total Total Loc     Pwr  Reg Init
Name                 Pts   Inps          Mode State
clkcounta<9>         5     14    FB2_8   STD  RESET
clkcounta<8>         5     13    FB2_9   STD  RESET
clkcounta<7>         5     12    FB2_10  STD  RESET
clkcounta<6>         5     11    FB2_11  STD  RESET
clkcounta<5>         5     10    FB2_12  STD  RESET
clkcounta<4>         5     9     FB2_13  STD  RESET
clkcounta<3>         5     8     FB2_14  STD  RESET
clkcounta<12>        5     17    FB2_15  STD  RESET
clkcounta<11>        5     16    FB2_16  STD  RESET
clkcounta<10>        5     15    FB2_17  STD  RESET
storecounta<13>      7     10    FB2_18  STD  RESET
alreadystoredcnt<0>  3     7     FB3_1   STD  RESET
uartskip<0>          3     7     FB3_3   STD  RESET
clkcounta<0>         3     5     FB3_4   STD  RESET
uartctr<4>           4     12    FB3_6   STD  RESET
uartctr<3>           4     12    FB3_7   STD  RESET
uartctr<2>           4     12    FB3_8   STD  RESET
uartctr<1>           4     12    FB3_9   STD  RESET
uartctr<0>           4     12    FB3_10  STD  RESET
clkcounta<2>         5     7     FB3_11  STD  RESET
clkcounta<1>         5     6     FB3_12  STD  RESET
storecounta<2>       6     9     FB3_13  STD  RESET
storecounta<1>       6     9     FB3_14  STD  RESET
resetclk<0>          2     3     FB3_15  STD  RESET
storecounta<5>       7     10    FB3_16  STD  RESET
storecounta<4>       7     10    FB3_17  STD  RESET
storecounta<3>       7     10    FB3_18  STD  RESET
storecounta<14>      7     10    FB4_1   STD  RESET
storecounta<18>      6     8     FB4_13  STD  RESET
storecounta<17>      6     9     FB4_14  STD  RESET
storecounta<16>      6     9     FB4_15  STD  RESET
storecounta<6>       7     10    FB4_17  STD  RESET
storecounta<15>      7     10    FB4_18  STD  RESET

** 2 Inputs **

Signal               Loc     Pin  Pin     Pin     
Name                         No.  Type    Use     
XSTALIN              FB4_5   20   I/O     I
HZIN                 FB4_8   21   I/O     I

Legend:
Pin No. - ~ - User Assigned
**************************  Function Block Details  ************************
Legend:
Total Pt     - Total product terms used by the macrocell signal
Imp Pt       - Product terms imported from other macrocells
Exp Pt       - Product terms exported to other macrocells
               in direction shown
Unused Pt    - Unused local product terms remaining in macrocell
Loc          - Location where logic was mapped in device
Pin Type/Use - I  - Input             GCK - Global Clock
               O  - Output            GTS - Global Output Enable
              (b) - Buried macrocell  GSR - Global Set/Reset
X            - Signal used as input to the macrocell logic.
Pin No.      - ~  - User Assigned
*********************************** FB1  ***********************************
Number of function block inputs used/remaining:               25/29
Number of signals used by logic mapping into function block:  25
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
(unused)              0       0     0   5     FB1_1         (b)     
(unused)              0       0     0   5     FB1_2   39    I/O     
(unused)              0       0     0   5     FB1_3         (b)     
(unused)              0       0     0   5     FB1_4         (b)     
(unused)              0       0   \/1   4     FB1_5   40    I/O     (b)
LED<0>                7       2<-   0   0     FB1_6   41    I/O     O
(unused)              0       0   /\1   4     FB1_7         (b)     (b)
LED<1>                7       2<-   0   0     FB1_8   42    I/O     O
LED<2>                7       4<- /\2   0     FB1_9   43    GCK/I/O O
(unused)              0       0   /\4   1     FB1_10        (b)     (b)
LED<3>                7       2<-   0   0     FB1_11  44    GCK/I/O O
(unused)              0       0   /\2   3     FB1_12        (b)     (b)
(unused)              0       0   \/2   3     FB1_13        (b)     (b)
LED<4>                7       2<-   0   0     FB1_14  1     GCK/I/O O
LED<5>                7       2<-   0   0     FB1_15  2     I/O     O
(unused)              0       0   /\2   3     FB1_16        (b)     (b)
LED<6>                5       0     0   0     FB1_17  3     I/O     O
(unused)              0       0     0   5     FB1_18        (b)     

Signals Used by Logic in Function Block
  1: HZIN              10: XSTALIN              18: resetclk<0> 
  2: LED<0>            11: alreadystoredcnt<0>  19: storecounta<13> 
  3: LED<1>            12: clkcounta<4>         20: uartctr<0> 
  4: LED<2>            13: clkcounta<5>         21: uartctr<1> 
  5: LED<3>            14: clkcounta<6>         22: uartctr<2> 
  6: LED<4>            15: clkcounta<7>         23: uartctr<3> 
  7: LED<5>            16: clkcounta<8>         24: uartctr<4> 
  8: LED<6>            17: clkcounta<9>         25: uartskip<0> 
  9: LED<7>           

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
LED<0>               XXX....XXXXX.....X......X............... 10
LED<1>               X.XX...XXXX.X....X......X............... 10
LED<2>               X..XX..XXXX..X...X......X............... 10
LED<3>               X...XX.XXXX...X..X......X............... 10
LED<4>               X....XXXXXX....X.X......X............... 10
LED<5>               X.....XXXXX.....XXX.....X............... 10
LED<6>               X......XXXX......X.XXXXXX............... 12
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB2  ***********************************
Number of function block inputs used/remaining:               22/32
Number of signals used by logic mapping into function block:  22
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
(unused)              0       0   /\2   3     FB2_1         (b)     (b)
(unused)              0       0     0   5     FB2_2   29    I/O     
(unused)              0       0     0   5     FB2_3         (b)     
(unused)              0       0     0   5     FB2_4         (b)     
(unused)              0       0     0   5     FB2_5   30    I/O     
(unused)              0       0     0   5     FB2_6   31    I/O     
(unused)              0       0     0   5     FB2_7         (b)     
clkcounta<9>          5       0     0   0     FB2_8   32    I/O     (b)
clkcounta<8>          5       0     0   0     FB2_9   33    GSR/I/O (b)
clkcounta<7>          5       0     0   0     FB2_10        (b)     (b)
clkcounta<6>          5       0     0   0     FB2_11  34    GTS/I/O (b)
clkcounta<5>          5       0     0   0     FB2_12        (b)     (b)
clkcounta<4>          5       0     0   0     FB2_13        (b)     (b)
clkcounta<3>          5       0     0   0     FB2_14  36    GTS/I/O (b)
clkcounta<12>         5       0     0   0     FB2_15  37    I/O     (b)
clkcounta<11>         5       0     0   0     FB2_16        (b)     (b)
clkcounta<10>         5       0     0   0     FB2_17  38    I/O     (b)
storecounta<13>       7       2<-   0   0     FB2_18        (b)     (b)

Signals Used by Logic in Function Block
  1: HZIN                  9: clkcounta<12>     16: clkcounta<7> 
  2: LED<6>               10: clkcounta<1>      17: clkcounta<8> 
  3: LED<7>               11: clkcounta<2>      18: clkcounta<9> 
  4: XSTALIN              12: clkcounta<3>      19: resetclk<0> 
  5: alreadystoredcnt<0>  13: clkcounta<4>      20: storecounta<13> 
  6: clkcounta<0>         14: clkcounta<5>      21: storecounta<14> 
  7: clkcounta<10>        15: clkcounta<6>      22: uartskip<0> 
  8: clkcounta<11>       

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
clkcounta<9>         X..XXX...XXXXXXXXXX..................... 14
clkcounta<8>         X..XXX...XXXXXXXX.X..................... 13
clkcounta<7>         X..XXX...XXXXXXX..X..................... 12
clkcounta<6>         X..XXX...XXXXXX...X..................... 11
clkcounta<5>         X..XXX...XXXXX....X..................... 10
clkcounta<4>         X..XXX...XXXX.....X..................... 9
clkcounta<3>         X..XXX...XXX......X..................... 8
clkcounta<12>        X..XXXXXXXXXXXXXXXX..................... 17
clkcounta<11>        X..XXXXX.XXXXXXXXXX..................... 16
clkcounta<10>        X..XXXX..XXXXXXXXXX..................... 15
storecounta<13>      XXXXX.X...........XXXX.................. 10
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB3  ***********************************
Number of function block inputs used/remaining:               22/32
Number of signals used by logic mapping into function block:  22
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
alreadystoredcnt<0>   3       1<- /\3   0     FB3_1         (b)     (b)
LED<7>                4       0   /\1   0     FB3_2   5     I/O     O
uartskip<0>           3       0     0   2     FB3_3         (b)     (b)
clkcounta<0>          3       0   \/1   1     FB3_4         (b)     (b)
TX                    6       1<-   0   0     FB3_5   6     I/O     O
uartctr<4>            4       0     0   1     FB3_6         (b)     (b)
uartctr<3>            4       0     0   1     FB3_7         (b)     (b)
uartctr<2>            4       0     0   1     FB3_8   7     I/O     (b)
uartctr<1>            4       0   \/1   0     FB3_9   8     I/O     (b)
uartctr<0>            4       1<- \/2   0     FB3_10        (b)     (b)
clkcounta<2>          5       2<- \/2   0     FB3_11  12    I/O     (b)
clkcounta<1>          5       2<- \/2   0     FB3_12        (b)     (b)
storecounta<2>        6       2<- \/1   0     FB3_13        (b)     (b)
storecounta<1>        6       1<-   0   0     FB3_14  13    I/O     (b)
resetclk<0>           2       0   \/3   0     FB3_15  14    I/O     (b)
storecounta<5>        7       3<- \/1   0     FB3_16  18    I/O     (b)
storecounta<4>        7       2<-   0   0     FB3_17  16    I/O     (b)
storecounta<3>        7       3<- /\1   0     FB3_18        (b)     (b)

Signals Used by Logic in Function Block
  1: HZIN                  9: clkcounta<2>      16: storecounta<6> 
  2: LED<6>               10: resetclk<0>       17: uartctr<0> 
  3: LED<7>               11: storecounta<1>    18: uartctr<1> 
  4: TX                   12: storecounta<2>    19: uartctr<2> 
  5: XSTALIN              13: storecounta<3>    20: uartctr<3> 
  6: alreadystoredcnt<0>  14: storecounta<4>    21: uartctr<4> 
  7: clkcounta<0>         15: storecounta<5>    22: uartskip<0> 
  8: clkcounta<1>        

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
alreadystoredcnt<0>  XXX.XX...X...........X.................. 7
LED<7>               XXX.XX...X......XXXXXX.................. 12
uartskip<0>          XXX.XX...X...........X.................. 7
clkcounta<0>         X...XXX..X.............................. 5
TX                   XXXXXX...XX..........X.................. 9
uartctr<4>           XXX.XX...X......XXXXXX.................. 12
uartctr<3>           XXX.XX...X......XXXXXX.................. 12
uartctr<2>           XXX.XX...X......XXXXXX.................. 12
uartctr<1>           XXX.XX...X......XXXXXX.................. 12
uartctr<0>           XXX.XX...X......XXXXXX.................. 12
clkcounta<2>         X...XXXXXX.............................. 7
clkcounta<1>         X...XXXX.X.............................. 6
storecounta<2>       XXX.XX...X.XX........X.................. 9
storecounta<1>       XXX.XX...XXX.........X.................. 9
resetclk<0>          X...XX.................................. 3
storecounta<5>       XXX.XX..XX....XX.....X.................. 10
storecounta<4>       XXX.XX.X.X...XX......X.................. 10
storecounta<3>       XXX.XXX..X..XX.......X.................. 10
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*********************************** FB4  ***********************************
Number of function block inputs used/remaining:               17/37
Number of signals used by logic mapping into function block:  17
Signal              Total   Imp   Exp Unused  Loc     Pin   Pin     Pin
Name                Pt      Pt    Pt  Pt               #    Type    Use
storecounta<14>       7       4<- /\2   0     FB4_1         (b)     (b)
(unused)              0       0   /\4   1     FB4_2   19    I/O     (b)
(unused)              0       0     0   5     FB4_3         (b)     
(unused)              0       0     0   5     FB4_4         (b)     
(unused)              0       0     0   5     FB4_5   20    I/O     I
(unused)              0       0     0   5     FB4_6         (b)     
(unused)              0       0     0   5     FB4_7         (b)     
(unused)              0       0     0   5     FB4_8   21    I/O     I
(unused)              0       0     0   5     FB4_9         (b)     
(unused)              0       0     0   5     FB4_10        (b)     
(unused)              0       0     0   5     FB4_11  22    I/O     
(unused)              0       0   \/3   2     FB4_12        (b)     (b)
storecounta<18>       6       3<- \/2   0     FB4_13        (b)     (b)
storecounta<17>       6       2<- \/1   0     FB4_14  23    I/O     (b)
storecounta<16>       6       1<-   0   0     FB4_15  27    I/O     (b)
(unused)              0       0   \/2   3     FB4_16        (b)     (b)
storecounta<6>        7       2<-   0   0     FB4_17  28    I/O     (b)
storecounta<15>       7       2<-   0   0     FB4_18        (b)     (b)

Signals Used by Logic in Function Block
  1: HZIN                  7: clkcounta<11>     13: storecounta<16> 
  2: LED<0>                8: clkcounta<12>     14: storecounta<17> 
  3: LED<6>                9: clkcounta<3>      15: storecounta<18> 
  4: LED<7>               10: resetclk<0>       16: storecounta<6> 
  5: XSTALIN              11: storecounta<14>   17: uartskip<0> 
  6: alreadystoredcnt<0>  12: storecounta<15>  

Signal                        1         2         3         4 FB
Name                0----+----0----+----0----+----0----+----0 Inputs
storecounta<14>      X.XXXXX..XXX....X....................... 10
storecounta<18>      X.XXXX...X....X.X....................... 8
storecounta<17>      X.XXXX...X...XX.X....................... 9
storecounta<16>      X.XXXX...X..XX..X....................... 9
storecounta<6>       XXXXXX..XX.....XX....................... 10
storecounta<15>      X.XXXX.X.X.XX...X....................... 10
                    0----+----1----+----2----+----3----+----4
                              0         0         0         0
*******************************  Equations  ********************************

********** Mapped Logic **********





















FDCPE_LED0: FDCPE port map (LED(0),LED_D(0),XSTALIN,'0','0');
LED_D(0) <= ((NOT LED(6) AND LED(0) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND LED(1) AND alreadystoredcnt(0))
	OR (LED(6) AND LED(1) AND NOT HZIN)
	OR (NOT LED(6) AND LED(0) AND alreadystoredcnt(0))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(4)));

FDCPE_LED1: FDCPE port map (LED(1),LED_D(1),XSTALIN,'0','0');
LED_D(1) <= ((NOT LED(6) AND LED(1) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND LED(2) AND alreadystoredcnt(0))
	OR (LED(6) AND LED(2) AND NOT HZIN)
	OR (NOT LED(6) AND LED(1) AND alreadystoredcnt(0))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(5)));

FDCPE_LED2: FDCPE port map (LED(2),LED_D(2),XSTALIN,'0','0');
LED_D(2) <= ((NOT LED(6) AND LED(2) AND alreadystoredcnt(0))
	OR (NOT LED(6) AND LED(2) AND NOT HZIN)
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(6))
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND LED(3) AND alreadystoredcnt(0))
	OR (LED(6) AND LED(3) AND NOT HZIN));

FDCPE_LED3: FDCPE port map (LED(3),LED_D(3),XSTALIN,'0','0');
LED_D(3) <= ((NOT LED(6) AND LED(3) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND LED(4) AND alreadystoredcnt(0))
	OR (LED(6) AND LED(4) AND NOT HZIN)
	OR (NOT LED(6) AND LED(3) AND alreadystoredcnt(0))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(7)));

FDCPE_LED4: FDCPE port map (LED(4),LED_D(4),XSTALIN,'0','0');
LED_D(4) <= ((NOT LED(6) AND LED(4) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND LED(5) AND alreadystoredcnt(0))
	OR (LED(6) AND LED(5) AND NOT HZIN)
	OR (NOT LED(6) AND LED(4) AND alreadystoredcnt(0))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(8)));

FDCPE_LED5: FDCPE port map (LED(5),LED_D(5),XSTALIN,'0','0');
LED_D(5) <= ((NOT LED(6) AND LED(5) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(13))
	OR (LED(6) AND storecounta(13) AND NOT HZIN)
	OR (NOT LED(6) AND LED(5) AND alreadystoredcnt(0))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(9)));

FTCPE_LED6: FTCPE port map (LED(6),LED_T(6),XSTALIN,'0','0');
LED_T(6) <= ((NOT LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND NOT uartskip(0))
	OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (LED(6) AND alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartskip(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND 
	uartctr(4) AND NOT HZIN));

FTCPE_LED7: FTCPE port map (LED(7),LED_T(7),XSTALIN,'0','0');
LED_T(7) <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1) AND 
	uartctr(2) AND uartctr(3) AND uartctr(4))
	OR (NOT LED(7) AND LED(6) AND NOT alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4) AND NOT HZIN));

FDCPE_TX: FDCPE port map (TX,TX_D,XSTALIN,'0','0');
TX_D <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND NOT resetclk(0) AND storecounta(1))
	OR (NOT LED(6) AND NOT resetclk(0) AND TX)
	OR (LED(6) AND NOT alreadystoredcnt(0) AND storecounta(1) AND 
	HZIN)
	OR (NOT LED(6) AND NOT alreadystoredcnt(0) AND HZIN AND TX));

FDCPE_alreadystoredcnt0: FDCPE port map (alreadystoredcnt(0),alreadystoredcnt_D(0),XSTALIN,'0','0');
alreadystoredcnt_D(0) <= ((LED(7) AND NOT LED(6) AND NOT resetclk(0) AND uartskip(0) AND 
	NOT HZIN)
	OR (NOT alreadystoredcnt(0) AND NOT HZIN));

FDCPE_clkcounta0: FDCPE port map (clkcounta(0),clkcounta_D(0),XSTALIN,'0','0');
clkcounta_D(0) <= ((NOT resetclk(0) AND NOT clkcounta(0))
	OR (NOT alreadystoredcnt(0) AND HZIN AND NOT clkcounta(0)));

FDCPE_clkcounta1: FDCPE port map (clkcounta(1),clkcounta_D(1),XSTALIN,'0','0');
clkcounta_D(1) <= ((NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	NOT clkcounta(1))
	OR (NOT alreadystoredcnt(0) AND HZIN AND NOT clkcounta(0) AND 
	clkcounta(1))
	OR (NOT resetclk(0) AND clkcounta(0) AND NOT clkcounta(1))
	OR (NOT resetclk(0) AND NOT clkcounta(0) AND clkcounta(1)));

FTCPE_clkcounta2: FTCPE port map (clkcounta(2),clkcounta_T(2),XSTALIN,'0','0');
clkcounta_T(2) <= ((NOT resetclk(0) AND clkcounta(0) AND clkcounta(1))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1))
	OR (alreadystoredcnt(0) AND resetclk(0) AND clkcounta(2))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(2)));

FTCPE_clkcounta3: FTCPE port map (clkcounta(3),clkcounta_T(3),XSTALIN,'0','0');
clkcounta_T(3) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(3))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(3))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2)));

FTCPE_clkcounta4: FTCPE port map (clkcounta(4),clkcounta_T(4),XSTALIN,'0','0');
clkcounta_T(4) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(4))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(4))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3)));

FTCPE_clkcounta5: FTCPE port map (clkcounta(5),clkcounta_T(5),XSTALIN,'0','0');
clkcounta_T(5) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(5))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(5))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3) AND clkcounta(4))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4)));

FTCPE_clkcounta6: FTCPE port map (clkcounta(6),clkcounta_T(6),XSTALIN,'0','0');
clkcounta_T(6) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(6))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(6))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND 
	clkcounta(5)));

FTCPE_clkcounta7: FTCPE port map (clkcounta(7),clkcounta_T(7),XSTALIN,'0','0');
clkcounta_T(7) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(7))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(7))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND 
	clkcounta(6))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND 
	clkcounta(5) AND clkcounta(6)));

FTCPE_clkcounta8: FTCPE port map (clkcounta(8),clkcounta_T(8),XSTALIN,'0','0');
clkcounta_T(8) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(8))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(8))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND 
	clkcounta(6) AND clkcounta(7))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND 
	clkcounta(5) AND clkcounta(6) AND clkcounta(7)));

FTCPE_clkcounta9: FTCPE port map (clkcounta(9),clkcounta_T(9),XSTALIN,'0','0');
clkcounta_T(9) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(9))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(9))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND 
	clkcounta(6) AND clkcounta(7) AND clkcounta(8))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND 
	clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND clkcounta(8)));

FTCPE_clkcounta10: FTCPE port map (clkcounta(10),clkcounta_T(10),XSTALIN,'0','0');
clkcounta_T(10) <= ((alreadystoredcnt(0) AND resetclk(0) AND 
	clkcounta(10))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(10))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND 
	clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND 
	clkcounta(6) AND clkcounta(7) AND clkcounta(8) AND clkcounta(9))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND 
	clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND clkcounta(8) AND 
	clkcounta(9)));

FTCPE_clkcounta11: FTCPE port map (clkcounta(11),clkcounta_T(11),XSTALIN,'0','0');
clkcounta_T(11) <= ((alreadystoredcnt(0) AND resetclk(0) AND 
	clkcounta(11))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(11))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(10) AND 
	clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND 
	clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND clkcounta(8) AND 
	clkcounta(9))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(10) AND clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND 
	clkcounta(4) AND clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND 
	clkcounta(8) AND clkcounta(9)));

FTCPE_clkcounta12: FTCPE port map (clkcounta(12),clkcounta_T(12),XSTALIN,'0','0');
clkcounta_T(12) <= ((alreadystoredcnt(0) AND resetclk(0) AND 
	clkcounta(12))
	OR (resetclk(0) AND NOT HZIN AND clkcounta(12))
	OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(10) AND 
	clkcounta(11) AND clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND 
	clkcounta(4) AND clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND 
	clkcounta(8) AND clkcounta(9))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND 
	clkcounta(10) AND clkcounta(11) AND clkcounta(1) AND clkcounta(2) AND 
	clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND clkcounta(6) AND 
	clkcounta(7) AND clkcounta(8) AND clkcounta(9)));

FDCPE_resetclk0: FDCPE port map (resetclk(0),resetclk_D(0),XSTALIN,'0','0');
resetclk_D(0) <= (NOT alreadystoredcnt(0) AND HZIN);

FDCPE_storecounta1: FDCPE port map (storecounta(1),storecounta_D(1),XSTALIN,'0','0');
storecounta_D(1) <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND NOT resetclk(0) AND storecounta(2))
	OR (NOT LED(6) AND NOT resetclk(0) AND storecounta(1))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND storecounta(2) AND 
	HZIN)
	OR (NOT LED(6) AND NOT alreadystoredcnt(0) AND storecounta(1) AND 
	HZIN));

FDCPE_storecounta2: FDCPE port map (storecounta(2),storecounta_D(2),XSTALIN,'0','0');
storecounta_D(2) <= ((NOT LED(6) AND storecounta(2))
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	uartskip(0) AND NOT HZIN)
	OR (LED(6) AND storecounta(3))
	OR (alreadystoredcnt(0) AND resetclk(0))
	OR (resetclk(0) AND NOT HZIN));

FDCPE_storecounta3: FDCPE port map (storecounta(3),storecounta_D(3),XSTALIN,'0','0');
storecounta_D(3) <= ((NOT LED(6) AND alreadystoredcnt(0) AND storecounta(3))
	OR (NOT LED(6) AND storecounta(3) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(4))
	OR (LED(6) AND storecounta(4) AND NOT HZIN)
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0)));

FDCPE_storecounta4: FDCPE port map (storecounta(4),storecounta_D(4),XSTALIN,'0','0');
storecounta_D(4) <= ((NOT LED(6) AND storecounta(4) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(5))
	OR (LED(6) AND storecounta(5) AND NOT HZIN)
	OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(4))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(1)));

FDCPE_storecounta5: FDCPE port map (storecounta(5),storecounta_D(5),XSTALIN,'0','0');
storecounta_D(5) <= ((NOT LED(6) AND alreadystoredcnt(0) AND storecounta(5))
	OR (NOT LED(6) AND storecounta(5) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(6))
	OR (LED(6) AND storecounta(6) AND NOT HZIN)
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(2)));

FDCPE_storecounta6: FDCPE port map (storecounta(6),storecounta_D(6),XSTALIN,'0','0');
storecounta_D(6) <= ((NOT LED(6) AND storecounta(6) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND LED(0) AND alreadystoredcnt(0))
	OR (LED(6) AND LED(0) AND NOT HZIN)
	OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(6))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(3)));

FDCPE_storecounta13: FDCPE port map (storecounta(13),storecounta_D(13),XSTALIN,'0','0');
storecounta_D(13) <= ((NOT LED(6) AND storecounta(13) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(14))
	OR (LED(6) AND storecounta(14) AND NOT HZIN)
	OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(13))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(10)));

FDCPE_storecounta14: FDCPE port map (storecounta(14),storecounta_D(14),XSTALIN,'0','0');
storecounta_D(14) <= ((NOT LED(6) AND alreadystoredcnt(0) AND storecounta(14))
	OR (NOT LED(6) AND storecounta(14) AND NOT HZIN)
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(11))
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(15))
	OR (LED(6) AND storecounta(15) AND NOT HZIN));

FDCPE_storecounta15: FDCPE port map (storecounta(15),storecounta_D(15),XSTALIN,'0','0');
storecounta_D(15) <= ((NOT LED(6) AND storecounta(15) AND NOT HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND alreadystoredcnt(0) AND storecounta(16))
	OR (LED(6) AND storecounta(16) AND NOT HZIN)
	OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(15))
	OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(12)));

FDCPE_storecounta16: FDCPE port map (storecounta(16),storecounta_D(16),XSTALIN,'0','0');
storecounta_D(16) <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	uartskip(0) AND NOT HZIN)
	OR (LED(6) AND storecounta(17))
	OR (NOT LED(6) AND storecounta(16))
	OR (alreadystoredcnt(0) AND resetclk(0))
	OR (resetclk(0) AND NOT HZIN));

FDCPE_storecounta17: FDCPE port map (storecounta(17),storecounta_D(17),XSTALIN,'0','0');
storecounta_D(17) <= ((NOT LED(6) AND NOT alreadystoredcnt(0) AND storecounta(17) AND 
	HZIN)
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
	OR (LED(6) AND NOT resetclk(0) AND storecounta(18))
	OR (NOT LED(6) AND NOT resetclk(0) AND storecounta(17))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND storecounta(18) AND 
	HZIN));

FDCPE_storecounta18: FDCPE port map (storecounta(18),storecounta_D(18),XSTALIN,'0','0');
storecounta_D(18) <= ((LED(6) AND NOT alreadystoredcnt(0) AND HZIN)
	OR (NOT alreadystoredcnt(0) AND storecounta(18) AND HZIN)
	OR (LED(7) AND alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartskip(0) AND NOT HZIN)
	OR (LED(6) AND NOT resetclk(0))
	OR (NOT resetclk(0) AND storecounta(18)));

FTCPE_uartctr0: FTCPE port map (uartctr(0),uartctr_T(0),XSTALIN,'0','0');
uartctr_T(0) <= ((LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND 
	uartctr(4) AND NOT HZIN));

FTCPE_uartctr1: FTCPE port map (uartctr(1),uartctr_T(1),XSTALIN,'0','0');
uartctr_T(1) <= ((NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND uartctr(0))
	OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND 
	uartctr(4) AND NOT HZIN));

FTCPE_uartctr2: FTCPE port map (uartctr(2),uartctr_T(2),XSTALIN,'0','0');
uartctr_T(2) <= ((NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1))
	OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND 
	uartctr(4) AND NOT HZIN));

FTCPE_uartctr3: FTCPE port map (uartctr(3),uartctr_T(3),XSTALIN,'0','0');
uartctr_T(3) <= ((NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1) AND 
	uartctr(2))
	OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND 
	uartctr(4) AND NOT HZIN));

FTCPE_uartctr4: FTCPE port map (uartctr(4),uartctr_T(4),XSTALIN,'0','0');
uartctr_T(4) <= ((LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND 
	uartctr(3) AND uartctr(4))
	OR (NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1) AND 
	uartctr(2) AND uartctr(3))
	OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND 
	uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND 
	uartctr(4) AND NOT HZIN));

FTCPE_uartskip0: FTCPE port map (uartskip(0),uartskip_T(0),XSTALIN,'0','0');
uartskip_T(0) <= ((NOT LED(7) AND alreadystoredcnt(0) AND NOT resetclk(0) AND 
	NOT uartskip(0))
	OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND 
	NOT resetclk(0) AND uartskip(0) AND NOT HZIN));

Register Legend:
 FDCPE (Q,D,C,CLR,PRE,CE); 
 FTCPE (Q,D,C,CLR,PRE,CE); 
 LDCP  (Q,D,G,CLR,PRE); 

******************************  Device Pin Out *****************************

Device : XC9572XL-5-VQ44


   --------------------------------  
  /44 43 42 41 40 39 38 37 36 35 34 \
 | 1                             33 | 
 | 2                             32 | 
 | 3                             31 | 
 | 4                             30 | 
 | 5         XC9572XL-5-VQ44     29 | 
 | 6                             28 | 
 | 7                             27 | 
 | 8                             26 | 
 | 9                             25 | 
 | 10                            24 | 
 | 11                            23 | 
 \ 12 13 14 15 16 17 18 19 20 21 22 /
   --------------------------------  


Pin Signal                         Pin Signal                        
No. Name                           No. Name                          
  1 LED<4>                           23 KPR                           
  2 LED<5>                           24 TDO                           
  3 LED<6>                           25 GND                           
  4 GND                              26 VCC                           
  5 LED<7>                           27 KPR                           
  6 TX                               28 KPR                           
  7 KPR                              29 KPR                           
  8 KPR                              30 KPR                           
  9 TDI                              31 KPR                           
 10 TMS                              32 KPR                           
 11 TCK                              33 KPR                           
 12 KPR                              34 KPR                           
 13 KPR                              35 VCC                           
 14 KPR                              36 KPR                           
 15 VCC                              37 KPR                           
 16 KPR                              38 KPR                           
 17 GND                              39 KPR                           
 18 KPR                              40 KPR                           
 19 KPR                              41 LED<0>                        
 20 XSTALIN                          42 LED<1>                        
 21 HZIN                             43 LED<2>                        
 22 KPR                              44 LED<3>                        


Legend :  NC  = Not Connected, unbonded pin
         PGND = Unused I/O configured as additional Ground pin
         TIE  = Unused I/O floating -- must tie to VCC, GND or other signal
         KPR  = Unused I/O with weak keeper (leave unconnected)
         VCC  = Dedicated Power Pin
         GND  = Dedicated Ground Pin
         TDI  = Test Data In, JTAG pin
         TDO  = Test Data Out, JTAG pin
         TCK  = Test Clock, JTAG pin
         TMS  = Test Mode Select, JTAG pin
  PROHIBITED  = User reserved pin
****************************  Compiler Options  ****************************

Following is a list of all global compiler options used by the fitter run.

Device(s) Specified                         : xc9572xl-5-VQ44
Optimization Method                         : SPEED
Multi-Level Logic Optimization              : ON
Ignore Timing Specifications                : OFF
Default Register Power Up Value             : LOW
Keep User Location Constraints              : ON
What-You-See-Is-What-You-Get                : OFF
Exhaustive Fitting                          : OFF
Keep Unused Inputs                          : OFF
Slew Rate                                   : FAST
Power Mode                                  : STD
Ground on Unused IOs                        : OFF
Set I/O Pin Termination                     : KEEPER
Global Clock Optimization                   : ON
Global Set/Reset Optimization               : ON
Global Ouput Enable Optimization            : ON
Input Limit                                 : 54
Pterm Limit                                 : 25
