ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           Atmel AVR 8-bit microcontroller
  Version:                           0x1
  Entry point address:               0x0
  Start of program headers:          52 (bytes into file)
  Start of section headers:          37220 (bytes into file)
  Flags:                             0x5, avr:5
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         3
  Size of section headers:           40 (bytes)
  Number of section headers:         17
  Section header string table index: 14

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] .data             PROGBITS        00800100 000fe8 000016 00  WA  0   0  1
  [ 2] .text             PROGBITS        00000000 000094 000f54 00  AX  0   0  2
  [ 3] .bss              NOBITS          00800116 000ffe 000126 00  WA  0   0  1
  [ 4] .comment          PROGBITS        00000000 000ffe 000011 01  MS  0   0  1
  [ 5] .note.gnu.avr.dev NOTE            00000000 001010 000040 00      0   0  4
  [ 6] .debug_aranges    PROGBITS        00000000 001050 000030 00      0   0  1
  [ 7] .debug_info       PROGBITS        00000000 001080 002eb4 00      0   0  1
  [ 8] .debug_abbrev     PROGBITS        00000000 003f34 000b61 00      0   0  1
  [ 9] .debug_line       PROGBITS        00000000 004a95 000b3d 00      0   0  1
  [10] .debug_frame      PROGBITS        00000000 0055d4 0003cc 00      0   0  4
  [11] .debug_str        PROGBITS        00000000 0059a0 000a88 00      0   0  1
  [12] .debug_loc        PROGBITS        00000000 006428 001a3f 00      0   0  1
  [13] .debug_ranges     PROGBITS        00000000 007e67 0000e0 00      0   0  1
  [14] .shstrtab         STRTAB          00000000 0090ae 0000b4 00      0   0  1
  [15] .symtab           SYMTAB          00000000 007f48 000940 10     16  81  4
  [16] .strtab           STRTAB          00000000 008888 000826 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  p (processor specific)

There are no section groups in this file.

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  LOAD           0x000094 0x00000000 0x00000000 0x00f54 0x00f54 R E 0x2
  LOAD           0x000fe8 0x00800100 0x00000f54 0x00016 0x00016 RW  0x1
  LOAD           0x000ffe 0x00800116 0x00800116 0x00000 0x00126 RW  0x1

 Section to Segment mapping:
  Segment Sections...
   00     .text 
   01     .data 
   02     .bss 

There is no dynamic section in this file.

There are no relocations in this file.

The decoding of unwind sections for machine type Atmel AVR 8-bit microcontroller is not currently supported.

Symbol table '.symtab' contains 148 entries:
   Num:    Value  Size Type    Bind   Vis      Ndx Name
     0: 00000000     0 NOTYPE  LOCAL  DEFAULT  UND 
     1: 00800100     0 SECTION LOCAL  DEFAULT    1 
     2: 00000000     0 SECTION LOCAL  DEFAULT    2 
     3: 00800116     0 SECTION LOCAL  DEFAULT    3 
     4: 00000000     0 SECTION LOCAL  DEFAULT    4 
     5: 00000000     0 SECTION LOCAL  DEFAULT    5 
     6: 00000000     0 SECTION LOCAL  DEFAULT    6 
     7: 00000000     0 SECTION LOCAL  DEFAULT    7 
     8: 00000000     0 SECTION LOCAL  DEFAULT    8 
     9: 00000000     0 SECTION LOCAL  DEFAULT    9 
    10: 00000000     0 SECTION LOCAL  DEFAULT   10 
    11: 00000000     0 SECTION LOCAL  DEFAULT   11 
    12: 00000000     0 SECTION LOCAL  DEFAULT   12 
    13: 00000000     0 SECTION LOCAL  DEFAULT   13 
    14: 00000000     0 FILE    LOCAL  DEFAULT  ABS 
    15: 0000003e     0 NOTYPE  LOCAL  DEFAULT  ABS __SP_H__
    16: 0000003d     0 NOTYPE  LOCAL  DEFAULT  ABS __SP_L__
    17: 0000003f     0 NOTYPE  LOCAL  DEFAULT  ABS __SREG__
    18: 00000000     0 NOTYPE  LOCAL  DEFAULT  ABS __tmp_reg__
    19: 00000001     0 NOTYPE  LOCAL  DEFAULT  ABS __zero_reg__
    20: 00000198    86 FUNC    LOCAL  DEFAULT    2 _ZN5Print5writeEPKhj
    21: 000001ee     2 FUNC    LOCAL  DEFAULT    2 _ZN5Print5flushEv
    22: 000001f0     6 FUNC    LOCAL  DEFAULT    2 _ZN5Print17availableForWr
    23: 000001f6    30 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial17avai
    24: 00000214    40 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial4readE
    25: 0000023c    28 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial4peekE
    26: 00000258    24 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial9avail
    27: 00000270    20 FUNC    LOCAL  DEFAULT    2 _Z17Serial0_availablev
    28: 00800147   157 OBJECT  LOCAL  DEFAULT    3 Serial
    29: 00000284    66 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial17_tx_
    30: 000002c6   142 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial5write
    31: 00000354    68 FUNC    LOCAL  DEFAULT    2 _ZN14HardwareSerial5flush
    32: 00000398    20 FUNC    LOCAL  DEFAULT    2 _Z14serialEventRunv
    33: 000003ac    82 FUNC    LOCAL  DEFAULT    2 turnOffPWM
    34: 000003fe    82 FUNC    LOCAL  DEFAULT    2 digitalRead
    35: 000000ae    20 OBJECT  LOCAL  DEFAULT    2 digital_pin_to_timer_PGM
    36: 0000009a    20 OBJECT  LOCAL  DEFAULT    2 digital_pin_to_bit_mask_P
    37: 00000086    20 OBJECT  LOCAL  DEFAULT    2 digital_pin_to_port_PGM
    38: 0000007c    10 OBJECT  LOCAL  DEFAULT    2 port_to_input_PGM
    39: 00000450    96 FUNC    LOCAL  DEFAULT    2 digitalWrite
    40: 00000072    10 OBJECT  LOCAL  DEFAULT    2 port_to_output_PGM
    41: 000004b0   120 FUNC    LOCAL  DEFAULT    2 pinMode
    42: 00000068    10 OBJECT  LOCAL  DEFAULT    2 port_to_mode_PGM
    43: 00000528    74 FUNC    LOCAL  DEFAULT    2 micros
    44: 0080011d     4 OBJECT  LOCAL  DEFAULT    3 timer0_overflow_count
    45: 00000572   104 FUNC    LOCAL  DEFAULT    2 _Z14checkCLKandBINv
    46: 00800116     1 OBJECT  LOCAL  DEFAULT    3 hzclkval
    47: 00800117     1 OBJECT  LOCAL  DEFAULT    3 readyet
    48: 00800146     1 OBJECT  LOCAL  DEFAULT    3 clkval
    49: 00800123    30 OBJECT  LOCAL  DEFAULT    3 hzbinval
    50: 000005da   270 FUNC    LOCAL  DEFAULT    2 _ZN10LedControl11spiTrans
    51: 000006e8    60 FUNC    LOCAL  DEFAULT    2 _ZN10LedControl8setDigitE
    52: 008001e4    88 OBJECT  LOCAL  DEFAULT    3 lc
    53: 000000c2   128 OBJECT  LOCAL  DEFAULT    2 _ZL9charTable
    54: 00000724   108 FUNC    LOCAL  DEFAULT    2 _ZN10LedControl12clearDis
    55: 00000790    36 FUNC    LOCAL  DEFAULT    2 _ZN5Print5writeEPKc.const
    56: 000007b4   130 FUNC    LOCAL  DEFAULT    2 _ZN5Print11printNumberEmh
    57: 00000836     4 FUNC    LOCAL  DEFAULT    2 __cxa_pure_virtual
    58: 0000097e   374 FUNC    LOCAL  DEFAULT    2 _GLOBAL__I_65535_0_shifti
    59: 00800100    18 OBJECT  LOCAL  DEFAULT    1 _ZTV14HardwareSerial
    60: 00800142     2 OBJECT  LOCAL  DEFAULT    3 bitfieldA
    61: 00800141     1 OBJECT  LOCAL  DEFAULT    3 x
    62: 00800121     2 OBJECT  LOCAL  DEFAULT    3 temp
    63: 00800144     2 OBJECT  LOCAL  DEFAULT    3 mainsfreq
    64: 00800119     4 OBJECT  LOCAL  DEFAULT    3 timer0_millis
    65: 00800118     1 OBJECT  LOCAL  DEFAULT    3 timer0_fract
    66: 00000000     0 FILE    LOCAL  DEFAULT  ABS _clear_bss.o
    67: 00000170     0 NOTYPE  LOCAL  DEFAULT    2 .do_clear_bss_start
    68: 0000016e     0 NOTYPE  LOCAL  DEFAULT    2 .do_clear_bss_loop
    69: 00000000     0 FILE    LOCAL  DEFAULT  ABS _divmodhi4.o
    70: 00000ebe     0 NOTYPE  LOCAL  DEFAULT    2 __divmodhi4_neg1
    71: 00000ec6     0 NOTYPE  LOCAL  DEFAULT    2 __divmodhi4_neg2
    72: 00000ecc     0 NOTYPE  LOCAL  DEFAULT    2 __divmodhi4_exit
    73: 00000000     0 FILE    LOCAL  DEFAULT  ABS _udivmodsi4.o
    74: 00000ef4     0 NOTYPE  LOCAL  DEFAULT    2 __udivmodsi4_ep
    75: 00000eda     0 NOTYPE  LOCAL  DEFAULT    2 __udivmodsi4_loop
    76: 00000000     0 FILE    LOCAL  DEFAULT  ABS _udivmodhi4.o
    77: 00000f28     0 NOTYPE  LOCAL  DEFAULT    2 __udivmodhi4_ep
    78: 00000f1a     0 NOTYPE  LOCAL  DEFAULT    2 __udivmodhi4_loop
    79: 00000000     0 FILE    LOCAL  DEFAULT  ABS _exit.o
    80: 00000f52     0 NOTYPE  LOCAL  DEFAULT    2 __stop_program
    81: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_22
    82: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_1
    83: 0000ffa0     0 NOTYPE  GLOBAL DEFAULT  ABS __DATA_REGION_LENGTH__
    84: 00000f12    40 NOTYPE  GLOBAL HIDDEN     2 __udivmodhi4
    85: 00000068     0 NOTYPE  GLOBAL DEFAULT    2 __trampolines_start
    86: 00000f54     0 NOTYPE  GLOBAL DEFAULT    2 _etext
    87: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_24
    88: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_12
    89: 00000194     0 NOTYPE  GLOBAL DEFAULT    2 __bad_interrupt
    90: 00000f6a     0 NOTYPE  GLOBAL DEFAULT  ABS __data_load_end
    91: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_6
    92: 00000068     0 NOTYPE  GLOBAL DEFAULT    2 __trampolines_end
    93: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_3
    94: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_23
    95: 00000f54     0 NOTYPE  GLOBAL DEFAULT  ABS __data_load_start
    96: 00000144     0 NOTYPE  GLOBAL DEFAULT    2 __dtors_end
    97: 0080023c     0 NOTYPE  GLOBAL DEFAULT    3 __bss_end
    98: 00000400     0 NOTYPE  GLOBAL DEFAULT  ABS __LOCK_REGION_LENGTH__
    99: 00000f46    10 FUNC    GLOBAL DEFAULT    2 abort
   100: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_25
   101: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_11
   102: 00000144     0 NOTYPE  WEAK   DEFAULT    2 __init
   103: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_13
   104: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_17
   105: 0000083a    76 FUNC    GLOBAL DEFAULT    2 __vector_19
   106: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_7
   107: 00000166    16 NOTYPE  GLOBAL HIDDEN     2 __do_clear_bss
   108: 00810000     0 NOTYPE  GLOBAL DEFAULT    4 __eeprom_end
   109: 00000000     0 NOTYPE  WEAK   DEFAULT  UND _Z11serialEventv
   110: 00000000     0 NOTYPE  GLOBAL DEFAULT    2 __vectors
   111: 00800116     0 NOTYPE  GLOBAL DEFAULT    1 __data_end
   112: 00000000     0 NOTYPE  WEAK   DEFAULT    2 __vector_default
   113: 00000ea6    40 NOTYPE  GLOBAL HIDDEN     2 __divmodhi4
   114: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_5
   115: 00000400     0 NOTYPE  GLOBAL DEFAULT  ABS __SIGNATURE_REGION_LENGTH
   116: 00000f3a    12 NOTYPE  GLOBAL HIDDEN     2 __tablejump2__
   117: 00000142     0 NOTYPE  GLOBAL DEFAULT    2 __ctors_start
   118: 00000150    22 NOTYPE  GLOBAL HIDDEN     2 __do_copy_data
   119: 00800116     0 NOTYPE  GLOBAL DEFAULT    3 __bss_start
   120: 00000af4   946 FUNC    GLOBAL DEFAULT    2 main
   121: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_4
   122: 00000000     0 NOTYPE  WEAK   DEFAULT  ABS __heap_end
   123: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_9
   124: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_2
   125: 00000400     0 NOTYPE  GLOBAL DEFAULT  ABS __USER_SIGNATURE_REGION_L
   126: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_21
   127: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_15
   128: 00000144     0 NOTYPE  GLOBAL DEFAULT    2 __dtors_start
   129: 00000144     0 NOTYPE  GLOBAL DEFAULT    2 __ctors_end
   130: 000008ff     0 NOTYPE  WEAK   DEFAULT  ABS __stack
   131: 00800116     0 NOTYPE  GLOBAL DEFAULT    1 _edata
   132: 0080023c     0 NOTYPE  GLOBAL DEFAULT    4 _end
   133: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_8
   134: 00000f50     0 NOTYPE  WEAK   HIDDEN     2 exit
   135: 00000ea6     0 NOTYPE  GLOBAL HIDDEN     2 _div
   136: 00000ece    68 NOTYPE  GLOBAL HIDDEN     2 __udivmodsi4
   137: 00010000     0 NOTYPE  GLOBAL DEFAULT  ABS __EEPROM_REGION_LENGTH__
   138: 00000f50     0 NOTYPE  GLOBAL HIDDEN     2 _exit
   139: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_14
   140: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_10
   141: 000008ea   148 FUNC    GLOBAL DEFAULT    2 __vector_16
   142: 00800100     0 NOTYPE  GLOBAL DEFAULT    1 __data_start
   143: 00000886   100 FUNC    GLOBAL DEFAULT    2 __vector_18
   144: 00000003     0 NOTYPE  GLOBAL DEFAULT  ABS __FUSE_REGION_LENGTH__
   145: 00020000     0 NOTYPE  GLOBAL DEFAULT  ABS __TEXT_REGION_LENGTH__
   146: 00000194     0 NOTYPE  WEAK   DEFAULT    2 __vector_20
   147: 00000176    22 NOTYPE  GLOBAL HIDDEN     2 __do_global_ctors

No version information found in this file.

Displaying notes found in: .note.gnu.avr.deviceinfo
  Owner                 Data size	Description
  AVR                  0x0000002d	NT_VERSION (version)
   description data: 00 00 00 00 00 ffffff80 00 00 00 01 00 00 00 08 00 00 00 00 00 00 00 04 00 00 08 00 00 00 01 00 00 00 00 61 74 6d 65 67 61 33 32 38 70 00 00 
