### Equations

********** Mapped Logic **********

FDCPE_LED0: FDCPE port map (LED(0),LED_D(0),XSTALIN,'0','0');
LED_D(0) <= ((NOT LED(6) AND LED(0) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND LED(1) AND alreadystoredcnt(0))
OR (LED(6) AND LED(1) AND NOT HZIN)
OR (NOT LED(6) AND LED(0) AND alreadystoredcnt(0))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(4)));

FDCPE_LED1: FDCPE port map (LED(1),LED_D(1),XSTALIN,'0','0');
LED_D(1) <= ((NOT LED(6) AND LED(1) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND LED(2) AND alreadystoredcnt(0))
OR (LED(6) AND LED(2) AND NOT HZIN)
OR (NOT LED(6) AND LED(1) AND alreadystoredcnt(0))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(5)));

FDCPE_LED2: FDCPE port map (LED(2),LED_D(2),XSTALIN,'0','0');
LED_D(2) <= ((NOT LED(6) AND LED(2) AND alreadystoredcnt(0))
OR (NOT LED(6) AND LED(2) AND NOT HZIN)
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(6))
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND LED(3) AND alreadystoredcnt(0))
OR (LED(6) AND LED(3) AND NOT HZIN));

FDCPE_LED3: FDCPE port map (LED(3),LED_D(3),XSTALIN,'0','0');
LED_D(3) <= ((NOT LED(6) AND LED(3) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND LED(4) AND alreadystoredcnt(0))
OR (LED(6) AND LED(4) AND NOT HZIN)
OR (NOT LED(6) AND LED(3) AND alreadystoredcnt(0))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(7)));

FDCPE_LED4: FDCPE port map (LED(4),LED_D(4),XSTALIN,'0','0');
LED_D(4) <= ((NOT LED(6) AND LED(4) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND LED(5) AND alreadystoredcnt(0))
OR (LED(6) AND LED(5) AND NOT HZIN)
OR (NOT LED(6) AND LED(4) AND alreadystoredcnt(0))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(8)));

FDCPE_LED5: FDCPE port map (LED(5),LED_D(5),XSTALIN,'0','0');
LED_D(5) <= ((NOT LED(6) AND LED(5) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(13))
OR (LED(6) AND storecounta(13) AND NOT HZIN)
OR (NOT LED(6) AND LED(5) AND alreadystoredcnt(0))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(9)));

FTCPE_LED6: FTCPE port map (LED(6),LED_T(6),XSTALIN,'0','0');
LED_T(6) <= ((NOT LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND NOT uartskip(0))
OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (LED(6) AND alreadystoredcnt(0) AND NOT resetclk(0) AND
uartskip(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND
uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND
uartctr(4) AND NOT HZIN));

FTCPE_LED7: FTCPE port map (LED(7),LED_T(7),XSTALIN,'0','0');
LED_T(7) <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1) AND
uartctr(2) AND uartctr(3) AND uartctr(4))
OR (NOT LED(7) AND LED(6) AND NOT alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4) AND NOT HZIN));

FDCPE_TX: FDCPE port map (TX,TX_D,XSTALIN,'0','0'); TX_D <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND NOT resetclk(0) AND uartskip(0) AND NOT HZIN) OR (LED(6) AND NOT resetclk(0) AND storecounta(1)) OR (NOT LED(6) AND NOT resetclk(0) AND TX) OR (LED(6) AND NOT alreadystoredcnt(0) AND storecounta(1) AND HZIN) OR (NOT LED(6) AND NOT alreadystoredcnt(0) AND HZIN AND TX));
FDCPE_alreadystoredcnt0: FDCPE port map (alreadystoredcnt(0),alreadystoredcnt_D(0),XSTALIN,'0','0'); alreadystoredcnt_D(0) <= ((LED(7) AND NOT LED(6) AND NOT resetclk(0) AND uartskip(0) AND NOT HZIN) OR (NOT alreadystoredcnt(0) AND NOT HZIN));
FDCPE_clkcounta0: FDCPE port map (clkcounta(0),clkcounta_D(0),XSTALIN,'0','0'); clkcounta_D(0) <= ((NOT resetclk(0) AND NOT clkcounta(0)) OR (NOT alreadystoredcnt(0) AND HZIN AND NOT clkcounta(0)));
FDCPE_clkcounta1: FDCPE port map (clkcounta(1),clkcounta_D(1),XSTALIN,'0','0'); clkcounta_D(1) <= ((NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND NOT clkcounta(1)) OR (NOT alreadystoredcnt(0) AND HZIN AND NOT clkcounta(0) AND clkcounta(1)) OR (NOT resetclk(0) AND clkcounta(0) AND NOT clkcounta(1)) OR (NOT resetclk(0) AND NOT clkcounta(0) AND clkcounta(1)));
FTCPE_clkcounta2: FTCPE port map (clkcounta(2),clkcounta_T(2),XSTALIN,'0','0'); clkcounta_T(2) <= ((NOT resetclk(0) AND clkcounta(0) AND clkcounta(1)) OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND clkcounta(1)) OR (alreadystoredcnt(0) AND resetclk(0) AND clkcounta(2)) OR (resetclk(0) AND NOT HZIN AND clkcounta(2)));
FTCPE_clkcounta3: FTCPE port map (clkcounta(3),clkcounta_T(3),XSTALIN,'0','0'); clkcounta_T(3) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(3)) OR (resetclk(0) AND NOT HZIN AND clkcounta(3)) OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND clkcounta(2)) OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND clkcounta(1) AND clkcounta(2)));
FTCPE_clkcounta4: FTCPE port map (clkcounta(4),clkcounta_T(4),XSTALIN,'0','0'); clkcounta_T(4) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(4)) OR (resetclk(0) AND NOT HZIN AND clkcounta(4)) OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND clkcounta(2) AND clkcounta(3)) OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND clkcounta(1) AND clkcounta(2) AND clkcounta(3)));

FTCPE_clkcounta5: FTCPE port map (clkcounta(5),clkcounta_T(5),XSTALIN,'0','0');
clkcounta_T(5) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(5))
OR (resetclk(0) AND NOT HZIN AND clkcounta(5))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND
clkcounta(2) AND clkcounta(3) AND clkcounta(4))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4)));

FTCPE_clkcounta6: FTCPE port map (clkcounta(6),clkcounta_T(6),XSTALIN,'0','0');
clkcounta_T(6) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(6))
OR (resetclk(0) AND NOT HZIN AND clkcounta(6))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND
clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND
clkcounta(5)));

FTCPE_clkcounta7: FTCPE port map (clkcounta(7),clkcounta_T(7),XSTALIN,'0','0');
clkcounta_T(7) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(7))
OR (resetclk(0) AND NOT HZIN AND clkcounta(7))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND
clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND
clkcounta(6))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND
clkcounta(5) AND clkcounta(6)));

FTCPE_clkcounta8: FTCPE port map (clkcounta(8),clkcounta_T(8),XSTALIN,'0','0');
clkcounta_T(8) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(8))
OR (resetclk(0) AND NOT HZIN AND clkcounta(8))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND
clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND
clkcounta(6) AND clkcounta(7))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND
clkcounta(5) AND clkcounta(6) AND clkcounta(7)));

FTCPE_clkcounta9: FTCPE port map (clkcounta(9),clkcounta_T(9),XSTALIN,'0','0');
clkcounta_T(9) <= ((alreadystoredcnt(0) AND resetclk(0) AND clkcounta(9))
OR (resetclk(0) AND NOT HZIN AND clkcounta(9))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND
clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND
clkcounta(6) AND clkcounta(7) AND clkcounta(8))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND
clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND clkcounta(8)));

FTCPE_clkcounta10: FTCPE port map (clkcounta(10),clkcounta_T(10),XSTALIN,'0','0');
clkcounta_T(10) <= ((alreadystoredcnt(0) AND resetclk(0) AND
clkcounta(10))
OR (resetclk(0) AND NOT HZIN AND clkcounta(10))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(1) AND
clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND
clkcounta(6) AND clkcounta(7) AND clkcounta(8) AND clkcounta(9))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND
clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND clkcounta(8) AND
clkcounta(9)));

FTCPE_clkcounta11: FTCPE port map (clkcounta(11),clkcounta_T(11),XSTALIN,'0','0');
clkcounta_T(11) <= ((alreadystoredcnt(0) AND resetclk(0) AND
clkcounta(11))
OR (resetclk(0) AND NOT HZIN AND clkcounta(11))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(10) AND
clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND clkcounta(4) AND
clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND clkcounta(8) AND
clkcounta(9))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(10) AND clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND
clkcounta(4) AND clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND
clkcounta(8) AND clkcounta(9)));

FTCPE_clkcounta12: FTCPE port map (clkcounta(12),clkcounta_T(12),XSTALIN,'0','0');
clkcounta_T(12) <= ((alreadystoredcnt(0) AND resetclk(0) AND
clkcounta(12))
OR (resetclk(0) AND NOT HZIN AND clkcounta(12))
OR (NOT resetclk(0) AND clkcounta(0) AND clkcounta(10) AND
clkcounta(11) AND clkcounta(1) AND clkcounta(2) AND clkcounta(3) AND
clkcounta(4) AND clkcounta(5) AND clkcounta(6) AND clkcounta(7) AND
clkcounta(8) AND clkcounta(9))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0) AND
clkcounta(10) AND clkcounta(11) AND clkcounta(1) AND clkcounta(2) AND
clkcounta(3) AND clkcounta(4) AND clkcounta(5) AND clkcounta(6) AND
clkcounta(7) AND clkcounta(8) AND clkcounta(9)));

FDCPE_resetclk0: FDCPE port map (resetclk(0),resetclk_D(0),XSTALIN,'0','0'); resetclk_D(0) <= (NOT alreadystoredcnt(0) AND HZIN);

FDCPE_storecounta1: FDCPE port map (storecounta(1),storecounta_D(1),XSTALIN,'0','0');
storecounta_D(1) <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND NOT resetclk(0) AND storecounta(2))
OR (NOT LED(6) AND NOT resetclk(0) AND storecounta(1))
OR (LED(6) AND NOT alreadystoredcnt(0) AND storecounta(2) AND
HZIN)
OR (NOT LED(6) AND NOT alreadystoredcnt(0) AND storecounta(1) AND
HZIN));

FDCPE_storecounta2: FDCPE port map (storecounta(2),storecounta_D(2),XSTALIN,'0','0'); storecounta_D(2) <= ((NOT LED(6) AND storecounta(2)) OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND uartskip(0) AND NOT HZIN) OR (LED(6) AND storecounta(3)) OR (alreadystoredcnt(0) AND resetclk(0)) OR (resetclk(0) AND NOT HZIN));

FDCPE_storecounta3: FDCPE port map (storecounta(3),storecounta_D(3),XSTALIN,'0','0');
storecounta_D(3) <= ((NOT LED(6) AND alreadystoredcnt(0) AND storecounta(3))
OR (NOT LED(6) AND storecounta(3) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(4))
OR (LED(6) AND storecounta(4) AND NOT HZIN)
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(0)));

FDCPE_storecounta4: FDCPE port map (storecounta(4),storecounta_D(4),XSTALIN,'0','0');
storecounta_D(4) <= ((NOT LED(6) AND storecounta(4) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(5))
OR (LED(6) AND storecounta(5) AND NOT HZIN)
OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(4))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(1)));

FDCPE_storecounta5: FDCPE port map (storecounta(5),storecounta_D(5),XSTALIN,'0','0');
storecounta_D(5) <= ((NOT LED(6) AND alreadystoredcnt(0) AND storecounta(5))
OR (NOT LED(6) AND storecounta(5) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(6))
OR (LED(6) AND storecounta(6) AND NOT HZIN)
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(2)));

FDCPE_storecounta6: FDCPE port map (storecounta(6),storecounta_D(6),XSTALIN,'0','0');
storecounta_D(6) <= ((NOT LED(6) AND storecounta(6) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND LED(0) AND alreadystoredcnt(0))
OR (LED(6) AND LED(0) AND NOT HZIN)
OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(6))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(3)));

FDCPE_storecounta13: FDCPE port map (storecounta(13),storecounta_D(13),XSTALIN,'0','0');
storecounta_D(13) <= ((NOT LED(6) AND storecounta(13) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(14))
OR (LED(6) AND storecounta(14) AND NOT HZIN)
OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(13))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(10)));

FDCPE_storecounta14: FDCPE port map (storecounta(14),storecounta_D(14),XSTALIN,'0','0');
storecounta_D(14) <= ((NOT LED(6) AND alreadystoredcnt(0) AND storecounta(14))
OR (NOT LED(6) AND storecounta(14) AND NOT HZIN)
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(11))
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(15))
OR (LED(6) AND storecounta(15) AND NOT HZIN));

FDCPE_storecounta15: FDCPE port map (storecounta(15),storecounta_D(15),XSTALIN,'0','0');
storecounta_D(15) <= ((NOT LED(6) AND storecounta(15) AND NOT HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND alreadystoredcnt(0) AND storecounta(16))
OR (LED(6) AND storecounta(16) AND NOT HZIN)
OR (NOT LED(6) AND alreadystoredcnt(0) AND storecounta(15))
OR (NOT alreadystoredcnt(0) AND HZIN AND clkcounta(12)));

FDCPE_storecounta16: FDCPE port map (storecounta(16),storecounta_D(16),XSTALIN,'0','0'); storecounta_D(16) <= ((LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND uartskip(0) AND NOT HZIN) OR (LED(6) AND storecounta(17)) OR (NOT LED(6) AND storecounta(16)) OR (alreadystoredcnt(0) AND resetclk(0)) OR (resetclk(0) AND NOT HZIN));

FDCPE_storecounta17: FDCPE port map (storecounta(17),storecounta_D(17),XSTALIN,'0','0');
storecounta_D(17) <= ((NOT LED(6) AND NOT alreadystoredcnt(0) AND storecounta(17) AND
HZIN)
OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND NOT HZIN)
OR (LED(6) AND NOT resetclk(0) AND storecounta(18))
OR (NOT LED(6) AND NOT resetclk(0) AND storecounta(17))
OR (LED(6) AND NOT alreadystoredcnt(0) AND storecounta(18) AND
HZIN));

FDCPE_storecounta18: FDCPE port map (storecounta(18),storecounta_D(18),XSTALIN,'0','0'); storecounta_D(18) <= ((LED(6) AND NOT alreadystoredcnt(0) AND HZIN) OR (NOT alreadystoredcnt(0) AND storecounta(18) AND HZIN) OR (LED(7) AND alreadystoredcnt(0) AND NOT resetclk(0) AND uartskip(0) AND NOT HZIN) OR (LED(6) AND NOT resetclk(0)) OR (NOT resetclk(0) AND storecounta(18)));

FTCPE_uartctr0: FTCPE port map (uartctr(0),uartctr_T(0),XSTALIN,'0','0');
uartctr_T(0) <= ((LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0))
OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND
uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND
uartctr(4) AND NOT HZIN));

FTCPE_uartctr1: FTCPE port map (uartctr(1),uartctr_T(1),XSTALIN,'0','0');
uartctr_T(1) <= ((NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND uartctr(0))
OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND
uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND
uartctr(4) AND NOT HZIN));

FTCPE_uartctr2: FTCPE port map (uartctr(2),uartctr_T(2),XSTALIN,'0','0');
uartctr_T(2) <= ((NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1))
OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND
uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND
uartctr(4) AND NOT HZIN));

FTCPE_uartctr3: FTCPE port map (uartctr(3),uartctr_T(3),XSTALIN,'0','0');
uartctr_T(3) <= ((NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1) AND
uartctr(2))
OR (LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND
uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND
uartctr(4) AND NOT HZIN));

FTCPE_uartctr4: FTCPE port map (uartctr(4),uartctr_T(4),XSTALIN,'0','0');
uartctr_T(4) <= ((LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartctr(0) AND uartctr(1) AND uartctr(2) AND
uartctr(3) AND uartctr(4))
OR (NOT LED(7) AND LED(6) AND alreadystoredcnt(0) AND
NOT resetclk(0) AND uartskip(0) AND uartctr(0) AND uartctr(1) AND
uartctr(2) AND uartctr(3))
OR (LED(6) AND NOT alreadystoredcnt(0) AND NOT resetclk(0) AND
uartctr(0) AND uartctr(1) AND uartctr(2) AND uartctr(3) AND
uartctr(4) AND NOT HZIN));

FTCPE_uartskip0: FTCPE port map (uartskip(0),uartskip_T(0),XSTALIN,'0','0'); uartskip_T(0) <= ((NOT LED(7) AND alreadystoredcnt(0) AND NOT resetclk(0) AND NOT uartskip(0)) OR (LED(7) AND NOT LED(6) AND alreadystoredcnt(0) AND NOT resetclk(0) AND uartskip(0) AND NOT HZIN));
Register Legend: FDCPE (Q,D,C,CLR,PRE,CE); FTCPE (Q,D,C,CLR,PRE,CE); LDCP (Q,D,G,CLR,PRE);