(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/FlammableGasSensor/pcb/gassensor.sch)
    (date "Wed 01 May 2019 08:50:48 PM EDT")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source gassensor.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Arduino_Nano_Header)
      (footprint w_conn_misc:arduino_nano_header)
      (libsource (lib w_connectors) (part Arduino_Nano_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9FA3E))
    (comp (ref LS1)
      (value Speaker)
      (footprint w_conn_mkds:mkds_1,5-2)
      (libsource (lib device) (part Speaker))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9FB90))
    (comp (ref CON1)
      (value BARREL_JACK)
      (footprint Connectors:BARREL_JACK)
      (libsource (lib conn) (part BARREL_JACK))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9FDCB))
    (comp (ref P1)
      (value Switcher)
      (footprint pot:SF_STS10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA0146))
    (comp (ref R1)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA0A96))
    (comp (ref RV1)
      (value 100K)
      (footprint pot:Potentiometer_Vishay_TS53YL_Vertical)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA14B5))
    (comp (ref C1)
      (value 10uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA1F5B))
    (comp (ref C2)
      (value 47uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA237B))
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA2D4F))
    (comp (ref D1)
      (value ReverseVoltageDiode)
      (footprint Diodes_THT:Diode_DO-41_SOD81_Horizontal_RM10)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA3E2A))
    (comp (ref D3)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4C40))
    (comp (ref R3)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4CD4))
    (comp (ref D4)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4E2B))
    (comp (ref R4)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4EC1))
    (comp (ref D5)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA572B))
    (comp (ref R5)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5731))
    (comp (ref D6)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5737))
    (comp (ref R6)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA573D))
    (comp (ref D7)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BE1))
    (comp (ref R7)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BE7))
    (comp (ref D8)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BED))
    (comp (ref R8)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BF3))
    (comp (ref D9)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BF9))
    (comp (ref R9)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BFF))
    (comp (ref D10)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5C05))
    (comp (ref R10)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5C0B))
    (comp (ref D2)
      (value PWRLED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA7FCB))
    (comp (ref R2)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA7FD1))
    (comp (ref P4)
      (value Arefbrk)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCAE976))
    (comp (ref P3)
      (value RST_brkout)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCAED2A))
    (comp (ref P8)
      (value SPI_Brkout)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCB5B84))
    (comp (ref P7)
      (value UART)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCB6AC0))
    (comp (ref P6)
      (value MISC_Brkout)
      (footprint Pin_Headers:Pin_Header_Straight_1x03)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCB798F))
    (comp (ref R13)
      (value 200K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCBB5E7))
    (comp (ref RV2)
      (value 1M)
      (footprint pot:Potentiometer_Vishay_TS53YL_Vertical)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCBB715))
    (comp (ref P9)
      (value GasSensorEdgeConnector)
      (footprint pot:EdgeConnectorGasSensorPCB)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCBE214))
    (comp (ref P2)
      (value GasSensor)
      (footprint w_conn_mkds:mkds_1,5-4)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA9BE8))
    (comp (ref MK4)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC47B4))
    (comp (ref MK3)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC48EE))
    (comp (ref MK2)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC4A58))
    (comp (ref MK1)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC4B04)))
  (libparts
    (libpart (lib conn) (part BARREL_JACK)
      (description "DC Barrel Jack")
      (fields
        (field (name Reference) CON)
        (field (name Value) BARREL_JACK))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector, single row, 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X10)
      (description "Connector, single row, 01x10")
      (footprints
        (fp Pin_Header_Straight_1X10)
        (fp Pin_Header_Angled_1X10)
        (fp Socket_Strip_Straight_1X10)
        (fp Socket_Strip_Angled_1X10))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X10))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp Diode_*)
        (fp D-*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentionmeter)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Speaker)
      (description speaker)
      (fields
        (field (name Reference) LS)
        (field (name Value) Speaker))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib mechanical) (part Mounting_Hole)
      (description "Mounting Hole without connection")
      (footprints
        (fp Mounting?Hole*)
        (fp Hole*))
      (fields
        (field (name Reference) MK)
        (field (name Value) Mounting_Hole)))
    (libpart (lib w_connectors) (part Arduino_Nano_Header)
      (fields
        (field (name Reference) J)
        (field (name Value) Arduino_Nano_Header))
      (pins
        (pin (num 1) (name D1/TX) (type passive))
        (pin (num 2) (name D0/RX) (type passive))
        (pin (num 3) (name RESET) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name D2/INT0) (type passive))
        (pin (num 6) (name D3/INT1) (type passive))
        (pin (num 7) (name D4/T0) (type passive))
        (pin (num 8) (name D5/T1) (type passive))
        (pin (num 9) (name D6/AIN0) (type passive))
        (pin (num 10) (name D7/AIN1) (type passive))
        (pin (num 11) (name D8/ICP) (type passive))
        (pin (num 12) (name D9/0C1) (type passive))
        (pin (num 13) (name D10/SS) (type passive))
        (pin (num 14) (name D11/MOSI) (type passive))
        (pin (num 15) (name D12/MISO) (type passive))
        (pin (num 16) (name SCK/D13) (type passive))
        (pin (num 17) (name 3V3) (type passive))
        (pin (num 18) (name AREF) (type passive))
        (pin (num 19) (name A0) (type passive))
        (pin (num 20) (name A1) (type passive))
        (pin (num 21) (name A2) (type passive))
        (pin (num 22) (name A3) (type passive))
        (pin (num 23) (name A4) (type passive))
        (pin (num 24) (name A5) (type passive))
        (pin (num 25) (name A6) (type passive))
        (pin (num 26) (name A7) (type passive))
        (pin (num 27) (name 5V) (type passive))
        (pin (num 28) (name RESET) (type passive))
        (pin (num 29) (name GND) (type passive))
        (pin (num 30) (name VIN) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical mechanical)
      (uri /usr/share/kicad/library/mechanical.lib))
    (library (logical w_connectors)
      (uri /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/FlammableGasSensor/pcb/symbols/w_connectors.lib)))
  (nets
    (net (code 1) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 2) (name VCC)
      (node (ref P1) (pin 1))
      (node (ref J1) (pin 30))
      (node (ref D1) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref F1) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 3) (name /SS)
      (node (ref J1) (pin 13))
      (node (ref P8) (pin 1)))
    (net (code 4) (name "Net-(J1-Pad3)")
      (node (ref P3) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 5) (name "Net-(J1-Pad18)")
      (node (ref J1) (pin 18))
      (node (ref P4) (pin 1)))
    (net (code 6) (name +5V)
      (node (ref J1) (pin 27))
      (node (ref P2) (pin 2))
      (node (ref P9) (pin 2)))
    (net (code 7) (name /A5)
      (node (ref D8) (pin 2))
      (node (ref J1) (pin 24)))
    (net (code 8) (name "Net-(D8-Pad1)")
      (node (ref D8) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 9) (name "Net-(D7-Pad1)")
      (node (ref R7) (pin 2))
      (node (ref D7) (pin 1)))
    (net (code 10) (name /A4)
      (node (ref D7) (pin 2))
      (node (ref J1) (pin 23)))
    (net (code 11) (name "Net-(D6-Pad1)")
      (node (ref R6) (pin 2))
      (node (ref D6) (pin 1)))
    (net (code 12) (name /A3)
      (node (ref J1) (pin 22))
      (node (ref D6) (pin 2)))
    (net (code 13) (name "Net-(D5-Pad1)")
      (node (ref R5) (pin 2))
      (node (ref D5) (pin 1)))
    (net (code 14) (name /A2)
      (node (ref J1) (pin 21))
      (node (ref D5) (pin 2)))
    (net (code 15) (name "Net-(D4-Pad1)")
      (node (ref R4) (pin 2))
      (node (ref D4) (pin 1)))
    (net (code 16) (name "Net-(D10-Pad1)")
      (node (ref D10) (pin 1))
      (node (ref R10) (pin 2)))
    (net (code 17) (name /MOSI)
      (node (ref J1) (pin 14))
      (node (ref P8) (pin 2)))
    (net (code 18) (name /A7)
      (node (ref D10) (pin 2))
      (node (ref J1) (pin 26)))
    (net (code 19) (name "Net-(D9-Pad1)")
      (node (ref R9) (pin 2))
      (node (ref D9) (pin 1)))
    (net (code 20) (name /A6)
      (node (ref J1) (pin 25))
      (node (ref D9) (pin 2)))
    (net (code 21) (name /VOUT+)
      (node (ref RV1) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref P2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref P9) (pin 1)))
    (net (code 22) (name /VSenseOut)
      (node (ref R13) (pin 1))
      (node (ref P2) (pin 4))
      (node (ref P9) (pin 4)))
    (net (code 23) (name /RX)
      (node (ref J1) (pin 2))
      (node (ref P7) (pin 2)))
    (net (code 24) (name /TX)
      (node (ref P7) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 25) (name /SCK)
      (node (ref P8) (pin 4))
      (node (ref J1) (pin 16)))
    (net (code 26) (name /MISO)
      (node (ref P8) (pin 3))
      (node (ref J1) (pin 15)))
    (net (code 27) (name "Net-(RV2-Pad3)")
      (node (ref RV2) (pin 3)))
    (net (code 28) (name "Net-(R13-Pad2)")
      (node (ref RV2) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 29) (name /D7)
      (node (ref J1) (pin 10))
      (node (ref P6) (pin 3)))
    (net (code 30) (name /D6)
      (node (ref P6) (pin 2))
      (node (ref J1) (pin 9)))
    (net (code 31) (name "Net-(P1-Pad2)")
      (node (ref P1) (pin 2)))
    (net (code 32) (name "Net-(P1-Pad8)")
      (node (ref P1) (pin 8)))
    (net (code 33) (name "Net-(P1-Pad4)")
      (node (ref P1) (pin 4)))
    (net (code 34) (name "Net-(P1-Pad3)")
      (node (ref P1) (pin 3)))
    (net (code 35) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5))
      (node (ref R1) (pin 2)))
    (net (code 36) (name /REMOTE)
      (node (ref R1) (pin 1))
      (node (ref P1) (pin 10)))
    (net (code 37) (name GND)
      (node (ref C2) (pin 2))
      (node (ref RV1) (pin 3))
      (node (ref C1) (pin 2))
      (node (ref J1) (pin 29))
      (node (ref CON1) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref P2) (pin 3))
      (node (ref P1) (pin 9))
      (node (ref R7) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref RV2) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref P9) (pin 3))
      (node (ref R9) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref CON1) (pin 3))
      (node (ref R6) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref P1) (pin 7)))
    (net (code 38) (name /TRIM)
      (node (ref RV1) (pin 2))
      (node (ref P1) (pin 6)))
    (net (code 39) (name /D9)
      (node (ref J1) (pin 12)))
    (net (code 40) (name /D8)
      (node (ref J1) (pin 11)))
    (net (code 41) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8))
      (node (ref LS1) (pin 1)))
    (net (code 42) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7))
      (node (ref LS1) (pin 2)))
    (net (code 43) (name /D3)
      (node (ref J1) (pin 6))
      (node (ref P6) (pin 1)))
    (net (code 44) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 45) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 46) (name /A1)
      (node (ref J1) (pin 20))
      (node (ref D4) (pin 2)))
    (net (code 47) (name "Net-(D3-Pad1)")
      (node (ref R3) (pin 2))
      (node (ref D3) (pin 1)))
    (net (code 48) (name /A0)
      (node (ref D3) (pin 2))
      (node (ref J1) (pin 19)))
    (net (code 49) (name +12V)
      (node (ref F1) (pin 2))
      (node (ref CON1) (pin 1)))))