(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/Car_Stereo_Replacement/pcb/pcb.sch)
    (date "Mon 12 Aug 2019 11:53:24 PM EDT")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source pcb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref DIN1)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_6mm)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4906D1))
    (comp (ref DIN2)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_6mm)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D49076D))
    (comp (ref STKLOGO1)
      (value OPEN_HARDWARE_1)
      (footprint SteakElectronics:steakelectronics_fmask)
      (libsource (lib logo) (part OPEN_HARDWARE_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D49086D))
    (comp (ref P1)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490AF6))
    (comp (ref P4)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490CEA))
    (comp (ref P7)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490D73))
    (comp (ref P10)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490D79))
    (comp (ref P2)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490EAC))
    (comp (ref P5)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490EB2))
    (comp (ref P8)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490EB8))
    (comp (ref P11)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D490EBE))
    (comp (ref P3)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D491190))
    (comp (ref P6)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D491196))
    (comp (ref P9)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D49119C))
    (comp (ref P12)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4911A2))
    (comp (ref J4)
      (value JACK_2P)
      (footprint Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles)
      (libsource (lib conn) (part JACK_2P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D49353F))
    (comp (ref J2)
      (value JACK_2P)
      (footprint Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles)
      (libsource (lib conn) (part JACK_2P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4936C7))
    (comp (ref J1)
      (value JACK_2P)
      (footprint Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles)
      (libsource (lib conn) (part JACK_2P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D493775))
    (comp (ref J3)
      (value JACK_2P)
      (footprint Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles)
      (libsource (lib conn) (part JACK_2P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D49366F))
    (comp (ref J5)
      (value JACK_2P)
      (footprint Connector_Audio:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical_CircularHoles)
      (libsource (lib conn) (part JACK_2P))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D495198))
    (comp (ref MK1)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B3459))
    (comp (ref MK2)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B34D0))
    (comp (ref P13)
      (value VCC7SEGCONN2)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B37E3))
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B436A))
    (comp (ref MK3)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B53D8))
    (comp (ref MK4)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B53DE))
    (comp (ref P14)
      (value AMP7SEGCONN3)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B5509))
    (comp (ref P15)
      (value PowerConn6)
      (footprint w_conn_mkds:mkds_1,5-6)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B63C4))
    (comp (ref P16)
      (value GndConn6)
      (footprint w_conn_mkds:mkds_1,5-6)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D4B64EE))
    (comp (ref P21)
      (value OLED_1_x_4)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5224F4))
    (comp (ref J6)
      (value Arduino_Nano_Header)
      (footprint w_conn_misc:arduino_nano_header)
      (libsource (lib w_connectors) (part Arduino_Nano_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D523A19))
    (comp (ref P19)
      (value duino4)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5259A1))
    (comp (ref P17)
      (value duino3)
      (footprint Pin_Headers:Pin_Header_Straight_1x03)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D525B7B))
    (comp (ref P20)
      (value duino7)
      (footprint Pin_Headers:Pin_Header_Straight_1x07)
      (libsource (lib conn) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D525F09))
    (comp (ref P18)
      (value duino11)
      (footprint Pin_Headers:Pin_Header_Straight_1x11)
      (libsource (lib conn) (part CONN_01X11))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D526123)))
  (libparts
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector, single row, 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector, single row, 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_01X07)
      (description "Connector, single row, 01x07")
      (footprints
        (fp Pin_Header_Straight_1X07)
        (fp Pin_Header_Angled_1X07)
        (fp Socket_Strip_Straight_1X07)
        (fp Socket_Strip_Angled_1X07))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X07))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib conn) (part CONN_01X11)
      (description "Connector, single row, 01x11")
      (footprints
        (fp Pin_Header_Straight_1X11)
        (fp Pin_Header_Angled_1X11)
        (fp Socket_Strip_Straight_1X11)
        (fp Socket_Strip_Angled_1X11))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X11))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))))
    (libpart (lib conn) (part JACK_2P)
      (fields
        (field (name Reference) J)
        (field (name Value) JACK_2P))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib logo) (part OPEN_HARDWARE_1)
      (description "Open Hardware Logo")
      (docs ~)
      (fields
        (field (name Reference) LOGO)
        (field (name Value) OPEN_HARDWARE_1)))
    (libpart (lib mechanical) (part Mounting_Hole)
      (description "Mounting Hole without connection")
      (footprints
        (fp Mounting?Hole*)
        (fp Hole*))
      (fields
        (field (name Reference) MK)
        (field (name Value) Mounting_Hole)))
    (libpart (lib w_connectors) (part Arduino_Nano_Header)
      (fields
        (field (name Reference) J)
        (field (name Value) Arduino_Nano_Header))
      (pins
        (pin (num 1) (name D1/TX) (type passive))
        (pin (num 2) (name D0/RX) (type passive))
        (pin (num 3) (name RESET) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name D2/INT0) (type passive))
        (pin (num 6) (name D3/INT1) (type passive))
        (pin (num 7) (name D4/T0) (type passive))
        (pin (num 8) (name D5/T1) (type passive))
        (pin (num 9) (name D6/AIN0) (type passive))
        (pin (num 10) (name D7/AIN1) (type passive))
        (pin (num 11) (name D8/ICP) (type passive))
        (pin (num 12) (name D9/0C1) (type passive))
        (pin (num 13) (name D10/SS) (type passive))
        (pin (num 14) (name D11/MOSI) (type passive))
        (pin (num 15) (name D12/MISO) (type passive))
        (pin (num 16) (name SCK/D13) (type passive))
        (pin (num 17) (name 3V3) (type passive))
        (pin (num 18) (name AREF) (type passive))
        (pin (num 19) (name A0) (type passive))
        (pin (num 20) (name A1) (type passive))
        (pin (num 21) (name A2) (type passive))
        (pin (num 22) (name A3) (type passive))
        (pin (num 23) (name A4) (type passive))
        (pin (num 24) (name A5) (type passive))
        (pin (num 25) (name A6) (type passive))
        (pin (num 26) (name A7) (type passive))
        (pin (num 27) (name 5V) (type passive))
        (pin (num 28) (name RESET) (type passive))
        (pin (num 29) (name GND) (type passive))
        (pin (num 30) (name VIN) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical logo)
      (uri /usr/share/kicad/library/logo.lib))
    (library (logical mechanical)
      (uri /usr/share/kicad/library/mechanical.lib))
    (library (logical w_connectors)
      (uri /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/Car_Stereo_Replacement/pcb/symbols/w_connectors.lib)))
  (nets
    (net (code 1) (name /duid11)
      (node (ref P18) (pin 2))
      (node (ref J6) (pin 14)))
    (net (code 2) (name /duid2)
      (node (ref J6) (pin 5))
      (node (ref P18) (pin 11)))
    (net (code 3) (name /duid3)
      (node (ref J6) (pin 6))
      (node (ref P18) (pin 10)))
    (net (code 4) (name /duid4)
      (node (ref P18) (pin 9))
      (node (ref J6) (pin 7)))
    (net (code 5) (name /duid5)
      (node (ref P18) (pin 8))
      (node (ref J6) (pin 8)))
    (net (code 6) (name /duid6)
      (node (ref P18) (pin 7))
      (node (ref J6) (pin 9)))
    (net (code 7) (name /duid7)
      (node (ref P18) (pin 6))
      (node (ref J6) (pin 10)))
    (net (code 8) (name /duia1)
      (node (ref P20) (pin 3))
      (node (ref J6) (pin 20)))
    (net (code 9) (name /duid8)
      (node (ref P18) (pin 5))
      (node (ref J6) (pin 11)))
    (net (code 10) (name /duia2)
      (node (ref J6) (pin 21))
      (node (ref P20) (pin 2)))
    (net (code 11) (name /duid9)
      (node (ref J6) (pin 12))
      (node (ref P18) (pin 4)))
    (net (code 12) (name /duia3)
      (node (ref J6) (pin 22))
      (node (ref P20) (pin 1)))
    (net (code 13) (name /duid10)
      (node (ref J6) (pin 13))
      (node (ref P18) (pin 3)))
    (net (code 14) (name /duid12)
      (node (ref P18) (pin 1))
      (node (ref J6) (pin 15)))
    (net (code 15) (name /duia6)
      (node (ref P19) (pin 4))
      (node (ref J6) (pin 25)))
    (net (code 16) (name /duid13)
      (node (ref P20) (pin 7))
      (node (ref J6) (pin 16)))
    (net (code 17) (name /duia7)
      (node (ref J6) (pin 26))
      (node (ref P19) (pin 3)))
    (net (code 18) (name /dui3v3)
      (node (ref J6) (pin 17))
      (node (ref P20) (pin 6)))
    (net (code 19) (name /dui5v)
      (node (ref P19) (pin 2))
      (node (ref J6) (pin 27)))
    (net (code 20) (name /duiaref)
      (node (ref P20) (pin 5))
      (node (ref J6) (pin 18)))
    (net (code 21) (name /duia0)
      (node (ref P20) (pin 4))
      (node (ref J6) (pin 19)))
    (net (code 22) (name +12V)
      (node (ref F1) (pin 2))
      (node (ref P15) (pin 6))
      (node (ref P15) (pin 5))
      (node (ref P15) (pin 4))
      (node (ref P15) (pin 3))
      (node (ref P15) (pin 2))
      (node (ref P15) (pin 1))
      (node (ref P6) (pin 1))
      (node (ref P2) (pin 2))
      (node (ref P4) (pin 1))
      (node (ref J6) (pin 30)))
    (net (code 23) (name /SDATA)
      (node (ref P21) (pin 1))
      (node (ref J6) (pin 23)))
    (net (code 24) (name GND)
      (node (ref P16) (pin 1))
      (node (ref P16) (pin 3))
      (node (ref P16) (pin 4))
      (node (ref J4) (pin 3))
      (node (ref J2) (pin 3))
      (node (ref P14) (pin 3))
      (node (ref J1) (pin 3))
      (node (ref P16) (pin 2))
      (node (ref J3) (pin 3))
      (node (ref P16) (pin 6))
      (node (ref J5) (pin 3))
      (node (ref J6) (pin 4))
      (node (ref P21) (pin 4))
      (node (ref J6) (pin 29))
      (node (ref P16) (pin 5)))
    (net (code 25) (name /SCLK)
      (node (ref J6) (pin 24))
      (node (ref P21) (pin 2)))
    (net (code 26) (name +5V)
      (node (ref P21) (pin 3)))
    (net (code 27) (name /duid1)
      (node (ref P17) (pin 3))
      (node (ref J6) (pin 1)))
    (net (code 28) (name /duid0)
      (node (ref P17) (pin 2))
      (node (ref J6) (pin 2)))
    (net (code 29) (name /duireset)
      (node (ref J6) (pin 28))
      (node (ref J6) (pin 3))
      (node (ref P17) (pin 1))
      (node (ref P19) (pin 1)))
    (net (code 30) (name /Rear_Rch+)
      (node (ref J2) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref P11) (pin 2)))
    (net (code 31) (name /BATT12V+)
      (node (ref P1) (pin 2)))
    (net (code 32) (name /DIM+)
      (node (ref P4) (pin 2)))
    (net (code 33) (name "Net-(P7-Pad1)")
      (node (ref P7) (pin 1)))
    (net (code 34) (name "Net-(P7-Pad2)")
      (node (ref P7) (pin 2)))
    (net (code 35) (name /Front_Rch-)
      (node (ref P10) (pin 1)))
    (net (code 36) (name /Rear_Rch-)
      (node (ref P10) (pin 2)))
    (net (code 37) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 38) (name "Net-(P5-Pad1)")
      (node (ref P5) (pin 1)))
    (net (code 39) (name /DIN-)
      (node (ref P5) (pin 2)))
    (net (code 40) (name /Rear_Lch+)
      (node (ref P8) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 41) (name /Front_Lch+)
      (node (ref P8) (pin 2))
      (node (ref J3) (pin 2))
      (node (ref J3) (pin 1)))
    (net (code 42) (name /Front_Rch+)
      (node (ref P11) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 43) (name /SW+12V)
      (node (ref P3) (pin 1)))
    (net (code 44) (name /+BCH)
      (node (ref J5) (pin 2))
      (node (ref P3) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 45) (name /AMP_SENS)
      (node (ref P6) (pin 2)))
    (net (code 46) (name /Rear_Lch-)
      (node (ref P9) (pin 1)))
    (net (code 47) (name /Front_Lch-)
      (node (ref P9) (pin 2)))
    (net (code 48) (name /BATGROUND)
      (node (ref P12) (pin 1))
      (node (ref P13) (pin 2))
      (node (ref P14) (pin 2)))
    (net (code 49) (name /PARK)
      (node (ref P12) (pin 2)))
    (net (code 50) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 51) (name /IGN12V+)
      (node (ref P14) (pin 1))
      (node (ref P13) (pin 1))
      (node (ref F1) (pin 1)))))