https://www.digikey.com/product-detail/en/murata-electronics-north-america/1255AY-150M=P3/490-10802-1-ND/5271544

see lt data sheet for details.
must not be series resistance greater than 0.1 ohms






s 	Inductors, Coils, Chokes 	
Arrays, Signal Transformers 	
Manufacturer 	Eaton - Electronics Division 	
Series 	OCTA-PAC® 	
Packaging ? 	Cut Tape (CT) ? 	
Part Status 	Active 	
Number of Coils 	2 	
Inductance - Connected In Parallel 	32.86µH 	
Inductance - Connected In Series 	131.42µH 	
Tolerance 	±20% 	
Current Rating - Parallel 	960mA 	
Current Rating - Series 	480mA 	
DC Resistance (DCR) - Parallel 	83mOhm Max 	
DC Resistance (DCR) - Series 	331mOhm Max 	
Shielding 	Unshielded 	
Ratings 	- 	
Operating Temperature 	-40°C ~ 85°C 	
Mounting Type 	Surface Mount 	
Package / Case 	Nonstandard 	
Size / Dimension 	0.550" L x 0.550" W (13.97mm x 13.97mm) 	
Height 	0.190" (4.83mm) 
