(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/batterycharge_stationdata/pcb/rev1/batterystation.sch)
    (date "Sun 21 Apr 2019 08:23:35 PM EDT")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source batterystation.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source STC4054_Liion_Charge.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /MAX6675/) (tstamps /5CBC1777/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source MAX6675.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /ENC28J60/) (tstamps /5CBC4480/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source ENC28J60_Arduino.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /BatteryChargerPower/) (tstamps /5CBC4AC4/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source BatteryChargerPower.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /LT1512/) (tstamps /5CBC6C0A/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source LT1512_universalcharger.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /CurrentSense_INA169_1/) (tstamps /5CBE9794/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source CurrentSense_INA169.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /sheet5CBEAB48/) (tstamps /5CBEAB48/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source CurrentSense_INA169.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /sheet5CBEAC38/) (tstamps /5CBEAC38/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source CurrentSense_INA169.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P7)
      (value LIION_CONN)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBC0E41))
    (comp (ref P8)
      (value LT_CONN)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBE92FB))
    (comp (ref P4)
      (value ScrewTerminal)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBEB5B3))
    (comp (ref P5)
      (value ScrewTerminal)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBEBB39))
    (comp (ref P6)
      (value ScrewTerminal)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBEBDEB))
    (comp (ref J1)
      (value Arduino_Nano_Header)
      (footprint w_conn_misc:arduino_nano_header)
      (libsource (lib w_connectors) (part Arduino_Nano_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBECE63))
    (comp (ref P3)
      (value 3v3breakout)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF2DCE))
    (comp (ref P2)
      (value AREFBREAKOUT)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF308E))
    (comp (ref P1)
      (value ADC_TerminalBlock)
      (footprint Pin_Headers:Pin_Header_Straight_1x08)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF36F0))
    (comp (ref P20)
      (value LTSENSESCREWTERMINAL)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF6691))
    (comp (ref P10)
      (value STC4054)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (libsource (lib conn) (part CONN_01X05))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBBEE8F))
    (comp (ref D1)
      (value LED)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part LED))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBBF242))
    (comp (ref R1)
      (value 5K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBBF689))
    (comp (ref C1)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBBFBC6))
    (comp (ref P9)
      (value VPROG_TAP)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBC014B))
    (comp (ref R2)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBC04AF))
    (comp (ref C2)
      (value 4.7uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /STC4054_Liion_Charge/) (tstamps /5CBBEAA9/))
      (tstamp 5CBC0798))
    (comp (ref P11)
      (value MAX6675)
      (footprint Power_Integrations:SO-8)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /MAX6675/) (tstamps /5CBC1777/))
      (tstamp 5CBC1B14))
    (comp (ref C3)
      (value 0.1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /MAX6675/) (tstamps /5CBC1777/))
      (tstamp 5CBC1EC5))
    (comp (ref TC1)
      (value Thermocouple)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (datasheet https://en.wikipedia.org/wiki/Thermocouple)
      (libsource (lib device) (part Thermocouple))
      (sheetpath (names /MAX6675/) (tstamps /5CBC1777/))
      (tstamp 5CBC268F))
    (comp (ref P12)
      (value max6675_nc)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /MAX6675/) (tstamps /5CBC1777/))
      (tstamp 5CBC3AC6))
    (comp (ref P15)
      (value ENCBREAKOUT2x5)
      (footprint Pin_Headers:Pin_Header_Straight_2x05)
      (libsource (lib conn) (part CONN_02X05))
      (sheetpath (names /ENC28J60/) (tstamps /5CBC4480/))
      (tstamp 5BF754F5))
    (comp (ref P16)
      (value ENCBREAKOUT2x6)
      (footprint Pin_Headers:Pin_Header_Straight_2x06)
      (libsource (lib conn) (part CONN_02X06))
      (sheetpath (names /ENC28J60/) (tstamps /5CBC4480/))
      (tstamp 5BF7553B))
    (comp (ref P13)
      (value PWRSELECT3v3)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /ENC28J60/) (tstamps /5CBC4480/))
      (tstamp 5BF75EA3))
    (comp (ref P14)
      (value PWRSELECT5V)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /ENC28J60/) (tstamps /5CBC4480/))
      (tstamp 5BF75ED4))
    (comp (ref U1)
      (value AP1117)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (datasheet http://www.diodes.com/datasheets/AP1117.pdf)
      (libsource (lib regul) (part AP1117))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC4E70))
    (comp (ref U2)
      (value LM317_SOT223)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (datasheet regulator/lm117.pdf)
      (libsource (lib regul) (part LM317_SOT223))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC50D3))
    (comp (ref R3)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC51CD))
    (comp (ref R4)
      (value 3K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC5278))
    (comp (ref C5)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC54F0))
    (comp (ref C4)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC5531))
    (comp (ref P17)
      (value LN2577IN)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC6395))
    (comp (ref P18)
      (value LM2577OUT)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBC63E0))
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBF5A27))
    (comp (ref CON1)
      (value BARREL_JACK)
      (footprint Connectors:BARREL_JACK)
      (libsource (lib conn) (part BARREL_JACK))
      (sheetpath (names /BatteryChargerPower/) (tstamps /5CBC4AC4/))
      (tstamp 5CBD2D8E))
    (comp (ref P19)
      (value LT1512)
      (footprint Housings_DIP:DIP-8_W7.62mm)
      (libsource (lib conn) (part CONN_01X08))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBC6E54))
    (comp (ref C6)
      (value 2.2uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBC7FC7))
    (comp (ref L1)
      (value 33uH)
      (footprint Inductors:Inductor_Taiyo-Yuden_NR-60xx_HandSoldering)
      (libsource (lib pspice) (part INDUCTOR))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBC842B))
    (comp (ref C8)
      (value 0.1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBC8B80))
    (comp (ref R12)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBC8C04))
    (comp (ref L2)
      (value 33uH)
      (footprint Inductors:Inductor_Taiyo-Yuden_NR-60xx_HandSoldering)
      (libsource (lib pspice) (part INDUCTOR))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCA135))
    (comp (ref C7)
      (value 2.2uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCA445))
    (comp (ref R11)
      (value 24)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCAC52))
    (comp (ref C9)
      (value 0.22uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBC988F))
    (comp (ref R10)
      (value 0.2)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCBDA1))
    (comp (ref D2)
      (value D_Schottky)
      (footprint Diodes_SMD:SOD-323_HandSoldering)
      (libsource (lib device) (part D_Schottky))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCC66F))
    (comp (ref R9)
      (value 100K)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib device) (part R_Variable))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCD72A))
    (comp (ref R13)
      (value 12.4K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCD7D5))
    (comp (ref C10)
      (value 22uF)
      (footprint Capacitors_Tantalum_SMD:Tantalum_Case-C_EIA-6032-28_Hand)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBCF221))
    (comp (ref R5)
      (value 536)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBD3F6D))
    (comp (ref R8)
      (value 2K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBD820D))
    (comp (ref SW2)
      (value SW_SP3T)
      (footprint Buttons_Switches_SMD:SW_SP3T_PCM13)
      (libsource (lib switches) (part SW_SP3T))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBDE680))
    (comp (ref SW1)
      (value SW_DPDT_x2)
      (footprint Buttons_Switches_SMD:SW_SPDT_PCM12)
      (libsource (lib switches) (part SW_DPDT_x2))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBE02E2))
    (comp (ref R6)
      (value "28.7K 1%")
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBE0901))
    (comp (ref R7)
      (value 54.9K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /LT1512/) (tstamps /5CBC6C0A/))
      (tstamp 5CBE4866))
    (comp (ref U3)
      (value INA169)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (datasheet http://www.ti.com/lit/ds/symlink/ina138.pdf)
      (libsource (lib sensors) (part INA168))
      (sheetpath (names /CurrentSense_INA169_1/) (tstamps /5CBE9794/))
      (tstamp 5CBE9994))
    (comp (ref R14)
      (value 1)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /CurrentSense_INA169_1/) (tstamps /5CBE9794/))
      (tstamp 5CBE9BDD))
    (comp (ref R15)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /CurrentSense_INA169_1/) (tstamps /5CBE9794/))
      (tstamp 5CBEA23D))
    (comp (ref U4)
      (value INA169)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (datasheet http://www.ti.com/lit/ds/symlink/ina138.pdf)
      (libsource (lib sensors) (part INA168))
      (sheetpath (names /sheet5CBEAB48/) (tstamps /5CBEAB48/))
      (tstamp 5CBE9994))
    (comp (ref R16)
      (value 1)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /sheet5CBEAB48/) (tstamps /5CBEAB48/))
      (tstamp 5CBE9BDD))
    (comp (ref R17)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /sheet5CBEAB48/) (tstamps /5CBEAB48/))
      (tstamp 5CBEA23D))
    (comp (ref U5)
      (value INA169)
      (footprint TO_SOT_Packages_SMD:SOT-23-5)
      (datasheet http://www.ti.com/lit/ds/symlink/ina138.pdf)
      (libsource (lib sensors) (part INA168))
      (sheetpath (names /sheet5CBEAC38/) (tstamps /5CBEAC38/))
      (tstamp 5CBE9994))
    (comp (ref R18)
      (value 1)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /sheet5CBEAC38/) (tstamps /5CBEAC38/))
      (tstamp 5CBE9BDD))
    (comp (ref R19)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /sheet5CBEAC38/) (tstamps /5CBEAC38/))
      (tstamp 5CBEA23D)))
  (libparts
    (libpart (lib conn) (part BARREL_JACK)
      (description "DC Barrel Jack")
      (fields
        (field (name Reference) CON)
        (field (name Value) BARREL_JACK))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (description "Connector, single row, 01x05")
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib conn) (part CONN_01X08)
      (description "Connector, single row, 01x08")
      (footprints
        (fp Pin_Header_Straight_1X08)
        (fp Pin_Header_Angled_1X08)
        (fp Socket_Strip_Straight_1X08)
        (fp Socket_Strip_Angled_1X08))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib conn) (part CONN_02X05)
      (description "Connector, double row, 02x05")
      (footprints
        (fp Pin_Header_Straight_2X05)
        (fp Pin_Header_Angled_2X05)
        (fp Socket_Strip_Straight_2X05)
        (fp Socket_Strip_Angled_2X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib conn) (part CONN_02X06)
      (description "Connector, double row, 02x06")
      (footprints
        (fp Pin_Header_Straight_2X06)
        (fp Pin_Header_Angled_2X06)
        (fp Socket_Strip_Straight_2X06)
        (fp Socket_Strip_Angled_2X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D_Schottky)
      (description "Schottky diode")
      (footprints
        (fp Diode_*)
        (fp D-*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R_Variable)
      (description "variable Resistor (Rheostat)")
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Variable))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Thermocouple)
      (description thermocouple)
      (docs https://en.wikipedia.org/wiki/Thermocouple)
      (footprints
        (fp PIN?ARRAY*)
        (fp bornier*)
        (fp *Terminal?Block*)
        (fp Thermo*Couple*))
      (fields
        (field (name Reference) TC)
        (field (name Value) Thermocouple))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib pspice) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib regul) (part AP1117)
      (aliases
        (alias AP111715)
        (alias AP111718)
        (alias AP111725)
        (alias AP111733)
        (alias AP111750))
      (description "1A Low Dropout regulator, positive, adjustable output, NRND")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT-223*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-223))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))
        (pin (num 4) (name VO) (type power_out))))
    (libpart (lib regul) (part LM317_SOT223)
      (description "Linear Regulator (adjustable)")
      (docs regulator/lm117.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) LM317_SOT223))
      (pins
        (pin (num 1) (name ADJ) (type input))
        (pin (num 2) (name OUT) (type power_out))
        (pin (num 3) (name IN) (type input))))
    (libpart (lib sensors) (part INA138)
      (aliases
        (alias INA168))
      (description "Unipolar high-side current shunt monitor, 36V common mode")
      (docs http://www.ti.com/lit/ds/symlink/ina138.pdf)
      (footprints
        (fp SOT-23-*))
      (fields
        (field (name Reference) U)
        (field (name Value) INA138)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name OUT) (type output))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name V+) (type power_in))
        (pin (num 4) (name +IN) (type input))
        (pin (num 5) (name -IN) (type input))))
    (libpart (lib switches) (part SW_DPDT_x2)
      (description "Switch, dual pole double throw, separate symbols")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DPDT_x2))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))
        (pin (num 4) (name B) (type passive))
        (pin (num 5) (name C) (type passive))))
    (libpart (lib switches) (part SW_SP3T)
      (description "Switch, three position, single pole triple throw, 3 position switch, SP3T")
      (footprints
        (fp SW*)
        (fp SP3T*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_SP3T))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib w_connectors) (part Arduino_Nano_Header)
      (fields
        (field (name Reference) J)
        (field (name Value) Arduino_Nano_Header))
      (pins
        (pin (num 1) (name D1/TX) (type passive))
        (pin (num 2) (name D0/RX) (type passive))
        (pin (num 3) (name RESET) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name D2/INT0) (type passive))
        (pin (num 6) (name D3/INT1) (type passive))
        (pin (num 7) (name D4/T0) (type passive))
        (pin (num 8) (name D5/T1) (type passive))
        (pin (num 9) (name D6/AIN0) (type passive))
        (pin (num 10) (name D7/AIN1) (type passive))
        (pin (num 11) (name D8/ICP) (type passive))
        (pin (num 12) (name D9/0C1) (type passive))
        (pin (num 13) (name D10/SS) (type passive))
        (pin (num 14) (name D11/MOSI) (type passive))
        (pin (num 15) (name D12/MISO) (type passive))
        (pin (num 16) (name SCK/D13) (type passive))
        (pin (num 17) (name 3V3) (type passive))
        (pin (num 18) (name AREF) (type passive))
        (pin (num 19) (name A0) (type passive))
        (pin (num 20) (name A1) (type passive))
        (pin (num 21) (name A2) (type passive))
        (pin (num 22) (name A3) (type passive))
        (pin (num 23) (name A4) (type passive))
        (pin (num 24) (name A5) (type passive))
        (pin (num 25) (name A6) (type passive))
        (pin (num 26) (name A7) (type passive))
        (pin (num 27) (name 5V) (type passive))
        (pin (num 28) (name RESET) (type passive))
        (pin (num 29) (name GND) (type passive))
        (pin (num 30) (name VIN) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical pspice)
      (uri /usr/share/kicad/library/pspice.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical sensors)
      (uri /usr/share/kicad/library/sensors.lib))
    (library (logical switches)
      (uri /usr/share/kicad/library/switches.lib))
    (library (logical w_connectors)
      (uri /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/batterycharge_stationdata/pcb/symbols/w_connectors.lib)))
  (nets
    (net (code 1) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17))
      (node (ref P3) (pin 1)))
    (net (code 2) (name /NANO_CS)
      (node (ref J1) (pin 13))
      (node (ref P15) (pin 8))
      (node (ref P16) (pin 4)))
    (net (code 3) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23))
      (node (ref P1) (pin 4)))
    (net (code 4) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24))
      (node (ref P1) (pin 3)))
    (net (code 5) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25))
      (node (ref P1) (pin 2)))
    (net (code 6) (name "Net-(J1-Pad26)")
      (node (ref P1) (pin 1))
      (node (ref J1) (pin 26)))
    (net (code 7) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22))
      (node (ref P1) (pin 5)))
    (net (code 8) (name "Net-(J1-Pad18)")
      (node (ref P2) (pin 1))
      (node (ref J1) (pin 18)))
    (net (code 9) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 10) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19))
      (node (ref P1) (pin 8)))
    (net (code 11) (name +5V)
      (node (ref C3) (pin 1))
      (node (ref P14) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref P10) (pin 5))
      (node (ref U5) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref P11) (pin 4))
      (node (ref L1) (pin 1))
      (node (ref P19) (pin 5))
      (node (ref C5) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref U3) (pin 3))
      (node (ref U4) (pin 3))
      (node (ref J1) (pin 27)))
    (net (code 12) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 13) (name /sheet5CBEAC38/LOADIN)
      (node (ref R18) (pin 1))
      (node (ref P6) (pin 2))
      (node (ref U5) (pin 4)))
    (net (code 14) (name /sheet5CBEAC38/LOADOUT)
      (node (ref P6) (pin 3))
      (node (ref R18) (pin 2))
      (node (ref U5) (pin 5)))
    (net (code 15) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1)))
    (net (code 16) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 17) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 18) (name GND)
      (node (ref U3) (pin 2))
      (node (ref P17) (pin 4))
      (node (ref P16) (pin 2))
      (node (ref P15) (pin 9))
      (node (ref R17) (pin 2))
      (node (ref P18) (pin 2))
      (node (ref P16) (pin 12))
      (node (ref P18) (pin 1))
      (node (ref P11) (pin 1))
      (node (ref P11) (pin 2))
      (node (ref P7) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref C10) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref P19) (pin 7))
      (node (ref P19) (pin 6))
      (node (ref C6) (pin 2))
      (node (ref J1) (pin 29))
      (node (ref CON1) (pin 3))
      (node (ref CON1) (pin 2))
      (node (ref P8) (pin 1))
      (node (ref R15) (pin 2))
      (node (ref P17) (pin 3))
      (node (ref R4) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref P10) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref P7) (pin 3))
      (node (ref TC1) (pin 2))
      (node (ref P8) (pin 3)))
    (net (code 19) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 20) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 21) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 22) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 23) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 24) (name "Net-(J1-Pad20)")
      (node (ref P1) (pin 7))
      (node (ref J1) (pin 20)))
    (net (code 25) (name "Net-(J1-Pad30)")
      (node (ref J1) (pin 30)))
    (net (code 26) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 27) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21))
      (node (ref P1) (pin 6)))
    (net (code 28) (name /LT1512/LTShutdownPin)
      (node (ref P20) (pin 1))
      (node (ref P19) (pin 4)))
    (net (code 29) (name /LT1512/LT_FloatVoltage)
      (node (ref R7) (pin 2))
      (node (ref P19) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref P20) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 30) (name /NANO_MOSI)
      (node (ref J1) (pin 14))
      (node (ref P15) (pin 6))
      (node (ref P16) (pin 6)))
    (net (code 31) (name /LT1512/LT_IFEEDBACK)
      (node (ref R11) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref L2) (pin 2)))
    (net (code 32) (name /NANO_MISO)
      (node (ref J1) (pin 15))
      (node (ref P11) (pin 7))
      (node (ref P15) (pin 3))
      (node (ref P16) (pin 7)))
    (net (code 33) (name /MAX_CS)
      (node (ref P11) (pin 6))
      (node (ref J1) (pin 12)))
    (net (code 34) (name /LT1512/LT_BATCHRG)
      (node (ref P8) (pin 4))
      (node (ref C10) (pin 1))
      (node (ref SW2) (pin 3))
      (node (ref D2) (pin 1))
      (node (ref P8) (pin 2)))
    (net (code 35) (name /STC4054_Liion_Charge/BAT_LIION_CHRG)
      (node (ref C2) (pin 1))
      (node (ref P7) (pin 4))
      (node (ref P10) (pin 3))
      (node (ref P7) (pin 2)))
    (net (code 36) (name "Net-(P6-Pad4)")
      (node (ref P6) (pin 4)))
    (net (code 37) (name /NANO_SCK)
      (node (ref P11) (pin 5))
      (node (ref J1) (pin 16))
      (node (ref P16) (pin 5))
      (node (ref P15) (pin 5)))
    (net (code 38) (name /sheet5CBEAB48/LOADOUT)
      (node (ref P5) (pin 3))
      (node (ref R16) (pin 2))
      (node (ref U4) (pin 5)))
    (net (code 39) (name /CurrentSense_INA169_1/LOADIN)
      (node (ref U3) (pin 4))
      (node (ref P4) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 40) (name /CurrentSense_INA169_1/LOADOUT)
      (node (ref R14) (pin 2))
      (node (ref U3) (pin 5))
      (node (ref P4) (pin 3)))
    (net (code 41) (name "Net-(P4-Pad4)")
      (node (ref P4) (pin 4)))
    (net (code 42) (name /CurrentSense_INA169_1/CurrentOUT)
      (node (ref P4) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 43) (name /sheet5CBEAB48/CurrentOUT)
      (node (ref U4) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref P5) (pin 1)))
    (net (code 44) (name /sheet5CBEAB48/LOADIN)
      (node (ref P5) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref U4) (pin 4)))
    (net (code 45) (name "Net-(P5-Pad4)")
      (node (ref P5) (pin 4)))
    (net (code 46) (name /sheet5CBEAC38/CurrentOUT)
      (node (ref R19) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref P6) (pin 1)))
    (net (code 47) (name /STC4054_Liion_Charge/CHRG)
      (node (ref D1) (pin 1))
      (node (ref P10) (pin 1)))
    (net (code 48) (name /STC4054_Liion_Charge/PROG)
      (node (ref P9) (pin 1))
      (node (ref P10) (pin 4))
      (node (ref R1) (pin 1)))
    (net (code 49) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 51) (name /MAX6675/NC)
      (node (ref P11) (pin 8))
      (node (ref P12) (pin 1)))
    (net (code 52) (name /MAX6675/T+)
      (node (ref TC1) (pin 1))
      (node (ref P11) (pin 3)))
    (net (code 53) (name +3V3)
      (node (ref P13) (pin 1)))
    (net (code 54) (name /ENC28J60/VCC_Branch)
      (node (ref P16) (pin 11))
      (node (ref P15) (pin 10))
      (node (ref P13) (pin 2))
      (node (ref P14) (pin 2)))
    (net (code 55) (name /ENC28J60/WOL)
      (node (ref P16) (pin 8))
      (node (ref P15) (pin 4)))
    (net (code 56) (name /ENC28J60/Q3)
      (node (ref P16) (pin 1)))
    (net (code 57) (name /ENC28J60/RSTENC)
      (node (ref P16) (pin 3))
      (node (ref P15) (pin 7)))
    (net (code 58) (name /ENC28J60/CLKOUT)
      (node (ref P16) (pin 10))
      (node (ref P15) (pin 2)))
    (net (code 59) (name /ENC28J60/INT)
      (node (ref P16) (pin 9))
      (node (ref P15) (pin 1)))
    (net (code 60) (name /BatteryChargerPower/+15.5V)
      (node (ref P18) (pin 3))
      (node (ref P18) (pin 4)))
    (net (code 61) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 62) (name +12V)
      (node (ref CON1) (pin 1))
      (node (ref P17) (pin 1))
      (node (ref F1) (pin 1))
      (node (ref P17) (pin 2)))
    (net (code 63) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref U2) (pin 1)))
    (net (code 64) (name "Net-(C4-Pad1)")
      (node (ref U2) (pin 3))
      (node (ref C4) (pin 1))
      (node (ref F1) (pin 2)))
    (net (code 65) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 2)))
    (net (code 66) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 67) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref SW1) (pin 3)))
    (net (code 68) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref SW1) (pin 1)))
    (net (code 69) (name "Net-(R7-Pad1)")
      (node (ref SW2) (pin 4))
      (node (ref SW1) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 70) (name "Net-(R8-Pad2)")
      (node (ref R8) (pin 2))
      (node (ref R9) (pin 2)))
    (net (code 71) (name "Net-(R8-Pad1)")
      (node (ref R8) (pin 1))
      (node (ref SW2) (pin 1)))
    (net (code 72) (name "Net-(SW2-Pad2)")
      (node (ref SW2) (pin 2)))
    (net (code 73) (name /LT1512/I_Feedback)
      (node (ref R11) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref P19) (pin 3)))
    (net (code 74) (name /LT1512/Vsw)
      (node (ref L1) (pin 2))
      (node (ref P19) (pin 8))
      (node (ref C7) (pin 1)))
    (net (code 75) (name "Net-(C7-Pad2)")
      (node (ref L2) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 76) (name "Net-(C8-Pad1)")
      (node (ref R12) (pin 2))
      (node (ref C8) (pin 1)))
    (net (code 77) (name /LT1512/Vcomp)
      (node (ref P19) (pin 1))
      (node (ref C8) (pin 2)))))