(module footprints:Barrier_Strip_1x3 (layer F.Cu) (tedit 5E16D6E2)
  (fp_text reference J47 (at -7 16) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Screw_Terminal_01x03 (at 1 10) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user ED2946-ND (at 3 13) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 16 15) (end 16 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.5 15) (end 16 15) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.5 2.5) (end -3 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.5 2.5) (end 16 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.5 14.5) (end -9.5 15) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.5 8.5) (end -9.5 14.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.5 2.5) (end -9.5 8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.5 2.5) (end -3 2.5) (layer F.SilkS) (width 0.15))
  (pad 3 thru_hole circle (at 11.5 5) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 3.25 5) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -5 5) (size 2.7 2.7) (drill 2) (layers *.Cu *.Mask))
)
