(module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5E881D08)
  (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
  (tags "Through hole pin header THT 1x01 1.27mm single row")
  (fp_text reference REF** (at 0 -1.695) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PinHeader_1x01_P1.27mm_Vertical (at 0 1.695) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
