(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2020/OV7670_Image_Sensor/pcb/pcb.sch)
    (date "Tue 31 Mar 2020 02:21:42 AM EDT")
    (tool "Eeschema 5.0.2+dfsg1-1~bpo9+1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source pcb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Conn_02x09_Counter_Clockwise)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x09_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x09_Odd_Even) (description "Generic connector, double row, 02x09, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E82D94D))
    (comp (ref A1)
      (value Arduino_UNO_R3)
      (footprint Module:Arduino_UNO_R3)
      (datasheet https://www.arduino.cc/en/Main/arduinoBoardUno)
      (libsource (lib MCU_Module) (part Arduino_UNO_R3) (description "Arduino UNO Microcontroller Module, release 3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E82DE4B))
    (comp (ref R2)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E82E56A))
    (comp (ref R1)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E82EAE2))
    (comp (ref R3)
      (value R680)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E82F3BF))
    (comp (ref R4)
      (value R1K)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E82F408)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_02x09_Odd_Even)
      (description "Generic connector, double row, 02x09, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x09_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MCU_Module) (part Arduino_UNO_R3)
      (description "Arduino UNO Microcontroller Module, release 3")
      (docs https://www.arduino.cc/en/Main/arduinoBoardUno)
      (footprints
        (fp Arduino*UNO*R3*))
      (fields
        (field (name Reference) A)
        (field (name Value) Arduino_UNO_R3)
        (field (name Footprint) Module:Arduino_UNO_R3))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name IOREF) (type output))
        (pin (num 3) (name RESET) (type input))
        (pin (num 4) (name 3V3) (type power_out))
        (pin (num 5) (name +5V) (type power_out))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name VIN) (type power_in))
        (pin (num 9) (name A0) (type BiDi))
        (pin (num 10) (name A1) (type BiDi))
        (pin (num 11) (name A2) (type BiDi))
        (pin (num 12) (name A3) (type BiDi))
        (pin (num 13) (name A4/SDA) (type BiDi))
        (pin (num 14) (name A5/SCL) (type BiDi))
        (pin (num 15) (name D0/RX) (type BiDi))
        (pin (num 16) (name D1/TX) (type BiDi))
        (pin (num 17) (name D2) (type BiDi))
        (pin (num 18) (name D3) (type BiDi))
        (pin (num 19) (name D4) (type BiDi))
        (pin (num 20) (name D5) (type BiDi))
        (pin (num 21) (name D6) (type BiDi))
        (pin (num 22) (name D7) (type BiDi))
        (pin (num 23) (name D8) (type BiDi))
        (pin (num 24) (name D9) (type BiDi))
        (pin (num 25) (name D10) (type BiDi))
        (pin (num 26) (name D11) (type BiDi))
        (pin (num 27) (name D12) (type BiDi))
        (pin (num 28) (name D13) (type BiDi))
        (pin (num 29) (name GND) (type power_in))
        (pin (num 30) (name AREF) (type input))
        (pin (num 31) (name SDA) (type BiDi))
        (pin (num 32) (name SCL) (type BiDi)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical MCU_Module)
      (uri /usr/share/kicad/library/MCU_Module.lib)))
  (nets
    (net (code 1) (name +3V3)
      (node (ref J1) (pin 17))
      (node (ref A1) (pin 4))
      (node (ref R1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 2) (name +5V)
      (node (ref A1) (pin 5)))
    (net (code 3) (name GND)
      (node (ref R4) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 18))
      (node (ref A1) (pin 29))
      (node (ref A1) (pin 7))
      (node (ref A1) (pin 6)))
    (net (code 4) (name /D0)
      (node (ref A1) (pin 9))
      (node (ref J1) (pin 16)))
    (net (code 5) (name "Net-(A1-Pad8)")
      (node (ref A1) (pin 8)))
    (net (code 6) (name "Net-(A1-Pad32)")
      (node (ref A1) (pin 32)))
    (net (code 7) (name "Net-(A1-Pad31)")
      (node (ref A1) (pin 31)))
    (net (code 8) (name "Net-(A1-Pad30)")
      (node (ref A1) (pin 30)))
    (net (code 9) (name "Net-(A1-Pad3)")
      (node (ref A1) (pin 3)))
    (net (code 10) (name "Net-(A1-Pad28)")
      (node (ref A1) (pin 28)))
    (net (code 11) (name "Net-(A1-Pad18)")
      (node (ref A1) (pin 18))
      (node (ref R3) (pin 1)))
    (net (code 12) (name /XCLK)
      (node (ref J1) (pin 8))
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 13) (name /NC-16)
      (node (ref J1) (pin 6)))
    (net (code 14) (name /SIOC)
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref A1) (pin 14)))
    (net (code 15) (name /PCLK)
      (node (ref J1) (pin 7))
      (node (ref A1) (pin 27)))
    (net (code 16) (name "Net-(A1-Pad26)")
      (node (ref A1) (pin 26)))
    (net (code 17) (name "Net-(A1-Pad25)")
      (node (ref A1) (pin 25)))
    (net (code 18) (name "Net-(A1-Pad24)")
      (node (ref A1) (pin 24)))
    (net (code 19) (name "Net-(A1-Pad23)")
      (node (ref A1) (pin 23)))
    (net (code 20) (name /D7)
      (node (ref A1) (pin 22))
      (node (ref J1) (pin 9)))
    (net (code 21) (name /D6)
      (node (ref J1) (pin 10))
      (node (ref A1) (pin 21)))
    (net (code 22) (name /D5)
      (node (ref A1) (pin 20))
      (node (ref J1) (pin 11)))
    (net (code 23) (name "Net-(A1-Pad2)")
      (node (ref A1) (pin 2)))
    (net (code 24) (name /D4)
      (node (ref J1) (pin 12))
      (node (ref A1) (pin 19)))
    (net (code 25) (name /VSYNC)
      (node (ref A1) (pin 17))
      (node (ref J1) (pin 5)))
    (net (code 26) (name "Net-(A1-Pad16)")
      (node (ref A1) (pin 16)))
    (net (code 27) (name "Net-(A1-Pad15)")
      (node (ref A1) (pin 15)))
    (net (code 28) (name /SIOD)
      (node (ref J1) (pin 4))
      (node (ref R2) (pin 2))
      (node (ref A1) (pin 13)))
    (net (code 29) (name /D3)
      (node (ref J1) (pin 13))
      (node (ref A1) (pin 12)))
    (net (code 30) (name /D2)
      (node (ref A1) (pin 11))
      (node (ref J1) (pin 14)))
    (net (code 31) (name /D1)
      (node (ref A1) (pin 10))
      (node (ref J1) (pin 15)))
    (net (code 32) (name "Net-(A1-Pad1)")
      (node (ref A1) (pin 1)))))