(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/cctv_camera_fuse/pcb/pcb.sch)
    (date "Mon 24 Jun 2019 10:04:43 PM EDT")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source pcb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D117F39))
    (comp (ref D1)
      (value D)
      (footprint Diodes_THT:Diode_DO-41_SOD81_Horizontal_RM10)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D1180A4))
    (comp (ref MK2)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D11843D))
    (comp (ref MK1)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_3.2mm_M3)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D1184DD))
    (comp (ref P1)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D1189CB))
    (comp (ref P2)
      (value CONN_01X02)
      (footprint Connectors_Molex:Molex_MiniFit-JR-5556-02A_2x01x4.20mm_Straight)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D118A24)))
  (libparts
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp Diode_*)
        (fp D-*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib mechanical) (part Mounting_Hole)
      (description "Mounting Hole without connection")
      (footprints
        (fp Mounting?Hole*)
        (fp Hole*))
      (fields
        (field (name Reference) MK)
        (field (name Value) Mounting_Hole))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical mechanical)
      (uri /usr/share/kicad/library/mechanical.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref D1) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref P2) (pin 2)))
    (net (code 2) (name VCC)
      (node (ref P2) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref F1) (pin 1)))
    (net (code 3) (name +12V)
      (node (ref F1) (pin 2))
      (node (ref P1) (pin 2)))))