(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/FlammableGasSensor/pcb/gassensor.sch)
    (date "Mon 03 Jun 2019 07:25:44 PM EDT")
    (tool "Eeschema 5.0.0-rc2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source gassensor.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Arduino_Nano_Header)
      (footprint w_conn_misc:arduino_nano_header)
      (libsource (lib w_connectors) (part Arduino_Nano_Header))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9FA3E))
    (comp (ref LS1)
      (value Speaker)
      (footprint w_conn_mkds:mkds_1,5-2)
      (libsource (lib device) (part Speaker))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9FB90))
    (comp (ref CON1)
      (value BARREL_JACK)
      (footprint Connectors:BARREL_JACK)
      (libsource (lib conn) (part BARREL_JACK))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9FDCB))
    (comp (ref P1)
      (value Switcher)
      (footprint pot:SF_STS10)
      (libsource (lib conn) (part CONN_01X10))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA0146))
    (comp (ref R1)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA0A96))
    (comp (ref RV1)
      (value 100K)
      (footprint pot:Potentiometer_Vishay_TS53YL_Vertical)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA14B5))
    (comp (ref C1)
      (value 10uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA1F5B))
    (comp (ref C2)
      (value 47uf)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA237B))
    (comp (ref F1)
      (value Fuse)
      (footprint Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm)
      (libsource (lib device) (part Fuse))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA2D4F))
    (comp (ref D1)
      (value ReverseVoltageDiode)
      (footprint Diodes_THT:Diode_DO-41_SOD81_Horizontal_RM10)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA3E2A))
    (comp (ref D3)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4C40))
    (comp (ref R3)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4CD4))
    (comp (ref D4)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4E2B))
    (comp (ref R4)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA4EC1))
    (comp (ref D5)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA572B))
    (comp (ref R5)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5731))
    (comp (ref D6)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5737))
    (comp (ref R6)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA573D))
    (comp (ref D7)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BE1))
    (comp (ref R7)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BE7))
    (comp (ref D8)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BED))
    (comp (ref R8)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BF3))
    (comp (ref D9)
      (value LED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BF9))
    (comp (ref R9)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5BFF))
    (comp (ref D10)
      (value D)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5C05))
    (comp (ref R10)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA5C0B))
    (comp (ref D2)
      (value PWRLED)
      (footprint LEDs:LED-3MM)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA7FCB))
    (comp (ref R2)
      (value 1K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA7FD1))
    (comp (ref P4)
      (value Arefbrk)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCAE976))
    (comp (ref P3)
      (value RST_brkout)
      (footprint Pin_Headers:Pin_Header_Straight_1x01)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCAED2A))
    (comp (ref P8)
      (value SPI_Brkout)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCB5B84))
    (comp (ref P7)
      (value UART)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCB6AC0))
    (comp (ref P6)
      (value MISC_Brkout)
      (footprint Pin_Headers:Pin_Header_Straight_1x03)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCB798F))
    (comp (ref R13)
      (value 200K)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCBB5E7))
    (comp (ref RV2)
      (value 1M)
      (footprint pot:Potentiometer_Vishay_TS53YL_Vertical)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCBB715))
    (comp (ref P9)
      (value GasSensorEdgeConnector)
      (footprint pot:EdgeConnectorGasSensorPCB)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCBE214))
    (comp (ref P2)
      (value GasSensor)
      (footprint w_conn_mkds:mkds_1,5-4)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA9BE8))
    (comp (ref MK4)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC47B4))
    (comp (ref MK3)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC48EE))
    (comp (ref MK2)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC4A58))
    (comp (ref MK1)
      (value Mounting_Hole)
      (footprint Mounting_Holes:MountingHole_5.3mm_M5)
      (libsource (lib mechanical) (part Mounting_Hole))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC4B04)))
  (libparts
    (libpart (lib conn) (part BARREL_JACK)
      (description "DC Barrel Jack")
      (fields
        (field (name Reference) CON)
        (field (name Value) BARREL_JACK))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector, single row, 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector, single row, 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X10)
      (description "Connector, single row, 01x10")
      (footprints
        (fp Pin_Header_Straight_1X10)
        (fp Pin_Header_Angled_1X10)
        (fp Socket_Strip_Straight_1X10)
        (fp Socket_Strip_Angled_1X10))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X10))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (footprints
        (fp Diode_*)
        (fp D-*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentionmeter)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Speaker)
      (description speaker)
      (fields
        (field (name Reference) LS)
        (field (name Value) Speaker))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib mechanical) (part Mounting_Hole)
      (description "Mounting Hole without connection")
      (footprints
        (fp Mounting?Hole*)
        (fp Hole*))
      (fields
        (field (name Reference) MK)
        (field (name Value) Mounting_Hole)))
    (libpart (lib w_connectors) (part Arduino_Nano_Header)
      (fields
        (field (name Reference) J)
        (field (name Value) Arduino_Nano_Header))
      (pins
        (pin (num 1) (name D1/TX) (type passive))
        (pin (num 2) (name D0/RX) (type passive))
        (pin (num 3) (name RESET) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name D2/INT0) (type passive))
        (pin (num 6) (name D3/INT1) (type passive))
        (pin (num 7) (name D4/T0) (type passive))
        (pin (num 8) (name D5/T1) (type passive))
        (pin (num 9) (name D6/AIN0) (type passive))
        (pin (num 10) (name D7/AIN1) (type passive))
        (pin (num 11) (name D8/ICP) (type passive))
        (pin (num 12) (name D9/0C1) (type passive))
        (pin (num 13) (name D10/SS) (type passive))
        (pin (num 14) (name D11/MOSI) (type passive))
        (pin (num 15) (name D12/MISO) (type passive))
        (pin (num 16) (name SCK/D13) (type passive))
        (pin (num 17) (name 3V3) (type passive))
        (pin (num 18) (name AREF) (type passive))
        (pin (num 19) (name A0) (type passive))
        (pin (num 20) (name A1) (type passive))
        (pin (num 21) (name A2) (type passive))
        (pin (num 22) (name A3) (type passive))
        (pin (num 23) (name A4) (type passive))
        (pin (num 24) (name A5) (type passive))
        (pin (num 25) (name A6) (type passive))
        (pin (num 26) (name A7) (type passive))
        (pin (num 27) (name 5V) (type passive))
        (pin (num 28) (name RESET) (type passive))
        (pin (num 29) (name GND) (type passive))
        (pin (num 30) (name VIN) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical mechanical)
      (uri /usr/share/kicad/library/mechanical.lib))
    (library (logical w_connectors)
      (uri /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/FlammableGasSensor/pcb/symbols/w_connectors.lib)))
  (nets
    (net (code 1) (name "Net-(D2-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref D2) (pin 1)))
    (net (code 2) (name VCC)
      (node (ref C1) (pin 1))
      (node (ref J1) (pin 30))
      (node (ref F1) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref D1) (pin 1)))
    (net (code 3) (name +5V)
      (node (ref J1) (pin 27))
      (node (ref P2) (pin 2))
      (node (ref P9) (pin 2)))
    (net (code 4) (name /SCK)
      (node (ref J1) (pin 16))
      (node (ref P8) (pin 4)))
    (net (code 5) (name /MISO)
      (node (ref P8) (pin 3))
      (node (ref J1) (pin 15)))
    (net (code 6) (name "Net-(J1-Pad3)")
      (node (ref P3) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 7) (name "Net-(J1-Pad18)")
      (node (ref P4) (pin 1))
      (node (ref J1) (pin 18)))
    (net (code 8) (name /A6)
      (node (ref R13) (pin 1))
      (node (ref J1) (pin 25))
      (node (ref P2) (pin 4))
      (node (ref P9) (pin 4)))
    (net (code 9) (name "Net-(D6-Pad1)")
      (node (ref D6) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 10) (name "Net-(D8-Pad1)")
      (node (ref D8) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 11) (name /A5)
      (node (ref J1) (pin 24))
      (node (ref D8) (pin 2)))
    (net (code 12) (name "Net-(D7-Pad1)")
      (node (ref D7) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 13) (name /A4)
      (node (ref J1) (pin 23))
      (node (ref D7) (pin 2)))
    (net (code 14) (name "Net-(D9-Pad1)")
      (node (ref R9) (pin 2))
      (node (ref D9) (pin 1)))
    (net (code 15) (name /A3)
      (node (ref D6) (pin 2))
      (node (ref J1) (pin 22)))
    (net (code 16) (name "Net-(D5-Pad1)")
      (node (ref D5) (pin 1))
      (node (ref R5) (pin 2)))
    (net (code 17) (name /A2)
      (node (ref J1) (pin 21))
      (node (ref D5) (pin 2)))
    (net (code 18) (name "Net-(D10-Pad1)")
      (node (ref R10) (pin 2))
      (node (ref D10) (pin 1)))
    (net (code 19) (name /D8)
      (node (ref J1) (pin 11))
      (node (ref D10) (pin 2)))
    (net (code 20) (name /D7)
      (node (ref J1) (pin 10))
      (node (ref P6) (pin 3))
      (node (ref D9) (pin 2)))
    (net (code 21) (name /VOUT+)
      (node (ref P9) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref C2) (pin 1))
      (node (ref RV1) (pin 1))
      (node (ref P2) (pin 1)))
    (net (code 22) (name /TX)
      (node (ref P7) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 23) (name "Net-(RV2-Pad3)")
      (node (ref RV2) (pin 3)))
    (net (code 24) (name "Net-(R13-Pad2)")
      (node (ref R13) (pin 2))
      (node (ref RV2) (pin 1)))
    (net (code 25) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 26) (name "Net-(P1-Pad2)")
      (node (ref P1) (pin 2)))
    (net (code 27) (name "Net-(P1-Pad8)")
      (node (ref P1) (pin 8)))
    (net (code 28) (name "Net-(P1-Pad4)")
      (node (ref P1) (pin 4)))
    (net (code 29) (name "Net-(P1-Pad3)")
      (node (ref P1) (pin 3)))
    (net (code 30) (name +12V)
      (node (ref F1) (pin 2))
      (node (ref CON1) (pin 1)))
    (net (code 31) (name "Net-(J1-Pad5)")
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 5)))
    (net (code 32) (name /REMOTE)
      (node (ref P1) (pin 10))
      (node (ref R1) (pin 1)))
    (net (code 33) (name GND)
      (node (ref D1) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref J1) (pin 29))
      (node (ref R6) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref RV1) (pin 3))
      (node (ref P2) (pin 3))
      (node (ref CON1) (pin 3))
      (node (ref P9) (pin 3))
      (node (ref RV2) (pin 2))
      (node (ref P1) (pin 9))
      (node (ref CON1) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref P1) (pin 7)))
    (net (code 34) (name /TRIM)
      (node (ref RV1) (pin 2))
      (node (ref P1) (pin 6)))
    (net (code 35) (name /D6)
      (node (ref P6) (pin 2))
      (node (ref J1) (pin 9)))
    (net (code 36) (name /SS)
      (node (ref P8) (pin 1))
      (node (ref J1) (pin 13)))
    (net (code 37) (name /D9)
      (node (ref J1) (pin 12)))
    (net (code 38) (name "Net-(J1-Pad8)")
      (node (ref LS1) (pin 1))
      (node (ref J1) (pin 8)))
    (net (code 39) (name "Net-(J1-Pad7)")
      (node (ref LS1) (pin 2))
      (node (ref J1) (pin 7)))
    (net (code 40) (name /D3)
      (node (ref P6) (pin 1))
      (node (ref J1) (pin 6)))
    (net (code 41) (name /RX)
      (node (ref P7) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 42) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 43) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 44) (name /A7)
      (node (ref J1) (pin 26)))
    (net (code 45) (name /MOSI)
      (node (ref P8) (pin 2))
      (node (ref J1) (pin 14)))
    (net (code 46) (name /A1)
      (node (ref D4) (pin 2))
      (node (ref J1) (pin 20)))
    (net (code 47) (name "Net-(D3-Pad1)")
      (node (ref R3) (pin 2))
      (node (ref D3) (pin 1)))
    (net (code 48) (name /A0)
      (node (ref D3) (pin 2))
      (node (ref J1) (pin 19)))))