(export (version D)
  (design
    (source /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/FlammableGasSensor/pcb/gassensorholder/gassensorholder.sch)
    (date "Fri 23 Aug 2019 02:12:56 AM EDT")
    (tool "Eeschema 5.0.2+dfsg1-1~bpo9+1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source gassensorholder.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value CONN_01X04)
      (footprint to_39:TO-39-4)
      (libsource (lib gassensorholder-rescue) (part CONN_01X04-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D113ADE)))
  (libparts
    (libpart (lib gassensorholder-rescue) (part CONN_01X04-conn)
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04-conn))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive)))))
  (libraries
    (library (logical gassensorholder-rescue)
      (uri /home/layoutdev/Desktop/code/documentation_general/Electronics_Projects_2019/FlammableGasSensor/pcb/gassensorholder/gassensorholder-rescue.lib)))
  (nets
    (net (code 1) (name /VSenseOUT)
      (node (ref P1) (pin 1)))
    (net (code 2) (name GND)
      (node (ref P1) (pin 2)))
    (net (code 3) (name /VOut+)
      (node (ref P1) (pin 4)))
    (net (code 4) (name +5V)
      (node (ref P1) (pin 3)))))