(module TO-220F-2_Horizontal_TabUp (layer F.Cu) (tedit 5ACC4AF2)
  (descr "TO-220F-2, Horizontal, RM 5.08mm, see http://www.onsemi.com/pub/Collateral/FFPF10F150S-D.pdf")
  (tags "TO-220F-2 Horizontal RM 5.08mm")
  (fp_text reference REF** (at 2.54 20.22) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TO-220F-2_Horizontal_TabUp (at 2.54 -2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 2.54 15.8) (end 4.39 15.8) (layer F.Fab) (width 0.1))
  (fp_line (start -2.59 12.42) (end -2.59 19.1) (layer F.Fab) (width 0.1))
  (fp_line (start -2.59 19.1) (end 7.67 19.1) (layer F.Fab) (width 0.1))
  (fp_line (start 7.67 19.1) (end 7.67 12.42) (layer F.Fab) (width 0.1))
  (fp_line (start 7.67 12.42) (end -2.59 12.42) (layer F.Fab) (width 0.1))
  (fp_line (start -2.59 3.23) (end -2.59 12.42) (layer F.Fab) (width 0.1))
  (fp_line (start -2.59 12.42) (end 7.67 12.42) (layer F.Fab) (width 0.1))
  (fp_line (start 7.67 12.42) (end 7.67 3.23) (layer F.Fab) (width 0.1))
  (fp_line (start 7.67 3.23) (end -2.59 3.23) (layer F.Fab) (width 0.1))
  (fp_line (start 0 3.23) (end 0 0) (layer F.Fab) (width 0.1))
  (fp_line (start 5.08 3.23) (end 5.08 0) (layer F.Fab) (width 0.1))
  (fp_line (start -2.71 3.11) (end 7.79 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.71 12.54) (end 7.79 12.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.71 3.11) (end -2.71 12.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.79 3.11) (end 7.79 12.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.71 19.22) (end -1.51 19.22) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.311 19.22) (end 0.89 19.22) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.09 19.22) (end 3.29 19.22) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.49 19.22) (end 5.69 19.22) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.89 19.22) (end 7.79 19.22) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.71 12.78) (end -2.71 13.98) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.71 15.18) (end -2.71 16.38) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.71 17.58) (end -2.71 18.78) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.79 12.78) (end 7.79 13.98) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.79 15.18) (end 7.79 16.38) (layer F.SilkS) (width 0.12))
  (fp_line (start 7.79 17.58) (end 7.79 18.78) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 1.15) (end 0 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.08 1.165) (end 5.08 3.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.84 -1.25) (end -2.84 19.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.84 19.35) (end 7.92 19.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.92 19.35) (end 7.92 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.92 -1.25) (end -2.84 -1.25) (layer F.CrtYd) (width 0.05))
  (pad "" np_thru_hole oval (at 2.54 15.8) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 5.08 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.54 20.22) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220F-2_Horizontal_TabUp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)