
\documentclass[11pt]{article}
%Gummi|065|=)
\usepackage{graphicx}
\usepackage{caption}
\usepackage{xcolor}
\usepackage[vcentering,dvips]{geometry}
\geometry{papersize={6in,9in},total={4.5in,6.8in}}
\title{\textbf{Door Alarm}}
\author{Steak Electronics}
\date{}
\begin{document}

\maketitle

%\tableofcontents
\textcolor{green!60!blue!70}{
  \section{Attiny Solar Energy Harvest Tests}}

I have the following:
\begin{itemize}
\item Solar panels
\item Attiny 10
\end{itemize}
To this list, I will add a supercap, and an energy harvesting IC. The goal being to load the super cap during the day, and to run 24/7. I will need an exceptionally low power micro. The super cap will need to be about 3.3V or 5V.

\subsection{Micro Considerations}
The Arduino Atmega328P is not an option. I'm looking to have a current draw of only 1mA max, (ideally 500uA) when active. Moteino is also not an option for this. Those are made for batteries. I want to be battery free. A super cap, however can be used to store energy. I'll get to that shortly.

For micros, I have some Attiny10 on hand, and these have a reasonably low power pull in active mode. Let's build those up first. What will the micro do? No idea. I haven't a clue.

\subsection{Energy Storage}
I don't want a battery. Let's go with a super cap. The solar panels will only be active some of the time, so I will want to harvest energy with some kind of IC into the cap when the sun is out.\footnote{Reference: www.analog.com/media/en/technical-documentation/technical-articles/solarenergyharvesting.pdf is a start. I'll need to do more research.}



\end{document}

